(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)

  (general
    (links 212)
    (no_connects 32)
    (area 52.599999 29.499999 123.700001 156.700001)
    (thickness 1.6)
    (drawings 4)
    (tracks 507)
    (zones 0)
    (modules 79)
    (nets 80)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00120_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/dmitryneuro/git.neuroidss.local/FreeSmartEEG/KiCad/out/))
  )

  (net 0 "")
  (net 1 _IO11)
  (net 2 IO12)
  (net 3 IO13)
  (net 4 AVSS)
  (net 5 AREF)
  (net 6 SDA)
  (net 7 SCL)
  (net 8 5V)
  (net 9 RESET)
  (net 10 IOREF)
  (net 11 3.3V)
  (net 12 VIN)
  (net 13 RX)
  (net 14 TX)
  (net 15 A0)
  (net 16 A1)
  (net 17 A2)
  (net 18 A3)
  (net 19 A4)
  (net 20 A5)
  (net 21 AUXAIN-)
  (net 22 AIN0-)
  (net 23 AIN1-)
  (net 24 AIN2-)
  (net 25 AIN3-)
  (net 26 AIN4-)
  (net 27 AIN5-)
  (net 28 AIN6-)
  (net 29 AIN7-)
  (net 30 AUXAIN+)
  (net 31 AIN0+)
  (net 32 AIN1+)
  (net 33 AIN2+)
  (net 34 AIN3+)
  (net 35 AIN4+)
  (net 36 AIN5+)
  (net 37 AIN6+)
  (net 38 AIN7+)
  (net 39 "Net-(C5-Pad2)")
  (net 40 AVDD)
  (net 41 "Net-(U2-Pad4)")
  (net 42 "Net-(U3-Pad4)")
  (net 43 "Net-(U4-Pad4)")
  (net 44 START)
  (net 45 ADC_RESET)
  (net 46 CS)
  (net 47 SCLK)
  (net 48 MCU_RESET)
  (net 49 DRDY)
  (net 50 DCLK)
  (net 51 DOUT0)
  (net 52 DOUT1)
  (net 53 DOUT2)
  (net 54 DOUT3)
  (net 55 CLK_SEL)
  (net 56 "Net-(P9-Pad7)")
  (net 57 "Net-(P11-Pad3)")
  (net 58 "Net-(P11-Pad11)")
  (net 59 GPIO0)
  (net 60 GPIO1)
  (net 61 GPIO2)
  (net 62 ALERT)
  (net 63 XTAL1)
  (net 64 XTAL2)
  (net 65 SYNC_OUT)
  (net 66 SYNC_IN)
  (net 67 REF_OUT)
  (net 68 VCM)
  (net 69 OUT_VREF)
  (net 70 "Net-(P13-Pad1)")
  (net 71 "Net-(P13-Pad2)")
  (net 72 "Net-(P15-Pad1)")
  (net 73 "Net-(P15-Pad2)")
  (net 74 "Net-(P17-Pad1)")
  (net 75 "Net-(P17-Pad2)")
  (net 76 "Net-(C9-Pad2)")
  (net 77 "Net-(C19-Pad1)")
  (net 78 MOSI)
  (net 79 MISO)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3V)
    (add_net 5V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net ADC_RESET)
    (add_net AIN0+)
    (add_net AIN0-)
    (add_net AIN1+)
    (add_net AIN1-)
    (add_net AIN2+)
    (add_net AIN2-)
    (add_net AIN3+)
    (add_net AIN3-)
    (add_net AIN4+)
    (add_net AIN4-)
    (add_net AIN5+)
    (add_net AIN5-)
    (add_net AIN6+)
    (add_net AIN6-)
    (add_net AIN7+)
    (add_net AIN7-)
    (add_net ALERT)
    (add_net AREF)
    (add_net AUXAIN+)
    (add_net AUXAIN-)
    (add_net AVDD)
    (add_net AVSS)
    (add_net CLK_SEL)
    (add_net CS)
    (add_net DCLK)
    (add_net DOUT0)
    (add_net DOUT1)
    (add_net DOUT2)
    (add_net DOUT3)
    (add_net DRDY)
    (add_net GPIO0)
    (add_net GPIO1)
    (add_net GPIO2)
    (add_net IO12)
    (add_net IO13)
    (add_net IOREF)
    (add_net MCU_RESET)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(P11-Pad11)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P13-Pad2)")
    (add_net "Net-(P15-Pad1)")
    (add_net "Net-(P15-Pad2)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(P17-Pad2)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad4)")
    (add_net OUT_VREF)
    (add_net REF_OUT)
    (add_net RESET)
    (add_net RX)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net START)
    (add_net SYNC_IN)
    (add_net SYNC_OUT)
    (add_net TX)
    (add_net VCM)
    (add_net VIN)
    (add_net XTAL1)
    (add_net XTAL2)
    (add_net _IO11)
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 5787BF7D)
    (at 106.68 68.58)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 5787BF6F)
    (at 106.68 66.04)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57843D6D)
    (at 74.676 151.384 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57878F16) (tstamp 578437EA)
    (at 71.12 147.32 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5787A49B)
    (fp_text reference P21 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value GNDAIN (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839C28)
    (at 55.88 121.92)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839C1A)
    (at 119.38 121.92)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839C0D)
    (at 119.38 127)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839BCB)
    (at 55.88 127)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839B2D)
    (at 101.6 149.86 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839B21)
    (at 78.74 149.86 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 578393FA) (tstamp 57839336)
    (at 116.84 111.76)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783940A) (tstamp 5783932A)
    (at 116.84 114.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839411) (tstamp 5783931E)
    (at 116.84 116.84)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839417) (tstamp 57839312)
    (at 116.84 119.38)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57878C87) (tstamp 57839304)
    (at 116.84 132.08)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839429) (tstamp 578392F8)
    (at 116.84 134.62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783942E) (tstamp 578392EB)
    (at 116.84 137.16)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839469) (tstamp 578392DF)
    (at 116.84 139.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839456) (tstamp 578392D3)
    (at 58.42 111.76)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839452) (tstamp 578392C7)
    (at 58.42 114.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783944F) (tstamp 578392BB)
    (at 58.42 116.84)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783944B) (tstamp 578392AF)
    (at 58.42 119.38)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839447) (tstamp 578392A3)
    (at 58.42 132.08)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783943E) (tstamp 57839297)
    (at 58.42 134.62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5783943A) (tstamp 57839285)
    (at 58.42 137.16)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57878F52) (tstamp 57839197)
    (at 60.96 111.76)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57879DC2)
    (fp_text reference P20 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AIN67 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 9.4) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 AIN7+))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 AIN7-))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 AIN6+))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 AIN6-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57878F4D) (tstamp 57839149)
    (at 60.96 132.08)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57879A6B)
    (fp_text reference P19 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AIN45 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 9.4) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 AIN5+))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 AIN5-))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 AIN4+))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 AIN4-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57878EEF) (tstamp 5783905E)
    (at 114.3 139.7 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5787A0C5)
    (fp_text reference P6 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AIN01 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 9.4) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 AIN0-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AIN0+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 AIN1-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AIN1+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module LFCSP-64-1EP_9x9mm_Pitch0.5mm (layer F.Cu) (tedit 57821FA2) (tstamp 57804CFA)
    (at 87.63 120.65 180)
    (descr "64-Lead Plastic Quad Flat, No Lead Package (MR) - 9x9x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "64-pin LFCSP 0.5")
    (path /577FE1B1)
    (attr smd)
    (fp_text reference U1 (at 0 -5.875 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD7779 (at 0 5.875 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.15 -5.15) (end -5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.15 -5.15) (end 5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 -5.15) (end 5.15 -5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 5.15) (end 5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 -4.7) (end 4.7 -4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 4.7) (end -4.7 4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 4.7) (end 4.7 4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 -4.7) (end -4.125 -4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 4.7) (end -4.125 4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 4.7) (end 4.125 4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 -4.7) (end 4.125 -4.7) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.5 -3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 AIN0-))
    (pad 2 smd rect (at -4.5 -3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 AIN0+))
    (pad 3 smd rect (at -4.5 -2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 AIN1-))
    (pad 4 smd rect (at -4.5 -2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 AIN1+))
    (pad 5 smd rect (at -4.5 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 6 smd rect (at -4.5 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 7 smd rect (at -4.5 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 8 smd rect (at -4.5 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (pad 9 smd rect (at -4.5 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 AIN2-))
    (pad 10 smd rect (at -4.5 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 AIN2+))
    (pad 11 smd rect (at -4.5 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 AIN3-))
    (pad 12 smd rect (at -4.5 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 AIN3+))
    (pad 13 smd rect (at -4.5 2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 GPIO0))
    (pad 14 smd rect (at -4.5 2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 GPIO1))
    (pad 15 smd rect (at -4.5 3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 GPIO2))
    (pad 16 smd rect (at -4.5 3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 ALERT))
    (pad 17 smd rect (at -3.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (pad 18 smd rect (at -3.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 CS))
    (pad 19 smd rect (at -2.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 SCLK))
    (pad 20 smd rect (at -2.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 MOSI))
    (pad 21 smd rect (at -1.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 MISO))
    (pad 22 smd rect (at -1.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 23 smd rect (at -0.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (pad 24 smd rect (at -0.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (pad 25 smd rect (at 0.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 DOUT3))
    (pad 26 smd rect (at 0.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 DOUT2))
    (pad 27 smd rect (at 1.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 DOUT1))
    (pad 28 smd rect (at 1.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 DOUT0))
    (pad 29 smd rect (at 2.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 DCLK))
    (pad 30 smd rect (at 2.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 DRDY))
    (pad 31 smd rect (at 3.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 XTAL1))
    (pad 32 smd rect (at 3.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 XTAL2))
    (pad 33 smd rect (at 4.5 3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 START))
    (pad 34 smd rect (at 4.5 3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 SYNC_OUT))
    (pad 35 smd rect (at 4.5 2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 SYNC_IN))
    (pad 36 smd rect (at 4.5 2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 ADC_RESET))
    (pad 37 smd rect (at 4.5 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 AIN7+))
    (pad 38 smd rect (at 4.5 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 AIN7-))
    (pad 39 smd rect (at 4.5 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 AIN6+))
    (pad 40 smd rect (at 4.5 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 AIN6-))
    (pad 41 smd rect (at 4.5 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (pad 42 smd rect (at 4.5 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 43 smd rect (at 4.5 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 44 smd rect (at 4.5 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 45 smd rect (at 4.5 -2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 AIN5+))
    (pad 46 smd rect (at 4.5 -2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 AIN5-))
    (pad 47 smd rect (at 4.5 -3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 AIN4+))
    (pad 48 smd rect (at 4.5 -3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 AIN4-))
    (pad 49 smd rect (at 3.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 REF_OUT))
    (pad 50 smd rect (at 3.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 51 smd rect (at 2.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C9-Pad2)"))
    (pad 52 smd rect (at 2.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 53 smd rect (at 1.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 54 smd rect (at 1.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (pad 55 smd rect (at 0.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (pad 56 smd rect (at 0.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (pad 57 smd rect (at -0.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 VCM))
    (pad 58 smd rect (at -0.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 59 smd rect (at -1.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C19-Pad1)"))
    (pad 60 smd rect (at -1.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 61 smd rect (at -2.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 62 smd rect (at -2.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 63 smd rect (at -3.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 AUXAIN+))
    (pad 64 smd rect (at -3.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 AUXAIN-))
    (pad 65 smd rect (at 2.85 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FED9) (tstamp 57833DD7)
    (at 92.71 73.66 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DBCD)
    (fp_text reference P17 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(P17-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(P17-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 OUT_VREF))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FED1) (tstamp 57833DC6)
    (at 85.09 68.58)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DB30)
    (fp_text reference P16 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FECB) (tstamp 57833DB5)
    (at 92.71 62.23 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DA96)
    (fp_text reference P15 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(P15-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(P15-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FEC5) (tstamp 57833DA4)
    (at 85.09 57.15)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D9FF)
    (fp_text reference P14 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FE32) (tstamp 57833D93)
    (at 92.71 85.09 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D91F)
    (fp_text reference P13 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(P13-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5FA) (tstamp 57833B8C)
    (at 68.58 142.24 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830FDE)
    (fp_text reference P11 (at 0 -5.1 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X16 (at 0 -3.1 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 REF_OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P11-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 VCM))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P11-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AUXAIN+))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 AUXAIN-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5F2) (tstamp 57833B6E)
    (at 66.04 101.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830EE7)
    (fp_text reference P10 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X16 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 START))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 SYNC_OUT))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 SYNC_IN))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 ADC_RESET))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 AIN7+))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 AIN7-))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 AIN6+))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 AIN6-))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 OUT_VREF))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 AIN5+))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 AIN5-))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 AIN4+))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 AIN4-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5EB) (tstamp 57833B50)
    (at 106.68 99.06 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830E1B)
    (fp_text reference P9 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X16 (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 CS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 SCLK))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 MOSI))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 MISO))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P9-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 CLK_SEL))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 DOUT3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 DOUT2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 DOUT1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 DOUT0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 DCLK))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 DRDY))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 XTAL1))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 XTAL2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57804FF2) (tstamp 57833A2E)
    (at 88.9 82.55 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE273)
    (attr smd)
    (fp_text reference U2 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-3.3Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57804FF9) (tstamp 57833A20)
    (at 88.9 59.69 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE246)
    (attr smd)
    (fp_text reference U3 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-3.3Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 0) (tstamp 57804D34)
    (at 111.76 72.136 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE5A9)
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DIGITAL(_PWM)" (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 24.65) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 24.13) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 START))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 ADC_RESET))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 CS))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 MOSI))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 MISO))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 SCLK))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 AREF))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 SDA))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B) (tstamp 57804D3E)
    (at 91.44 91.567 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57801C6A)
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ICSP (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 0 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.3 -1.75) (end 4.3 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 4.3 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 4.3 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 3.81 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 6.35) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end -1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 IO12))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 IO13))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 _IO11))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0) (tstamp 57804D4A)
    (at 63.5 58.42)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE40C)
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value POWER (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 AREF))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 IOREF))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 MCU_RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 5V))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 VIN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0) (tstamp 57804D56)
    (at 111.76 93.98 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE497)
    (fp_text reference P4 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DIGITAL(_PWM)" (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 TX))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 DOUT3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 DOUT2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 DOUT1))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 DOUT0))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 DCLK))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 DRDY))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0) (tstamp 57804D60)
    (at 63.5 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57800D6E)
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ANALOG_IN (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 14.45) (end 1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 13.97) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 13.97) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 A0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 A1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 A2))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 A3))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 A4))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 A5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57805000) (tstamp 578050B1)
    (at 88.9 71.12 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE314)
    (attr smd)
    (fp_text reference U4 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-2.5Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5DD) (tstamp 5780E56E)
    (at 109.22 139.7 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830D69)
    (fp_text reference P8 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X16 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 AIN0-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AIN0+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 AIN1-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AIN1+))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 OUT_VREF))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AIN2-))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AIN2+))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 AIN3-))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 AIN3+))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 GPIO0))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 GPIO1))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 GPIO2))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 ALERT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FE12) (tstamp 5780FD8A)
    (at 85.09 80.01)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D841)
    (fp_text reference P12 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F9D)
    (at 91.44 132.969)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780EAA6)
    (attr smd)
    (fp_text reference C19 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F82)
    (at 100.2792 124.6378 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DE66)
    (attr smd)
    (fp_text reference C18 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F68)
    (at 89.535 129.2352)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FBDF)
    (attr smd)
    (fp_text reference C15 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F50)
    (at 101.7778 122.1232 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780D089)
    (attr smd)
    (fp_text reference C14 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F38)
    (at 82.4484 133.0198)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5781025B)
    (attr smd)
    (fp_text reference C11 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F2A)
    (at 79.5528 133.01726)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57810352)
    (attr smd)
    (fp_text reference C9 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F1E)
    (at 75.438 124.3838 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578108CA)
    (attr smd)
    (fp_text reference C7 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F06)
    (at 73.9394 122.047 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57810A46)
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EEE)
    (at 94.3356 133.1468)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FF65)
    (attr smd)
    (fp_text reference C21 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804ED6)
    (at 76.76388 134.51586)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578103BF)
    (attr smd)
    (fp_text reference C10 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 67 REF_OUT))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EBC)
    (at 89.8398 109.3216 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780CC33)
    (attr smd)
    (fp_text reference C6 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804E9D)
    (at 88.6968 112.3188 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780CC6E)
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F74)
    (at 101.7778 125.2982 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DE17)
    (attr smd)
    (fp_text reference C17 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F44)
    (at 103.2764 122.3772 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DDD1)
    (attr smd)
    (fp_text reference C13 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F12)
    (at 90.2462 107.823 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780C539)
    (attr smd)
    (fp_text reference C5 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EFA)
    (at 88.9762 110.8202 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57803D35)
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BA9)
    (at 87.63 80.01 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5784635D)
    (attr smd)
    (fp_text reference C23 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BAF)
    (at 90.17 57.15)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578461F6)
    (attr smd)
    (fp_text reference C24 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BB5)
    (at 87.63 57.15 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5784673C)
    (attr smd)
    (fp_text reference C25 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BBB)
    (at 90.17 68.58)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578462B7)
    (attr smd)
    (fp_text reference C26 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BC1)
    (at 87.63 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57846404)
    (attr smd)
    (fp_text reference C27 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804CEE)
    (at 95.3008 134.6454)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FFD0)
    (attr smd)
    (fp_text reference C22 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EAC)
    (at 72.4408 122.2502 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578109CD)
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 OUT_VREF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EC8)
    (at 73.9394 124.9934 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5781095F)
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EE2)
    (at 81.5848 134.5184)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578102EE)
    (attr smd)
    (fp_text reference C12 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F5C)
    (at 90.043 130.7338)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FC4A)
    (attr smd)
    (fp_text reference C16 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F8F)
    (at 90.17 80.01)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57846078)
    (attr smd)
    (fp_text reference C20 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module FreeSmartEEG:SMD0503_4P_Crystal (layer F.Cu) (tedit 57824BEC) (tstamp 57804CFB)
    (at 74.53 104.46 306)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 4 Pads")
    (tags "crystal oscillator quartz SMD0503 4P")
    (path /57804CA7)
    (attr smd)
    (fp_text reference Y1 (at 0 -4 306) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "8.192 MHz" (at 0 4 306) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.5 2.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 2.5) (end -3.5 2.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 -2.5) (end 3.5 2.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.5 -2.5) (end 3.5 -2.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.6 2.3) (end -4.15 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 2.6) (end 3.6 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 -2.6) (end 3.6 -2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 -2.6) (end -3.6 -2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.6) (end -3.6 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.6) (end 3.6 2.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 0.2) (end -4.15 0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.75 -3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.1) (end -4.75 -3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.6 -2.6) (end 3.6 -2.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 0.2) (end 3.6 -0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 0.2) (end -3.6 -0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.75 3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.1) (end 4.75 3.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.5 1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 64 XTAL2))
    (pad 3 smd rect (at 2.5 1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.5 -1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 63 XTAL1))
    (pad 3 smd rect (at -2.5 -1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask))
  )

  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57878EF5) (tstamp 57839043)
    (at 114.3 119.38 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5787A19D)
    (fp_text reference P7 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AIN23 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 9.4) (end 1.75 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 8.89) (end 1.27 8.89) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AIN2-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AIN2+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 AIN3-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 AIN3+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57878F1C) (tstamp 578391C9)
    (at 106.68 147.32 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5787A728)
    (fp_text reference P18 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AUXAIN (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.27 1.27) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 4.3) (end 1.75 4.3) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 1.27) (end -1.27 3.81) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 3.81) (end 1.27 3.81) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 AUXAIN-))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AUXAIN+))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839436) (tstamp 5783926C)
    (at 58.42 139.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1k (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57839AA1) (tstamp 57839AC9)
    (at 76.2 149.86 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 52.7 156.6) (end 52.7 29.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 123.58 156.6) (end 52.7 156.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 123.6 29.6) (end 123.6 156.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 52.7 29.6) (end 123.58 29.6) (angle 90) (layer Dwgs.User) (width 0.2))

  (segment (start 55.118 121.92) (end 53.594 123.444) (width 0.25) (layer B.Cu) (net 0))
  (segment (start 121.92 123.952) (end 120.142 122.174) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843E08))
  (segment (start 121.92 139.954) (end 121.92 123.952) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843E01))
  (segment (start 108.458 153.416) (end 121.92 139.954) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843DF8))
  (segment (start 64.77 153.416) (end 108.458 153.416) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843DE4))
  (segment (start 53.594 142.24) (end 64.77 153.416) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843DD8))
  (segment (start 53.594 123.444) (end 53.594 142.24) (width 0.25) (layer B.Cu) (net 0) (tstamp 57843DD1))
  (segment (start 87.884 59.69) (end 88.265 59.69) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.42 58.535) (end 89.42 57.15) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67E0))
  (segment (start 88.265 59.69) (end 89.42 58.535) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67DF))
  (segment (start 87.884 71.12) (end 88.265 71.12) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.42 69.965) (end 89.42 68.58) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67DB))
  (segment (start 88.265 71.12) (end 89.42 69.965) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67D9))
  (segment (start 87.884 82.55) (end 88.265 82.55) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.42 81.395) (end 89.42 80.01) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67D5))
  (segment (start 88.265 82.55) (end 89.42 81.395) (width 0.25) (layer F.Cu) (net 4) (tstamp 578B67D3))
  (segment (start 101.346 76.2) (end 82.55 76.2) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 82.55 76.2) (end 77.47 71.12) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B6873))
  (segment (start 93.98 99.06) (end 95.504 97.536) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838EA5))
  (segment (start 113.5888 97.7138) (end 95.504 97.536) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838EA3))
  (segment (start 113.8174 47.0408) (end 113.5888 97.7138) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E9E))
  (segment (start 109.7026 47.0408) (end 113.8174 47.0408) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E91))
  (segment (start 109.6264 68.4784) (end 109.7026 47.0408) (width 0.25) (layer B.Cu) (net 4) (tstamp 5784C756))
  (segment (start 101.346 76.2) (end 109.6264 68.4784) (width 0.25) (layer B.Cu) (net 4) (tstamp 5784C74E))
  (segment (start 77.47 71.12) (end 63.5 71.12) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B66A5))
  (segment (start 63.5 71.12) (end 77.47 71.12) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 77.47 71.12) (end 82.55 76.2) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B65F2))
  (segment (start 82.55 76.2) (end 82.55 80.645) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B6896))
  (segment (start 82.55 80.645) (end 85.09 82.55) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B68F9))
  (segment (start 63.5 71.12) (end 85.09 71.12) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 77.47 71.12) (end 85.09 59.69) (width 0.25) (layer B.Cu) (net 4) (tstamp 578B65EB))
  (segment (start 89.42 80.01) (end 88.38 80.01) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 87.884 82.55) (end 85.09 82.55) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.42 68.58) (end 88.38 68.58) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 87.884 71.12) (end 85.09 71.12) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.42 57.15) (end 88.38 57.15) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 87.884 59.69) (end 85.09 59.69) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 109.22 129.54) (end 104.902 127.508) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 104.902 127.508) (end 100.2792 125.3878) (width 0.25) (layer F.Cu) (net 4) (tstamp 578790AB))
  (segment (start 109.22 129.54) (end 105.41 127.762) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 105.41 127.762) (end 101.7778 126.0482) (width 0.25) (layer F.Cu) (net 4) (tstamp 578790A7))
  (segment (start 109.22 124.46) (end 105.664 123.698) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 105.664 123.698) (end 101.7778 122.8732) (width 0.25) (layer F.Cu) (net 4) (tstamp 5787909B))
  (segment (start 109.22 124.46) (end 105.664 123.698) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 105.664 123.698) (end 103.2764 123.1272) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879097))
  (segment (start 93.98 99.06) (end 92.202 104.394) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 92.202 104.394) (end 89.4468 112.3188) (width 0.25) (layer F.Cu) (net 4) (tstamp 5787908D))
  (segment (start 93.98 99.06) (end 92.202 104.394) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 92.202 104.394) (end 89.7262 110.8202) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879089))
  (segment (start 93.98 99.06) (end 92.202 104.394) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 92.202 104.394) (end 90.5898 109.3216) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879085))
  (segment (start 66.04 124.46) (end 69.85 123.698) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 69.85 123.698) (end 73.9394 122.797) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879061))
  (segment (start 66.04 124.46) (end 69.85 123.698) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 69.85 123.698) (end 72.4408 123.0002) (width 0.25) (layer F.Cu) (net 4) (tstamp 5787905D))
  (segment (start 66.04 129.54) (end 69.85 127.762) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 69.85 127.762) (end 75.438 125.1338) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879051))
  (segment (start 66.04 129.54) (end 69.342 128.016) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 69.342 128.016) (end 73.9394 125.7434) (width 0.25) (layer F.Cu) (net 4) (tstamp 5787904D))
  (segment (start 71.12 142.24) (end 73.914 138.938) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 73.914 138.938) (end 78.8028 133.01726) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879046))
  (segment (start 71.12 142.24) (end 73.66 139.192) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 73.66 139.192) (end 77.51388 134.51586) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879042))
  (segment (start 78.74 142.24) (end 80.772 137.922) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 80.772 137.922) (end 83.1984 133.0198) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879032))
  (segment (start 78.74 142.24) (end 80.772 137.922) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 80.772 137.922) (end 82.3348 134.5184) (width 0.25) (layer F.Cu) (net 4) (tstamp 5787902D))
  (segment (start 96.52 142.24) (end 94.742 138.43) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 94.742 138.43) (end 90.793 130.7338) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879019))
  (segment (start 99.06 142.24) (end 96.962038 138.723352) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 96.962038 138.723352) (end 94.5508 134.6454) (width 0.25) (layer F.Cu) (net 4) (tstamp 57878FDF))
  (segment (start 99.06 142.24) (end 96.672129 138.237762) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 96.672129 138.237762) (end 93.5856 133.1468) (width 0.25) (layer F.Cu) (net 4) (tstamp 57878FE7))
  (segment (start 96.52 142.24) (end 94.488 137.922) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 94.488 137.922) (end 92.19 132.969) (width 0.25) (layer F.Cu) (net 4) (tstamp 57878FF7))
  (segment (start 71.12 142.24) (end 71.12 147.32) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 86.36 121.92) (end 86.36 127) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 127) (end 71.12 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 5782701C))
  (segment (start 86.36 121.92) (end 86.36 134.62) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 134.62) (end 78.74 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827018))
  (segment (start 88.9 121.92) (end 88.9 134.62) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 134.62) (end 96.52 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827014))
  (segment (start 88.9 121.92) (end 88.9 132.08) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 132.08) (end 99.06 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827010))
  (segment (start 88.9 121.92) (end 101.6 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 101.6 121.92) (end 109.22 129.54) (width 0.25) (layer B.Cu) (net 4) (tstamp 5782700C) (status 20))
  (segment (start 88.9 121.92) (end 106.68 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 106.68 121.92) (end 109.22 124.46) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827008) (status 20))
  (segment (start 88.9 119.38) (end 88.9 104.14) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 104.14) (end 93.98 99.06) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827004))
  (segment (start 86.36 121.92) (end 73.66 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 73.66 121.92) (end 66.04 129.54) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827000))
  (segment (start 86.36 121.92) (end 68.58 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 68.58 121.92) (end 66.04 124.46) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FFC))
  (segment (start 86.36 119.38) (end 88.9 119.38) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 121.92) (end 86.36 119.38) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF7))
  (segment (start 88.9 121.92) (end 86.36 121.92) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF6))
  (segment (start 88.9 119.38) (end 88.9 121.92) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF5))
  (segment (start 89.88 125.15) (end 89.88 126.86) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.38 125.15) (end 89.38 127.11) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.38 127.11) (end 96.52 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 57824096))
  (segment (start 85.88 125.15) (end 85.88 127.11) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 85.88 127.11) (end 78.74 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782407A))
  (segment (start 84.38 125.15) (end 84.38 126.36) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 84.38 126.36) (end 71.12 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782406E))
  (segment (start 83.13 122.4) (end 81.14 122.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.14 122.4) (end 66.04 129.54) (width 0.25) (layer F.Cu) (net 4) (tstamp 57824052))
  (segment (start 83.13 121.4) (end 80.64 121.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 88.88 116.15) (end 88.88 113.86) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 92.13 121.4) (end 94.39 121.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 94.39 121.4) (end 109.22 124.46) (width 0.25) (layer F.Cu) (net 4) (tstamp 578215C7) (status 20))
  (segment (start 92.13 122.4) (end 93.89 122.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 93.89 122.4) (end 109.22 129.54) (width 0.25) (layer F.Cu) (net 4) (tstamp 578215B2) (status 20))
  (segment (start 89.88 126.86) (end 99.06 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782409A))
  (segment (start 80.64 121.4) (end 66.04 124.46) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782404E))
  (segment (start 88.88 113.86) (end 93.98 99.06) (width 0.25) (layer F.Cu) (net 4) (tstamp 57823FFE))
  (segment (start 91.44 107.3792) (end 90.9962 107.823) (width 0.25) (layer F.Cu) (net 4) (tstamp 57879080))
  (segment (start 63.5 66.04) (end 79.375 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 79.375 66.04) (end 81.28 67.945) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65E4))
  (segment (start 81.28 67.945) (end 81.28 81.28) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6A2C))
  (segment (start 81.28 81.28) (end 85.09 85.09) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B696A))
  (segment (start 63.5 66.04) (end 79.375 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 79.375 66.04) (end 81.28 67.945) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65E0))
  (segment (start 81.28 67.945) (end 81.28 76.835) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6A43))
  (segment (start 81.28 76.835) (end 85.09 80.01) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6972))
  (segment (start 63.5 66.04) (end 79.375 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 79.375 66.04) (end 81.28 67.945) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65DC))
  (segment (start 81.28 67.945) (end 81.28 71.12) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6A29))
  (segment (start 81.28 71.12) (end 85.09 73.66) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6975))
  (segment (start 63.5 66.04) (end 82.55 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 82.55 66.04) (end 85.09 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65D8))
  (segment (start 63.5 66.04) (end 79.375 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 79.375 66.04) (end 82.55 66.04) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65D3))
  (segment (start 82.55 66.04) (end 85.09 62.23) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6A6A))
  (segment (start 63.5 66.04) (end 79.375 66.04) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 79.375 66.04) (end 81.28 63.5) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65C2))
  (segment (start 81.28 63.5) (end 81.28 59.69) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6A53))
  (segment (start 81.28 59.69) (end 85.09 57.15) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B697E))
  (segment (start 86.88 80.01) (end 85.09 80.01) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 87.884 83.2104) (end 86.9696 83.2104) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 83.2104) (end 85.09 85.09) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65AD))
  (segment (start 87.884 81.8896) (end 86.9696 81.8896) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 81.8896) (end 85.09 80.01) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B65A8))
  (segment (start 86.88 68.58) (end 85.09 68.58) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 87.884 70.4596) (end 86.9696 70.4596) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 70.4596) (end 85.09 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6596))
  (segment (start 87.884 71.7804) (end 86.9696 71.7804) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 71.7804) (end 85.09 73.66) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6591))
  (segment (start 86.88 57.15) (end 85.09 57.15) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 87.884 59.0296) (end 86.9696 59.0296) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 59.0296) (end 85.09 57.15) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B6523))
  (segment (start 87.884 60.3504) (end 86.9696 60.3504) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 86.9696 60.3504) (end 85.09 62.23) (width 0.25) (layer F.Cu) (net 11) (tstamp 578B651D))
  (segment (start 106.68 142.24) (end 106.68 147.32) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 91.38 125.15) (end 91.38 126.11) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 91.38 126.11) (end 106.68 142.24) (width 0.25) (layer F.Cu) (net 21) (tstamp 578240A6))
  (segment (start 109.22 139.7) (end 114.3 139.7) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 92.13 124.4) (end 92.89 124.4) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 92.89 124.4) (end 109.22 139.7) (width 0.25) (layer F.Cu) (net 22) (tstamp 57823DF7) (status 20))
  (segment (start 116.09 139.7) (end 114.3 139.7) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 109.22 134.62) (end 114.3 134.62) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 92.13 123.4) (end 93.39 123.4) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 93.39 123.4) (end 109.22 134.62) (width 0.25) (layer F.Cu) (net 23) (tstamp 57821592) (status 20))
  (segment (start 116.09 134.62) (end 114.3 134.62) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 116.09 119.38) (end 114.3 119.38) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 109.22 119.38) (end 114.3 119.38) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 92.13 120.4) (end 94.64 120.4) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 94.64 120.4) (end 109.22 119.38) (width 0.25) (layer F.Cu) (net 24) (tstamp 578215E3) (status 20))
  (segment (start 116.09 114.3) (end 114.3 114.3) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 109.22 114.3) (end 114.3 114.3) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 94.14 119.4) (end 109.22 114.3) (width 0.25) (layer F.Cu) (net 25) (tstamp 57823DD7) (status 20))
  (segment (start 92.13 119.4) (end 94.14 119.4) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 83.13 124.4) (end 82.14 124.4) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 82.14 124.4) (end 66.04 139.7) (width 0.25) (layer F.Cu) (net 26) (tstamp 57824066))
  (segment (start 59.17 139.7) (end 60.96 139.7) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 66.04 139.7) (end 60.96 139.7) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 83.13 123.4) (end 81.64 123.4) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 81.64 123.4) (end 66.04 134.62) (width 0.25) (layer F.Cu) (net 27) (tstamp 5782405E))
  (segment (start 59.17 134.62) (end 60.96 134.62) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 66.04 134.62) (end 60.96 134.62) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 59.17 119.38) (end 60.96 119.38) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 66.04 119.38) (end 60.96 119.38) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 83.13 120.4) (end 80.39 120.4) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 80.39 120.4) (end 66.04 119.38) (width 0.25) (layer F.Cu) (net 28) (tstamp 57824046))
  (segment (start 59.17 114.3) (end 60.96 114.3) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 66.04 114.3) (end 60.96 114.3) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 80.89 119.4) (end 66.04 114.3) (width 0.25) (layer F.Cu) (net 29) (tstamp 5782403E))
  (segment (start 83.13 119.4) (end 80.89 119.4) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 104.14 142.24) (end 104.14 147.32) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 90.88 125.15) (end 90.88 126.36) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 90.88 126.36) (end 104.14 142.24) (width 0.25) (layer F.Cu) (net 30) (tstamp 578240A2))
  (segment (start 109.22 137.16) (end 114.3 137.16) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 92.13 123.9) (end 93.139889 123.89737) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 93.139889 123.90263) (end 109.22 137.16) (width 0.25) (layer F.Cu) (net 31) (tstamp 57821567) (status 20))
  (segment (start 116.09 137.16) (end 114.3 137.16) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 109.22 132.08) (end 114.3 132.08) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 93.64 122.9) (end 109.22 132.08) (width 0.25) (layer F.Cu) (net 32) (tstamp 578215A9) (status 20))
  (segment (start 92.13 122.9) (end 93.64 122.9) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 116.09 132.08) (end 114.3 132.08) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 116.09 116.84) (end 114.3 116.84) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 109.22 116.84) (end 114.3 116.84) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 92.13 119.9) (end 94.39 119.9) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 94.39 119.9) (end 109.22 116.84) (width 0.25) (layer F.Cu) (net 33) (tstamp 57823DD3) (status 20))
  (segment (start 116.09 111.76) (end 114.3 111.76) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 109.22 111.76) (end 114.3 111.76) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 92.13 118.9) (end 93.89 118.9) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 93.89 118.9) (end 109.22 111.76) (width 0.25) (layer F.Cu) (net 34) (tstamp 57823DDB) (status 20))
  (segment (start 83.13 123.9) (end 81.89 123.9) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 81.89 123.9) (end 66.04 137.16) (width 0.25) (layer F.Cu) (net 35) (tstamp 57824062))
  (segment (start 59.17 137.16) (end 60.96 137.16) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 66.04 137.16) (end 60.96 137.16) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 81.39 122.9) (end 66.04 132.08) (width 0.25) (layer F.Cu) (net 36) (tstamp 5782405A))
  (segment (start 83.13 122.9) (end 81.39 122.9) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 59.17 132.08) (end 60.96 132.08) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 66.04 132.08) (end 60.96 132.08) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 59.17 116.84) (end 60.96 116.84) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 66.04 116.84) (end 60.96 116.84) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 80.64 119.9) (end 66.04 116.84) (width 0.25) (layer F.Cu) (net 37) (tstamp 57824042))
  (segment (start 83.13 119.9) (end 80.64 119.9) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 59.17 111.76) (end 60.96 111.76) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 66.04 111.76) (end 60.96 111.76) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 81.14 118.9) (end 66.04 111.76) (width 0.25) (layer F.Cu) (net 38) (tstamp 5782403A))
  (segment (start 83.13 118.9) (end 81.14 118.9) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 88.38 116.15) (end 88.38 113.61) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 90.506278 103.395719) (end 89.4962 107.823) (width 0.25) (layer F.Cu) (net 39) (tstamp 578792EB))
  (segment (start 90.640385 102.862089) (end 89.0898 109.3216) (width 0.25) (layer F.Cu) (net 39) (tstamp 578792DE))
  (segment (start 108.585 41.402) (end 108.458 41.402) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 108.458 41.402) (end 92.71 57.15) (width 0.25) (layer F.Cu) (net 40) (tstamp 578B6726))
  (segment (start 90.92 57.15) (end 92.71 57.15) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 89.916 59.0296) (end 90.8304 59.0296) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 90.8304 59.0296) (end 92.71 57.15) (width 0.25) (layer F.Cu) (net 40) (tstamp 578B652A))
  (segment (start 55.13 127) (end 56.63 127) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 118.63 127) (end 120.13 127) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 101.6 149.11) (end 101.6 150.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 74.676 152.134) (end 74.676 150.634) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 76.2 150.61) (end 76.2 149.11) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 76.2 150.61) (end 74.7 150.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 74.7 150.61) (end 74.676 150.634) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843DA8))
  (segment (start 76.2 150.61) (end 65.798 150.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 55.13 139.942) (end 55.13 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843CFC))
  (segment (start 65.798 150.61) (end 55.13 139.942) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843CF4))
  (segment (start 109.22 127) (end 105.41 125.73) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 105.41 125.73) (end 100.2792 123.8878) (width 0.25) (layer F.Cu) (net 40) (tstamp 578790A3))
  (segment (start 109.22 127) (end 105.41 125.73) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 105.41 125.73) (end 101.7778 124.5482) (width 0.25) (layer F.Cu) (net 40) (tstamp 5787909F))
  (segment (start 66.04 127) (end 69.088 125.984) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 69.088 125.984) (end 75.438 123.6338) (width 0.25) (layer F.Cu) (net 40) (tstamp 57879059))
  (segment (start 66.04 127) (end 69.088 125.984) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 69.088 125.984) (end 73.9394 124.2434) (width 0.25) (layer F.Cu) (net 40) (tstamp 57879055))
  (segment (start 76.2 142.24) (end 78.486 138.43) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 78.486 138.43) (end 81.6984 133.0198) (width 0.25) (layer F.Cu) (net 40) (tstamp 5787903A))
  (segment (start 76.2 142.24) (end 78.232 138.938) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 78.232 138.938) (end 80.8348 134.5184) (width 0.25) (layer F.Cu) (net 40) (tstamp 57879036))
  (segment (start 91.44 142.24) (end 90.17 136.144) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 90.17 136.144) (end 89.293 130.7338) (width 0.25) (layer F.Cu) (net 40) (tstamp 57879028))
  (segment (start 101.6 142.24) (end 99.06 138.684) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 99.06 138.684) (end 95.0856 133.1468) (width 0.25) (layer F.Cu) (net 40) (tstamp 57878FF3))
  (segment (start 101.6 142.24) (end 99.06 138.684) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 99.06 138.684) (end 96.0508 134.6454) (width 0.25) (layer F.Cu) (net 40) (tstamp 57878FEF))
  (segment (start 74.676 152.134) (end 100.076 152.134) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 100.076 152.134) (end 101.6 150.61) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843DB8))
  (segment (start 101.6 150.61) (end 109.208 150.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 120.13 139.688) (end 120.13 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843D31))
  (segment (start 109.208 150.61) (end 120.13 139.688) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843D2D))
  (segment (start 120.13 127) (end 120.142 127) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 120.142 127) (end 121.158 125.984) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843BB4))
  (segment (start 121.158 125.984) (end 121.158 48.26) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843BBC))
  (segment (start 121.158 48.26) (end 114.3 41.402) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843BCB))
  (segment (start 114.3 41.402) (end 108.585 41.402) (width 0.25) (layer F.Cu) (net 40) (tstamp 57843BDB))
  (segment (start 109.22 127) (end 118.63 127) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 66.04 127) (end 56.63 127) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 101.6 147.32) (end 99.06 144.78) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 93.98 144.78) (end 99.06 144.78) (width 0.25) (layer F.Cu) (net 40) (tstamp 57839B87))
  (segment (start 93.98 144.78) (end 91.44 142.24) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 101.6 142.24) (end 101.6 147.32) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 101.6 147.32) (end 101.6 149.11) (width 0.25) (layer F.Cu) (net 40) (tstamp 57839B58))
  (segment (start 76.2 142.24) (end 76.2 149.11) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 90.38 126.61) (end 101.6 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 5782409E))
  (segment (start 94.14 121.9) (end 109.22 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 578215BB) (status 20))
  (segment (start 80.89 121.9) (end 66.04 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 57824056))
  (segment (start 90.38 125.15) (end 90.38 126.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 88.38 125.15) (end 88.38 127.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 88.38 127.61) (end 91.44 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 5782408E))
  (segment (start 85.38 125.15) (end 85.38 126.86) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 83.13 121.9) (end 80.89 121.9) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 92.13 121.9) (end 94.14 121.9) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 85.38 126.86) (end 76.2 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 57824076))
  (segment (start 89.916 83.2104) (end 90.8304 83.2104) (width 0.25) (layer F.Cu) (net 41))
  (segment (start 89.916 60.3504) (end 90.8304 60.3504) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 89.916 71.7804) (end 90.8304 71.7804) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 74.549 88.7984) (end 95.0976 88.7984) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 63.9064 99.441) (end 74.549 88.7984) (width 0.25) (layer B.Cu) (net 44) (tstamp 5784392D))
  (segment (start 66.04 101.6) (end 63.9064 99.441) (width 0.25) (layer B.Cu) (net 44))
  (segment (start 95.0976 88.7984) (end 111.76 72.136) (width 0.25) (layer B.Cu) (net 44) (tstamp 578B66B6))
  (segment (start 83.13 116.9) (end 82.14 116.9) (width 0.25) (layer F.Cu) (net 44))
  (segment (start 82.14 116.9) (end 66.04 101.6) (width 0.25) (layer F.Cu) (net 44) (tstamp 5782402A))
  (segment (start 74.269602 88.239298) (end 93.116702 88.239298) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 93.116702 88.239298) (end 111.76 69.596) (width 0.25) (layer B.Cu) (net 45) (tstamp 578B66D1))
  (segment (start 59.2328 103.0986) (end 74.269602 88.239298) (width 0.25) (layer B.Cu) (net 45) (tstamp 5784394E))
  (segment (start 74.269602 88.239298) (end 74.295 88.2142) (width 0.25) (layer B.Cu) (net 45) (tstamp 578B66CF))
  (segment (start 66.04 109.22) (end 59.2328 103.0986) (width 0.25) (layer B.Cu) (net 45))
  (segment (start 81.39 118.4) (end 66.04 109.22) (width 0.25) (layer F.Cu) (net 45) (tstamp 57824036))
  (segment (start 83.13 118.4) (end 81.39 118.4) (width 0.25) (layer F.Cu) (net 45))
  (segment (start 104.14 99.06) (end 109.22 93.98) (width 0.25) (layer F.Cu) (net 46))
  (segment (start 109.22 69.596) (end 111.76 67.056) (width 0.25) (layer F.Cu) (net 46) (tstamp 5787BE71))
  (segment (start 109.22 93.98) (end 109.22 69.596) (width 0.25) (layer F.Cu) (net 46) (tstamp 5787BE6E))
  (segment (start 90.88 116.15) (end 90.88 114.86) (width 0.25) (layer F.Cu) (net 46))
  (segment (start 90.88 114.86) (end 104.14 99.06) (width 0.25) (layer F.Cu) (net 46) (tstamp 57823FEA))
  (segment (start 101.6 99.06) (end 106.68 93.98) (width 0.25) (layer F.Cu) (net 47))
  (segment (start 106.68 64.516) (end 111.76 59.436) (width 0.25) (layer F.Cu) (net 47) (tstamp 5787BE8B))
  (segment (start 106.68 93.98) (end 106.68 64.516) (width 0.25) (layer F.Cu) (net 47) (tstamp 5787BE7F))
  (segment (start 90.38 116.15) (end 90.38 114.61) (width 0.25) (layer F.Cu) (net 47))
  (segment (start 90.38 114.61) (end 101.6 99.06) (width 0.25) (layer F.Cu) (net 47) (tstamp 57823FEE))
  (segment (start 73.66 99.06) (end 84.5566 89.1286) (width 0.25) (layer B.Cu) (net 49))
  (segment (start 84.5566 89.1286) (end 98.806 89.281) (width 0.25) (layer B.Cu) (net 49) (tstamp 5784C53B))
  (segment (start 84.88 114.61) (end 73.66 99.06) (width 0.25) (layer F.Cu) (net 49) (tstamp 5782401E))
  (segment (start 84.88 116.15) (end 84.88 114.61) (width 0.25) (layer F.Cu) (net 49))
  (segment (start 98.806 89.281) (end 111.76 76.2) (width 0.25) (layer B.Cu) (net 49) (tstamp 5784C564))
  (segment (start 76.2 99.06) (end 76.2 97.282) (width 0.25) (layer B.Cu) (net 50))
  (segment (start 76.2 97.282) (end 84.5312 89.5604) (width 0.25) (layer B.Cu) (net 50) (tstamp 5784C575))
  (segment (start 85.38 114.36) (end 76.2 99.06) (width 0.25) (layer F.Cu) (net 50) (tstamp 5782401A))
  (segment (start 85.38 116.15) (end 85.38 114.36) (width 0.25) (layer F.Cu) (net 50))
  (segment (start 84.5312 89.5604) (end 100.8888 89.6112) (width 0.25) (layer B.Cu) (net 50) (tstamp 5784C585))
  (segment (start 100.8888 89.6112) (end 111.76 78.74) (width 0.25) (layer B.Cu) (net 50) (tstamp 5784C596))
  (segment (start 78.74 99.06) (end 80.5942 96.139) (width 0.25) (layer B.Cu) (net 51))
  (segment (start 80.5942 96.139) (end 97.282 96.1644) (width 0.25) (layer B.Cu) (net 51) (tstamp 5784C59E))
  (segment (start 85.88 116.15) (end 85.88 114.11) (width 0.25) (layer F.Cu) (net 51))
  (segment (start 85.88 114.11) (end 78.74 99.06) (width 0.25) (layer F.Cu) (net 51) (tstamp 57824016))
  (segment (start 97.282 96.1644) (end 103.886 89.154) (width 0.25) (layer B.Cu) (net 51) (tstamp 5784C5AA))
  (segment (start 103.886 89.154) (end 111.76 81.28) (width 0.25) (layer B.Cu) (net 51) (tstamp 5784C5B0))
  (segment (start 105.918 89.662) (end 111.76 83.82) (width 0.25) (layer B.Cu) (net 52) (tstamp 5784C5CA))
  (segment (start 99.6188 96.647) (end 105.918 89.662) (width 0.25) (layer B.Cu) (net 52) (tstamp 5784C5C5))
  (segment (start 83.3882 96.4692) (end 99.6188 96.647) (width 0.25) (layer B.Cu) (net 52) (tstamp 5784C5B9))
  (segment (start 81.28 99.06) (end 83.3882 96.4692) (width 0.25) (layer B.Cu) (net 52))
  (segment (start 86.38 116.15) (end 86.38 113.86) (width 0.25) (layer F.Cu) (net 52))
  (segment (start 86.38 113.86) (end 81.28 99.06) (width 0.25) (layer F.Cu) (net 52) (tstamp 57824012))
  (segment (start 101.6762 97.0026) (end 111.76 86.36) (width 0.25) (layer B.Cu) (net 53) (tstamp 5784C5EF))
  (segment (start 87.3506 96.7994) (end 101.6762 97.0026) (width 0.25) (layer B.Cu) (net 53) (tstamp 5784C5E3))
  (segment (start 85.8266 96.8502) (end 87.3506 96.7994) (width 0.25) (layer B.Cu) (net 53) (tstamp 5784C5D1))
  (segment (start 83.82 99.06) (end 85.8266 96.8502) (width 0.25) (layer B.Cu) (net 53))
  (segment (start 86.88 116.15) (end 86.88 113.61) (width 0.25) (layer F.Cu) (net 53))
  (segment (start 86.88 113.61) (end 83.82 99.06) (width 0.25) (layer F.Cu) (net 53) (tstamp 5782400E))
  (segment (start 103.8352 97.3328) (end 111.76 88.9) (width 0.25) (layer B.Cu) (net 54) (tstamp 5784C602))
  (segment (start 88.6206 97.155) (end 103.8352 97.3328) (width 0.25) (layer B.Cu) (net 54) (tstamp 5784C5FA))
  (segment (start 86.36 99.06) (end 88.6206 97.155) (width 0.25) (layer B.Cu) (net 54))
  (segment (start 87.38 116.15) (end 87.38 113.36) (width 0.25) (layer F.Cu) (net 54))
  (segment (start 87.38 113.36) (end 86.36 99.06) (width 0.25) (layer F.Cu) (net 54) (tstamp 5782400A))
  (segment (start 74.1045 88.7095) (end 93.5355 88.7095) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 95.25 82.55) (end 92.71 80.01) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B6711))
  (segment (start 95.25 86.995) (end 95.25 82.55) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B6707))
  (segment (start 93.5355 88.7095) (end 95.25 86.995) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B66EF))
  (segment (start 96.52 93.98) (end 96.52 83.82) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 96.52 83.82) (end 92.71 80.01) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B66E2))
  (segment (start 88.9 99.06) (end 91.44 96.52) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 93.98 96.52) (end 96.52 93.98) (width 0.25) (layer F.Cu) (net 55) (tstamp 5782BEB8))
  (segment (start 91.44 96.52) (end 93.98 96.52) (width 0.25) (layer F.Cu) (net 55) (tstamp 5782BEB3))
  (segment (start 90.92 80.01) (end 92.71 80.01) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 89.916 81.8896) (end 90.8304 81.8896) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 90.8304 81.8896) (end 92.71 80.01) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B65B0))
  (segment (start 88.9 99.06) (end 88.574172 103.628525) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 88.574172 103.628525) (end 88.2262 110.8202) (width 0.25) (layer F.Cu) (net 55) (tstamp 578792BF))
  (segment (start 88.9 99.06) (end 88.610336 103.121456) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 88.610336 103.121456) (end 87.9468 112.3188) (width 0.25) (layer F.Cu) (net 55) (tstamp 578792B7))
  (segment (start 78.74 150.61) (end 78.74 149.11) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 78.74 150.61) (end 78.74 150.622) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 78.74 150.622) (end 77.978 151.384) (width 0.25) (layer F.Cu) (net 55) (tstamp 57843C2F))
  (segment (start 77.978 151.384) (end 64.77 151.384) (width 0.25) (layer F.Cu) (net 55) (tstamp 57843C37))
  (segment (start 64.77 151.384) (end 54.102 140.97) (width 0.25) (layer F.Cu) (net 55) (tstamp 57843C44))
  (segment (start 54.102 140.97) (end 54.102 108.712) (width 0.25) (layer F.Cu) (net 55) (tstamp 57843C50))
  (segment (start 54.102 108.712) (end 74.1045 88.7095) (width 0.25) (layer F.Cu) (net 55) (tstamp 57843C61))
  (segment (start 74.1045 88.7095) (end 74.168 88.646) (width 0.25) (layer F.Cu) (net 55) (tstamp 578B66ED))
  (segment (start 86.36 142.24) (end 83.82 144.78) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 83.82 144.78) (end 81.28 144.78) (width 0.25) (layer F.Cu) (net 55) (tstamp 57839B9C))
  (segment (start 78.74 147.32) (end 81.28 144.78) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 81.28 144.78) (end 83.82 142.24) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 81.28 142.24) (end 78.74 144.78) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 78.74 144.78) (end 78.74 147.32) (width 0.25) (layer F.Cu) (net 55) (tstamp 57839B3C))
  (segment (start 78.74 147.32) (end 78.74 149.11) (width 0.25) (layer F.Cu) (net 55) (tstamp 57839B42))
  (segment (start 91.38 115.11) (end 106.68 99.06) (width 0.25) (layer F.Cu) (net 55) (tstamp 57823FE6))
  (segment (start 87.88 113.36) (end 88.9 99.06) (width 0.25) (layer F.Cu) (net 55) (tstamp 57824006))
  (segment (start 86.38 127.36) (end 81.28 142.24) (width 0.25) (layer F.Cu) (net 55) (tstamp 5782407E))
  (segment (start 87.38 125.15) (end 87.38 127.86) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 87.38 127.86) (end 86.36 142.24) (width 0.25) (layer F.Cu) (net 55) (tstamp 57824086))
  (segment (start 86.88 125.15) (end 86.88 127.61) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 86.88 127.61) (end 83.82 142.24) (width 0.25) (layer F.Cu) (net 55) (tstamp 57824082))
  (segment (start 86.38 125.15) (end 86.38 127.36) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 87.88 116.15) (end 87.88 113.36) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 91.38 116.15) (end 91.38 115.11) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 91.44 99.06) (end 90.506278 103.395719) (width 0.25) (layer F.Cu) (net 56))
  (segment (start 91.44 99.06) (end 90.640385 102.862089) (width 0.25) (layer F.Cu) (net 56))
  (segment (start 88.38 113.61) (end 91.44 99.06) (width 0.25) (layer F.Cu) (net 56) (tstamp 57824002))
  (segment (start 73.66 142.24) (end 75.692 139.446) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 84.88 126.61) (end 73.66 142.24) (width 0.25) (layer F.Cu) (net 57) (tstamp 57824072))
  (segment (start 93.98 142.24) (end 92.202 136.906) (width 0.25) (layer F.Cu) (net 58))
  (segment (start 88.88 127.36) (end 93.98 142.24) (width 0.25) (layer F.Cu) (net 58) (tstamp 57824092))
  (segment (start 93.64 118.4) (end 109.22 109.22) (width 0.25) (layer F.Cu) (net 59) (tstamp 57823DDF) (status 20))
  (segment (start 92.13 118.4) (end 93.64 118.4) (width 0.25) (layer F.Cu) (net 59))
  (segment (start 93.39 117.9) (end 109.22 106.68) (width 0.25) (layer F.Cu) (net 60) (tstamp 57823DE3) (status 20))
  (segment (start 92.13 117.9) (end 93.39 117.9) (width 0.25) (layer F.Cu) (net 60))
  (segment (start 92.13 117.4) (end 93.14 117.4) (width 0.25) (layer F.Cu) (net 61))
  (segment (start 93.14 117.4) (end 109.22 104.14) (width 0.25) (layer F.Cu) (net 61) (tstamp 57823DE7) (status 20))
  (segment (start 92.89 116.9) (end 109.22 101.6) (width 0.25) (layer F.Cu) (net 62) (tstamp 57823DEB) (status 20))
  (segment (start 92.13 116.9) (end 92.89 116.9) (width 0.25) (layer F.Cu) (net 62))
  (segment (start 71.12 99.06) (end 71.12 99.368196) (width 0.25) (layer F.Cu) (net 63))
  (segment (start 71.12 99.368196) (end 77.29389 105.542086) (width 0.25) (layer F.Cu) (net 63) (tstamp 5787906F))
  (segment (start 84.38 116.15) (end 84.38 114.86) (width 0.25) (layer F.Cu) (net 63))
  (segment (start 84.38 114.86) (end 71.12 99.06) (width 0.25) (layer F.Cu) (net 63) (tstamp 57824022))
  (segment (start 68.58 99.06) (end 68.58 100.191804) (width 0.25) (layer F.Cu) (net 64))
  (segment (start 68.58 100.191804) (end 71.76611 103.377914) (width 0.25) (layer F.Cu) (net 64) (tstamp 5787906B))
  (segment (start 83.88 115.11) (end 68.58 99.06) (width 0.25) (layer F.Cu) (net 64) (tstamp 57824026))
  (segment (start 83.88 116.15) (end 83.88 115.11) (width 0.25) (layer F.Cu) (net 64))
  (segment (start 83.13 117.4) (end 81.89 117.4) (width 0.25) (layer F.Cu) (net 65))
  (segment (start 81.89 117.4) (end 66.04 104.14) (width 0.25) (layer F.Cu) (net 65) (tstamp 5782402E))
  (segment (start 81.64 117.9) (end 66.04 106.68) (width 0.25) (layer F.Cu) (net 66) (tstamp 57824032))
  (segment (start 83.13 117.9) (end 81.64 117.9) (width 0.25) (layer F.Cu) (net 66))
  (segment (start 68.58 142.24) (end 68.58 141.94974) (width 0.25) (layer F.Cu) (net 67))
  (segment (start 68.58 141.94974) (end 76.01388 134.51586) (width 0.25) (layer F.Cu) (net 67) (tstamp 5787904A))
  (segment (start 83.88 126.11) (end 68.58 142.24) (width 0.25) (layer F.Cu) (net 67) (tstamp 5782406A))
  (segment (start 83.88 125.15) (end 83.88 126.11) (width 0.25) (layer F.Cu) (net 67))
  (segment (start 57.67 132.08) (end 55.88 132.08) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 134.62) (end 55.88 134.62) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 137.16) (end 55.88 137.16) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 139.7) (end 55.88 139.7) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 114.3) (end 55.88 114.3) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 116.84) (end 55.88 116.84) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 57.67 119.38) (end 55.88 119.38) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 139.7) (end 119.38 139.7) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 137.16) (end 119.38 137.16) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 134.62) (end 119.38 134.62) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 132.08) (end 119.38 132.08) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 119.38) (end 119.38 119.38) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 116.84) (end 119.38 116.84) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 117.59 114.3) (end 119.38 114.3) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 55.88 113.55) (end 57.67 111.76) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393B0))
  (segment (start 55.88 139.7) (end 55.88 137.16) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393AF))
  (segment (start 55.88 137.16) (end 55.88 134.62) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393C7))
  (segment (start 55.88 134.62) (end 55.88 132.08) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393CB))
  (segment (start 55.88 132.08) (end 55.88 119.38) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393CF))
  (segment (start 55.88 119.38) (end 55.88 116.84) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393D3))
  (segment (start 55.88 116.84) (end 55.88 114.3) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393D7))
  (segment (start 55.88 114.3) (end 55.88 113.55) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393DB))
  (segment (start 66.04 149.86) (end 55.88 139.7) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393AE))
  (segment (start 81.28 149.86) (end 66.04 149.86) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393AD))
  (segment (start 119.38 113.55) (end 117.59 111.76) (width 0.25) (layer F.Cu) (net 68) (tstamp 57839380))
  (segment (start 119.38 139.7) (end 119.38 137.16) (width 0.25) (layer F.Cu) (net 68) (tstamp 5783937F))
  (segment (start 119.38 137.16) (end 119.38 134.62) (width 0.25) (layer F.Cu) (net 68) (tstamp 578393A1))
  (segment (start 119.38 134.62) (end 119.38 132.08) (width 0.25) (layer F.Cu) (net 68) (tstamp 5783939D))
  (segment (start 119.38 132.08) (end 119.38 119.38) (width 0.25) (layer F.Cu) (net 68) (tstamp 57839399))
  (segment (start 119.38 119.38) (end 119.38 116.84) (width 0.25) (layer F.Cu) (net 68) (tstamp 57839395))
  (segment (start 119.38 116.84) (end 119.38 114.3) (width 0.25) (layer F.Cu) (net 68) (tstamp 57839391))
  (segment (start 119.38 114.3) (end 119.38 113.55) (width 0.25) (layer F.Cu) (net 68) (tstamp 5783938D))
  (segment (start 109.22 149.86) (end 119.38 139.7) (width 0.25) (layer F.Cu) (net 68) (tstamp 5783937E))
  (segment (start 96.52 149.86) (end 109.22 149.86) (width 0.25) (layer F.Cu) (net 68) (tstamp 5783937D))
  (segment (start 88.9 142.24) (end 81.28 149.86) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 88.9 142.24) (end 96.52 149.86) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 87.88 127.86) (end 88.9 142.24) (width 0.25) (layer F.Cu) (net 68) (tstamp 5782408A))
  (segment (start 87.88 125.15) (end 87.88 127.86) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 108.6358 52.705) (end 108.585 52.705) (width 0.25) (layer B.Cu) (net 69))
  (segment (start 108.585 52.705) (end 92.71 68.58) (width 0.25) (layer B.Cu) (net 69) (tstamp 578B6733))
  (segment (start 120.142 121.92) (end 120.1928 48.6664) (width 0.25) (layer B.Cu) (net 69))
  (segment (start 108.6358 42.9768) (end 108.6358 52.705) (width 0.25) (layer B.Cu) (net 69) (tstamp 578439E2))
  (segment (start 108.6358 52.705) (end 108.6358 52.8574) (width 0.25) (layer B.Cu) (net 69) (tstamp 578B6731))
  (segment (start 114.046 42.6974) (end 108.6358 42.9768) (width 0.25) (layer B.Cu) (net 69) (tstamp 578439D0))
  (segment (start 120.1928 48.6664) (end 114.046 42.6974) (width 0.25) (layer B.Cu) (net 69) (tstamp 578439AE))
  (segment (start 89.916 70.4596) (end 90.8304 70.4596) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 90.8304 70.4596) (end 92.71 68.58) (width 0.25) (layer F.Cu) (net 69) (tstamp 578B659F))
  (segment (start 90.92 68.58) (end 92.71 68.58) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 56.63 121.92) (end 55.13 121.92) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 118.63 121.92) (end 120.13 121.92) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 109.22 121.92) (end 105.41 121.666) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 105.41 121.666) (end 101.7778 121.3732) (width 0.25) (layer F.Cu) (net 69) (tstamp 57879094))
  (segment (start 109.22 121.92) (end 105.664 121.666) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 105.664 121.666) (end 103.2764 121.6272) (width 0.25) (layer F.Cu) (net 69) (tstamp 57879091))
  (segment (start 66.04 121.92) (end 69.85 121.666) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 69.85 121.666) (end 73.9394 121.297) (width 0.25) (layer F.Cu) (net 69) (tstamp 57879068))
  (segment (start 66.04 121.92) (end 69.85 121.666) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 69.85 121.666) (end 72.4408 121.5002) (width 0.25) (layer F.Cu) (net 69) (tstamp 57879065))
  (segment (start 109.22 121.92) (end 118.63 121.92) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 66.04 121.92) (end 56.63 121.92) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 109.22 121.92) (end 109.74 121.92) (width 0.25) (layer F.Cu) (net 69) (status 30))
  (segment (start 80.39 120.9) (end 66.04 121.92) (width 0.25) (layer F.Cu) (net 69) (tstamp 5782404A))
  (segment (start 94.64 120.9) (end 109.22 121.92) (width 0.25) (layer F.Cu) (net 69) (tstamp 578215D7) (status 20))
  (segment (start 83.13 120.9) (end 80.39 120.9) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 92.13 120.9) (end 94.64 120.9) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 90.8304 83.2104) (end 92.71 85.09) (width 0.25) (layer F.Cu) (net 70) (tstamp 578B65B3))
  (segment (start 90.8304 60.3504) (end 92.71 62.23) (width 0.25) (layer F.Cu) (net 72) (tstamp 578B653A))
  (segment (start 90.8304 71.7804) (end 92.71 73.66) (width 0.25) (layer F.Cu) (net 74) (tstamp 578B65A2))
  (segment (start 75.692 139.446) (end 80.3028 133.01726) (width 0.25) (layer F.Cu) (net 76) (tstamp 5787903E))
  (segment (start 84.88 125.15) (end 84.88 126.61) (width 0.25) (layer F.Cu) (net 76))
  (segment (start 92.202 136.906) (end 90.69 132.969) (width 0.25) (layer F.Cu) (net 77) (tstamp 578791EB))
  (segment (start 88.88 125.15) (end 88.88 127.36) (width 0.25) (layer F.Cu) (net 77))
  (segment (start 107.43 68.58) (end 107.696 68.58) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 107.696 68.58) (end 111.76 64.516) (width 0.25) (layer F.Cu) (net 78) (tstamp 5787BF8F))
  (segment (start 105.93 68.58) (end 107.43 68.58) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 99.06 99.06) (end 104.14 93.98) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 104.14 70.37) (end 105.93 68.58) (width 0.25) (layer F.Cu) (net 78) (tstamp 5787BF9A))
  (segment (start 104.14 93.98) (end 104.14 70.37) (width 0.25) (layer F.Cu) (net 78) (tstamp 5787BF92))
  (segment (start 89.88 116.15) (end 89.88 114.36) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 89.88 114.36) (end 99.06 99.06) (width 0.25) (layer F.Cu) (net 78) (tstamp 57823FF2))
  (segment (start 107.43 66.04) (end 107.696 66.04) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 107.696 66.04) (end 111.76 61.976) (width 0.25) (layer F.Cu) (net 79) (tstamp 5787BF8C))
  (segment (start 105.93 66.04) (end 107.43 66.04) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 96.52 99.06) (end 101.6 93.98) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 101.6 70.37) (end 105.93 66.04) (width 0.25) (layer F.Cu) (net 79) (tstamp 5787BFA2))
  (segment (start 101.6 93.98) (end 101.6 70.37) (width 0.25) (layer F.Cu) (net 79) (tstamp 5787BFA0))
  (segment (start 89.38 116.15) (end 89.38 114.11) (width 0.25) (layer F.Cu) (net 79))
  (segment (start 89.38 114.11) (end 96.52 99.06) (width 0.25) (layer F.Cu) (net 79) (tstamp 57823FF9))

)
