(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)

  (general
    (links 212)
    (no_connects 86)
    (area 52.599999 29.499999 123.700001 156.700001)
    (thickness 1.6)
    (drawings 4)
    (tracks 360)
    (zones 0)
    (modules 57)
    (nets 80)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00120_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/dmitryneuro/git.neuroidss.local/FreeSmartEEG/KiCad/out/))
  )

  (net 0 "")
  (net 1 _IO11)
  (net 2 IO12)
  (net 3 IO13)
  (net 4 AVSS)
  (net 5 AREF)
  (net 6 SDA)
  (net 7 SCL)
  (net 8 5V)
  (net 9 RESET)
  (net 10 IOREF)
  (net 11 3.3V)
  (net 12 VIN)
  (net 13 RX)
  (net 14 TX)
  (net 15 A0)
  (net 16 A1)
  (net 17 A2)
  (net 18 A3)
  (net 19 A4)
  (net 20 A5)
  (net 21 AUXAIN-)
  (net 22 AIN0-)
  (net 23 AIN1-)
  (net 24 AIN2-)
  (net 25 AIN3-)
  (net 26 AIN4-)
  (net 27 AIN5-)
  (net 28 AIN6-)
  (net 29 AIN7-)
  (net 30 AUXAIN+)
  (net 31 AIN0+)
  (net 32 AIN1+)
  (net 33 AIN2+)
  (net 34 AIN3+)
  (net 35 AIN4+)
  (net 36 AIN5+)
  (net 37 AIN6+)
  (net 38 AIN7+)
  (net 39 "Net-(C5-Pad2)")
  (net 40 AVDD)
  (net 41 "Net-(U2-Pad4)")
  (net 42 "Net-(U3-Pad4)")
  (net 43 "Net-(U4-Pad4)")
  (net 44 START)
  (net 45 ADC_RESET)
  (net 46 CS)
  (net 47 SCLK)
  (net 48 SDI)
  (net 49 SDO)
  (net 50 MCU_RESET)
  (net 51 DRDY)
  (net 52 DCLK)
  (net 53 DOUT0)
  (net 54 DOUT1)
  (net 55 DOUT2)
  (net 56 DOUT3)
  (net 57 CLK_SEL)
  (net 58 "Net-(P9-Pad7)")
  (net 59 "Net-(P11-Pad3)")
  (net 60 "Net-(P11-Pad11)")
  (net 61 GPIO0)
  (net 62 GPIO1)
  (net 63 GPIO2)
  (net 64 ALERT)
  (net 65 XTAL1)
  (net 66 XTAL2)
  (net 67 SYNC_OUT)
  (net 68 SYNC_IN)
  (net 69 REF_OUT)
  (net 70 VCM)
  (net 71 OUT_VREF)
  (net 72 "Net-(P13-Pad1)")
  (net 73 "Net-(P13-Pad2)")
  (net 74 "Net-(P15-Pad1)")
  (net 75 "Net-(P15-Pad2)")
  (net 76 "Net-(P17-Pad1)")
  (net 77 "Net-(P17-Pad2)")
  (net 78 "Net-(C9-Pad2)")
  (net 79 "Net-(C19-Pad1)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3V)
    (add_net 5V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net ADC_RESET)
    (add_net AIN0+)
    (add_net AIN0-)
    (add_net AIN1+)
    (add_net AIN1-)
    (add_net AIN2+)
    (add_net AIN2-)
    (add_net AIN3+)
    (add_net AIN3-)
    (add_net AIN4+)
    (add_net AIN4-)
    (add_net AIN5+)
    (add_net AIN5-)
    (add_net AIN6+)
    (add_net AIN6-)
    (add_net AIN7+)
    (add_net AIN7-)
    (add_net ALERT)
    (add_net AREF)
    (add_net AUXAIN+)
    (add_net AUXAIN-)
    (add_net AVDD)
    (add_net AVSS)
    (add_net CLK_SEL)
    (add_net CS)
    (add_net DCLK)
    (add_net DOUT0)
    (add_net DOUT1)
    (add_net DOUT2)
    (add_net DOUT3)
    (add_net DRDY)
    (add_net GPIO0)
    (add_net GPIO1)
    (add_net GPIO2)
    (add_net IO12)
    (add_net IO13)
    (add_net IOREF)
    (add_net MCU_RESET)
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(P11-Pad11)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P13-Pad1)")
    (add_net "Net-(P13-Pad2)")
    (add_net "Net-(P15-Pad1)")
    (add_net "Net-(P15-Pad2)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(P17-Pad2)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad4)")
    (add_net OUT_VREF)
    (add_net REF_OUT)
    (add_net RESET)
    (add_net RX)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net SDI)
    (add_net SDO)
    (add_net START)
    (add_net SYNC_IN)
    (add_net SYNC_OUT)
    (add_net TX)
    (add_net VCM)
    (add_net VIN)
    (add_net XTAL1)
    (add_net XTAL2)
    (add_net _IO11)
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 57838D4D)
    (at 59.69 128.27)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 57838D40)
    (at 60.96 130.81)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 57838AA2)
    (at 115.57 128.27)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 57838A96)
    (at 114.3 130.81)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 578264ED)
    (at 115.57 123.19)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 578264BC)
    (at 114.3 125.73)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 578263D4)
    (at 59.69 123.19)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LFCSP-64-1EP_9x9mm_Pitch0.5mm (layer F.Cu) (tedit 57821FA2) (tstamp 57804CFA)
    (at 87.63 120.65 180)
    (descr "64-Lead Plastic Quad Flat, No Lead Package (MR) - 9x9x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "64-pin LFCSP 0.5")
    (path /577FE1B1)
    (attr smd)
    (fp_text reference U1 (at 0 -5.875 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value AD7779 (at 0 5.875 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -5.15 -5.15) (end -5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.15 -5.15) (end 5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 -5.15) (end 5.15 -5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 5.15) (end 5.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.7 -4.7) (end 4.7 -4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 4.7) (end -4.7 4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 4.7) (end 4.7 4.125) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 -4.7) (end -4.125 -4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.7 4.7) (end -4.125 4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 4.7) (end 4.125 4.7) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.7 -4.7) (end 4.125 -4.7) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -4.5 -3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 AIN0-))
    (pad 2 smd rect (at -4.5 -3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 AIN0+))
    (pad 3 smd rect (at -4.5 -2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 AIN1-))
    (pad 4 smd rect (at -4.5 -2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 AIN1+))
    (pad 5 smd rect (at -4.5 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 6 smd rect (at -4.5 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 7 smd rect (at -4.5 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 8 smd rect (at -4.5 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (pad 9 smd rect (at -4.5 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 AIN2-))
    (pad 10 smd rect (at -4.5 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 AIN2+))
    (pad 11 smd rect (at -4.5 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 AIN3-))
    (pad 12 smd rect (at -4.5 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 AIN3+))
    (pad 13 smd rect (at -4.5 2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 GPIO0))
    (pad 14 smd rect (at -4.5 2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 GPIO1))
    (pad 15 smd rect (at -4.5 3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 GPIO2))
    (pad 16 smd rect (at -4.5 3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 ALERT))
    (pad 17 smd rect (at -3.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (pad 18 smd rect (at -3.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 CS))
    (pad 19 smd rect (at -2.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 SCLK))
    (pad 20 smd rect (at -2.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 SDI))
    (pad 21 smd rect (at -1.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 SDO))
    (pad 22 smd rect (at -1.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 23 smd rect (at -0.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (pad 24 smd rect (at -0.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (pad 25 smd rect (at 0.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 DOUT3))
    (pad 26 smd rect (at 0.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 DOUT2))
    (pad 27 smd rect (at 1.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 DOUT1))
    (pad 28 smd rect (at 1.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 DOUT0))
    (pad 29 smd rect (at 2.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 DCLK))
    (pad 30 smd rect (at 2.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 DRDY))
    (pad 31 smd rect (at 3.25 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 XTAL1))
    (pad 32 smd rect (at 3.75 4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 XTAL2))
    (pad 33 smd rect (at 4.5 3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 START))
    (pad 34 smd rect (at 4.5 3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 SYNC_OUT))
    (pad 35 smd rect (at 4.5 2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 SYNC_IN))
    (pad 36 smd rect (at 4.5 2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 ADC_RESET))
    (pad 37 smd rect (at 4.5 1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 AIN7+))
    (pad 38 smd rect (at 4.5 1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 AIN7-))
    (pad 39 smd rect (at 4.5 0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 AIN6+))
    (pad 40 smd rect (at 4.5 0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 AIN6-))
    (pad 41 smd rect (at 4.5 -0.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (pad 42 smd rect (at 4.5 -0.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 43 smd rect (at 4.5 -1.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 44 smd rect (at 4.5 -1.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 45 smd rect (at 4.5 -2.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 AIN5+))
    (pad 46 smd rect (at 4.5 -2.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 AIN5-))
    (pad 47 smd rect (at 4.5 -3.25 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 AIN4+))
    (pad 48 smd rect (at 4.5 -3.75 180) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 AIN4-))
    (pad 49 smd rect (at 3.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 REF_OUT))
    (pad 50 smd rect (at 3.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 51 smd rect (at 2.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C9-Pad2)"))
    (pad 52 smd rect (at 2.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 53 smd rect (at 1.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 54 smd rect (at 1.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (pad 55 smd rect (at 0.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (pad 56 smd rect (at 0.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (pad 57 smd rect (at -0.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 VCM))
    (pad 58 smd rect (at -0.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 59 smd rect (at -1.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C19-Pad1)"))
    (pad 60 smd rect (at -1.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 61 smd rect (at -2.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 62 smd rect (at -2.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 63 smd rect (at -3.25 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 AUXAIN+))
    (pad 64 smd rect (at -3.75 -4.5 270) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 AUXAIN-))
    (pad 65 smd rect (at 2.85 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 2.85 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at 0.95 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -0.95 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 -0.95 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (pad 65 smd rect (at -2.85 -2.85 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FED9) (tstamp 57833DD7)
    (at 93.98 73.66 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DBCD)
    (fp_text reference P17 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(P17-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(P17-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 OUT_VREF))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FED1) (tstamp 57833DC6)
    (at 83.82 68.58)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DB30)
    (fp_text reference P16 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FECB) (tstamp 57833DB5)
    (at 93.98 60.96 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783DA96)
    (fp_text reference P15 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(P15-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(P15-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FEC5) (tstamp 57833DA4)
    (at 83.82 55.88)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D9FF)
    (fp_text reference P14 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FE32) (tstamp 57833D93)
    (at 93.98 86.36 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D91F)
    (fp_text reference P13 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(P13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(P13-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5FA) (tstamp 57833B8C)
    (at 68.58 142.24 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830FDE)
    (fp_text reference P11 (at 0 -5.1 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_AD7779_4 (at 0 -3.1 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 REF_OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P11-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 VCM))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P11-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AUXAIN+))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 AUXAIN-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5F2) (tstamp 57833B6E)
    (at 66.04 101.6)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830EE7)
    (fp_text reference P10 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_AD7779_3 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 START))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 SYNC_OUT))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 SYNC_IN))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 ADC_RESET))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 AIN7+))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 AIN7-))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 AIN6+))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 AIN6-))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 OUT_VREF))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 AIN5+))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 AIN5-))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 AIN4+))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 AIN4-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5EB) (tstamp 57833B50)
    (at 106.68 99.06 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830E1B)
    (fp_text reference P9 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_AD7779_2 (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 CS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 SCLK))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 SDI))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 SDO))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P9-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 CLK_SEL))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 DOUT3))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 DOUT2))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 DOUT1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 DOUT0))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 DCLK))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 DRDY))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 XTAL1))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 XTAL2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57804FF2) (tstamp 57833A2E)
    (at 88.9 83.82 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE273)
    (attr smd)
    (fp_text reference U2 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-3.3Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57804FF9) (tstamp 57833A20)
    (at 88.9 58.42 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE246)
    (attr smd)
    (fp_text reference U3 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-3.3Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 0) (tstamp 57804D34)
    (at 111.76 72.136 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE5A9)
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DIGITAL(_PWM)" (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 24.65) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 24.13) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 START))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 ADC_RESET))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 CS))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 SCLK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 SDI))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 SDO))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 AREF))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 SDA))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 SCL))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B) (tstamp 57804D3E)
    (at 91.44 91.567 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57801C6A)
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ICSP (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 0 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.3 -1.75) (end 4.3 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 4.3 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 4.3 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 3.81 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 6.35) (end 3.81 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end -1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 -1.27) (end 1.27 -1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.81 1.27) (end 3.81 -1.27) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 IO12))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 IO13))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 _IO11))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0) (tstamp 57804D4A)
    (at 63.5 58.42)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE40C)
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value POWER (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 AREF))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 IOREF))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 MCU_RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 5V))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 VIN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0) (tstamp 57804D56)
    (at 111.76 93.98 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /577FE497)
    (fp_text reference P4 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "DIGITAL(_PWM)" (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 19.55) (end 1.75 19.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 19.05) (end -1.27 19.05) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 19.05) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 TX))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 DRDY))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 DCLK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 DOUT0))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 DOUT1))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 DOUT2))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 DOUT3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0) (tstamp 57804D60)
    (at 63.5 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57800D6E)
    (fp_text reference P5 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ANALOG_IN (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 14.45) (end 1.75 14.45) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 13.97) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 13.97) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 A0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 A1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 A2))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 A3))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 A4))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 A5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 5782C59C) (tstamp 57804D6E)
    (at 99.06 152.4 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5781FBE7)
    (fp_text reference P6 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_- (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 24.65) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 24.13) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 AUXAIN-))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 AIN0-))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 AIN1-))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AIN2-))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 AIN3-))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 AIN4-))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 AIN5-))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 AIN6-))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 AIN7-))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x10 (layer F.Cu) (tedit 5782C5A4) (tstamp 57804D7C)
    (at 99.06 147.32 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5781DDD8)
    (fp_text reference P7 (at 0 -5.1 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_+ (at 0 -3.1 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 24.65) (end 1.75 24.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.27 1.27) (end 1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 24.13) (end -1.27 24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 24.13) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 AUXAIN+))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AIN0+))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AIN1+))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AIN2+))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 AIN3+))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 AIN4+))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 AIN5+))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 AIN6+))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 AIN7+))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x10.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module TO_SOT_Packages_SMD:SC-70-5 (layer F.Cu) (tedit 57805000) (tstamp 578050B1)
    (at 88.9 71.12 270)
    (descr "SC70-5 SOT323-5")
    (path /577FE314)
    (attr smd)
    (fp_text reference U4 (at 1.5 -0.4 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value LP5907QMFX-2.5Q1 (at 2.2 0.3 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.1 0.3) (end -0.8 0.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.8 0.3) (end -0.8 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 -0.6) (end -1.1 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 -0.6) (end -1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.1 0.6) (end 1.1 0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.1 0.6) (end 1.1 -0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 3 smd rect (at 0.6604 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (pad 2 smd rect (at 0 1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 4 smd rect (at 0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -0.6604 -1.016 270) (size 0.4064 0.6604) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (model TO_SOT_Packages_SMD.3dshapes/SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5782C5DD) (tstamp 5780E56E)
    (at 109.22 139.7 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /57830D69)
    (fp_text reference P8 (at 0 -5.1 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_AD7779_1 (at 0 -3.1 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 39.85) (end 1.75 39.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 39.37) (end 1.27 39.37) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 39.37) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 AIN0-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 AIN0+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 AIN1-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AIN1+))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 AVDD))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 OUT_VREF))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 AIN2-))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 AIN2+))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 AIN3-))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 AIN3+))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 GPIO0))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 GPIO1))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 GPIO2))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 ALERT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5780FE12) (tstamp 5780FD8A)
    (at 83.82 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (path /5783D841)
    (fp_text reference P12 (at 0 -5.1) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.75 -1.75) (end -1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.75 -1.75) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 -1.75) (end 1.75 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.75 6.85) (end 1.75 6.85) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.27 1.27) (end -1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.27 6.35) (end 1.27 6.35) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 6.35) (end 1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.55 -1.55) (end 1.55 0) (layer F.SilkS) (width 0.15))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 0) (end -1.55 -1.55) (layer F.SilkS) (width 0.15))
    (fp_line (start -1.55 -1.55) (end 1.55 -1.55) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 AVSS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F9D)
    (at 91.44 132.969)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780EAA6)
    (attr smd)
    (fp_text reference C19 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F82)
    (at 100.2792 124.6378 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DE66)
    (attr smd)
    (fp_text reference C18 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F68)
    (at 89.535 129.2352)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FBDF)
    (attr smd)
    (fp_text reference C15 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F50)
    (at 101.7778 122.1232 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780D089)
    (attr smd)
    (fp_text reference C14 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F38)
    (at 82.4484 133.0198)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5781025B)
    (attr smd)
    (fp_text reference C11 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F2A)
    (at 79.5528 133.01726)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57810352)
    (attr smd)
    (fp_text reference C9 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F1E)
    (at 75.438 124.3838 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578108CA)
    (attr smd)
    (fp_text reference C7 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F06)
    (at 73.9394 122.047 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57810A46)
    (attr smd)
    (fp_text reference C3 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EEE)
    (at 94.3356 133.1468)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FF65)
    (attr smd)
    (fp_text reference C21 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804ED6)
    (at 76.76388 134.51586)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578103BF)
    (attr smd)
    (fp_text reference C10 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 69 REF_OUT))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EBC)
    (at 89.8398 109.3216 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780CC33)
    (attr smd)
    (fp_text reference C6 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804E9D)
    (at 88.6968 112.3188 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780CC6E)
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100pF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F74)
    (at 101.7778 125.2982 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DE17)
    (attr smd)
    (fp_text reference C17 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F44)
    (at 103.2764 122.3772 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780DDD1)
    (attr smd)
    (fp_text reference C13 (at 0 -1.9 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F12)
    (at 90.2462 107.823 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780C539)
    (attr smd)
    (fp_text reference C5 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EFA)
    (at 88.9762 110.8202 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57803D35)
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "C 1uF" (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BA9)
    (at 86.36 81.28 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5784635D)
    (attr smd)
    (fp_text reference C23 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BAF)
    (at 91.44 55.88)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578461F6)
    (attr smd)
    (fp_text reference C24 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BB5)
    (at 86.36 55.88 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5784673C)
    (attr smd)
    (fp_text reference C25 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BBB)
    (at 91.44 68.58)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578462B7)
    (attr smd)
    (fp_text reference C26 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57818BC1)
    (at 86.36 68.58 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57846404)
    (attr smd)
    (fp_text reference C27 (at 0 -1.9 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 3.3V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804CEE)
    (at 95.3008 134.6454)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FFD0)
    (attr smd)
    (fp_text reference C22 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EAC)
    (at 72.4408 122.2502 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578109CD)
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 71 OUT_VREF))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EC8)
    (at 73.9394 124.9934 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5781095F)
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804EE2)
    (at 81.5848 134.5184)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /578102EE)
    (attr smd)
    (fp_text reference C12 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F5C)
    (at 90.043 130.7338)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /5780FC4A)
    (attr smd)
    (fp_text reference C16 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 AVDD))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631) (tstamp 57804F8F)
    (at 91.44 81.28)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (path /57846078)
    (attr smd)
    (fp_text reference C20 (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1uF (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.45 -0.75) (end 1.45 -0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.45 -0.75) (end -1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.45 -0.75) (end 1.45 0.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.35 -0.6) (end 0.35 -0.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 0.35 0.6) (end -0.35 0.6) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 AVSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 CLK_SEL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module FreeSmartEEG:SMD0503_4P_Crystal (layer F.Cu) (tedit 57824BEC) (tstamp 57804CFB)
    (at 74.53 104.46 306)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 4 Pads")
    (tags "crystal oscillator quartz SMD0503 4P")
    (path /57804CA7)
    (attr smd)
    (fp_text reference Y1 (at 0 -4 306) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "8.192 MHz" (at 0 4 306) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.5 2.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 2.5) (end -3.5 2.5) (layer F.Fab) (width 0.15))
    (fp_line (start 3.5 -2.5) (end 3.5 2.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.5 -2.5) (end 3.5 -2.5) (layer F.Fab) (width 0.15))
    (fp_line (start -3.6 2.3) (end -4.15 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 2.6) (end 3.6 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 -2.6) (end 3.6 -2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 -2.6) (end -3.6 -2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.6) (end -3.6 2.3) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 2.6) (end 3.6 2.6) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 0.2) (end -4.15 0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -4.75 -3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.1) (end -4.75 -3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.6 -2.6) (end 3.6 -2.6) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.6 0.2) (end 3.6 -0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.6 0.2) (end -3.6 -0.2) (layer F.SilkS) (width 0.15))
    (fp_line (start 4.75 3.1) (end -4.75 3.1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 4.75 -3.1) (end 4.75 3.1) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -2.5 1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 XTAL2))
    (pad 3 smd rect (at 2.5 1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.5 -1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 XTAL1))
    (pad 3 smd rect (at -2.5 -1.6 306) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask))
  )

  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5782639B) (tstamp 5782708B)
    (at 60.96 125.73)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference REF** (at 0 -1.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0 (at 0 1.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1.3 -0.8) (end 1.3 -0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.3 -0.8) (end -1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.3 -0.8) (end 1.3 0.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.5 0.675) (end -0.5 0.675) (layer F.SilkS) (width 0.15))
    (fp_line (start -0.5 -0.675) (end 0.5 -0.675) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 52.7 156.6) (end 52.7 29.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 123.58 156.6) (end 52.7 156.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 123.6 29.6) (end 123.6 156.6) (angle 90) (layer Dwgs.User) (width 0.2))
  (gr_line (start 52.7 29.6) (end 123.58 29.6) (angle 90) (layer Dwgs.User) (width 0.2))

  (segment (start 60.21 130.81) (end 60.21 128.5) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 60.21 128.5) (end 60.44 128.27) (width 0.25) (layer F.Cu) (net 0) (tstamp 57838D5B))
  (segment (start 115.05 130.81) (end 115.05 128.5) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 115.05 128.5) (end 114.82 128.27) (width 0.25) (layer F.Cu) (net 0) (tstamp 57838B00))
  (segment (start 115.05 125.73) (end 114.82 123.19) (width 0.25) (layer F.Cu) (net 0) (status 20))
  (segment (start 60.44 123.19) (end 60.21 125.73) (width 0.25) (layer F.Cu) (net 0) (status 10))
  (segment (start 63.5 71.12) (end 78.74 71.12) (width 0.25) (layer B.Cu) (net 4) (status 400000))
  (segment (start 78.74 71.12) (end 81.28 73.66) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E85))
  (segment (start 81.28 73.66) (end 81.28 76.2) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E86))
  (segment (start 81.28 76.2) (end 83.82 78.74) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E8D))
  (segment (start 83.82 78.74) (end 96.52 78.74) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E91))
  (segment (start 96.52 78.74) (end 99.06 81.28) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E9E))
  (segment (start 99.06 81.28) (end 99.06 93.98) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838EA3))
  (segment (start 99.06 93.98) (end 93.98 99.06) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838EA5) (status 800000))
  (segment (start 78.74 71.12) (end 81.28 73.66) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E7D))
  (segment (start 81.28 81.28) (end 83.82 83.82) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E81) (status 800000))
  (segment (start 81.28 73.66) (end 81.28 81.28) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E7F))
  (segment (start 81.28 60.96) (end 83.82 58.42) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E79) (status 800000))
  (segment (start 81.28 68.58) (end 81.28 60.96) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E76))
  (segment (start 78.74 71.12) (end 81.28 68.58) (width 0.25) (layer B.Cu) (net 4) (tstamp 57838E6F))
  (segment (start 63.5 71.12) (end 71.12 71.12) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 63.5 71.12) (end 83.82 71.12) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 121.92) (end 86.36 127) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 127) (end 71.12 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 5782701C))
  (segment (start 86.36 121.92) (end 86.36 134.62) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 134.62) (end 78.74 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827018))
  (segment (start 88.9 121.92) (end 88.9 134.62) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 134.62) (end 96.52 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827014))
  (segment (start 88.9 121.92) (end 88.9 132.08) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 132.08) (end 99.06 142.24) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827010))
  (segment (start 88.9 121.92) (end 101.6 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 101.6 121.92) (end 109.22 129.54) (width 0.25) (layer B.Cu) (net 4) (tstamp 5782700C) (status 20))
  (segment (start 88.9 121.92) (end 106.68 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 106.68 121.92) (end 109.22 124.46) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827008) (status 20))
  (segment (start 88.9 119.38) (end 88.9 104.14) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 88.9 104.14) (end 93.98 99.06) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827004))
  (segment (start 86.36 121.92) (end 73.66 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 73.66 121.92) (end 66.04 129.54) (width 0.25) (layer B.Cu) (net 4) (tstamp 57827000))
  (segment (start 86.36 121.92) (end 68.58 121.92) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 68.58 121.92) (end 66.04 124.46) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FFC))
  (segment (start 86.36 119.38) (end 88.9 119.38) (width 0.25) (layer B.Cu) (net 4))
  (segment (start 86.36 121.92) (end 86.36 119.38) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF7))
  (segment (start 88.9 121.92) (end 86.36 121.92) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF6))
  (segment (start 88.9 119.38) (end 88.9 121.92) (width 0.25) (layer B.Cu) (net 4) (tstamp 57826FF5))
  (segment (start 63.5 71.12) (end 71.12 71.12) (width 0.25) (layer B.Cu) (net 4) (status 10))
  (segment (start 87.884 83.82) (end 88.15 83.82) (width 0.25) (layer F.Cu) (net 4) (status 30))
  (segment (start 88.15 83.82) (end 90.69 81.28) (width 0.25) (layer F.Cu) (net 4) (tstamp 57825E97) (status 10))
  (segment (start 90.69 81.28) (end 87.11 81.28) (width 0.25) (layer F.Cu) (net 4) (tstamp 57825E98) (status 20))
  (segment (start 87.884 71.12) (end 88.15 71.12) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 88.15 71.12) (end 90.69 68.58) (width 0.25) (layer F.Cu) (net 4) (tstamp 57825E85))
  (segment (start 90.69 68.58) (end 87.11 68.58) (width 0.25) (layer F.Cu) (net 4) (tstamp 57825E86))
  (segment (start 87.884 71.12) (end 83.82 71.12) (width 0.25) (layer F.Cu) (net 4) (status 20))
  (segment (start 87.1093 55.88) (end 90.6907 55.88) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 88.1507 58.42) (end 90.6907 55.88) (width 0.25) (layer F.Cu) (net 4) (tstamp 57825C85))
  (segment (start 87.884 58.42) (end 83.82 58.42) (width 0.25) (layer F.Cu) (net 4) (status 20))
  (segment (start 87.884 58.42) (end 88.1507 58.42) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.88 125.15) (end 89.88 126.86) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.38 125.15) (end 89.38 127.11) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 89.38 127.11) (end 96.52 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 57824096))
  (segment (start 85.88 125.15) (end 85.88 127.11) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 85.88 127.11) (end 78.74 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782407A))
  (segment (start 84.38 125.15) (end 84.38 126.36) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 84.38 126.36) (end 71.12 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782406E))
  (segment (start 83.13 122.4) (end 81.14 122.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 81.14 122.4) (end 66.04 129.54) (width 0.25) (layer F.Cu) (net 4) (tstamp 57824052))
  (segment (start 83.13 121.4) (end 80.64 121.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 88.88 116.15) (end 88.88 113.86) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 92.13 121.4) (end 94.39 121.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 94.39 121.4) (end 109.22 124.46) (width 0.25) (layer F.Cu) (net 4) (tstamp 578215C7) (status 20))
  (segment (start 92.13 122.4) (end 93.89 122.4) (width 0.25) (layer F.Cu) (net 4))
  (segment (start 93.89 122.4) (end 109.22 129.54) (width 0.25) (layer F.Cu) (net 4) (tstamp 578215B2) (status 20))
  (segment (start 89.88 126.86) (end 99.06 142.24) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782409A))
  (segment (start 80.64 121.4) (end 66.04 124.46) (width 0.25) (layer F.Cu) (net 4) (tstamp 5782404E))
  (segment (start 88.88 113.86) (end 93.98 99.06) (width 0.25) (layer F.Cu) (net 4) (tstamp 57823FFE))
  (segment (start 87.884 83.82) (end 83.82 83.82) (width 0.25) (layer F.Cu) (net 4) (status 10))
  (segment (start 63.5 66.04) (end 78.74 66.04) (width 0.25) (layer F.Cu) (net 11) (status 400000))
  (segment (start 78.74 66.04) (end 81.28 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E52))
  (segment (start 81.28 68.58) (end 81.28 83.82) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E56))
  (segment (start 81.28 83.82) (end 83.82 86.36) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E59) (status 800000))
  (segment (start 78.74 66.04) (end 81.28 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E46))
  (segment (start 81.28 68.58) (end 81.28 78.74) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E48))
  (segment (start 81.28 78.74) (end 83.82 81.28) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E4B) (status 800000))
  (segment (start 78.74 66.04) (end 81.28 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E3B))
  (segment (start 81.28 68.58) (end 81.28 71.12) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E3D))
  (segment (start 81.28 71.12) (end 83.82 73.66) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E42) (status 800000))
  (segment (start 78.74 66.04) (end 81.28 63.5) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E2E))
  (segment (start 81.28 58.42) (end 83.82 55.88) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E37) (status 800000))
  (segment (start 81.28 63.5) (end 81.28 58.42) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E31))
  (segment (start 78.74 66.04) (end 83.82 60.96) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E26) (status 800000))
  (segment (start 81.28 68.58) (end 83.82 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E22) (status 800000))
  (segment (start 78.74 66.04) (end 81.28 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57838E1C))
  (segment (start 85.6996 83.1596) (end 83.82 81.28) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825E9D) (status 20))
  (segment (start 85.61 81.28) (end 83.82 81.28) (width 0.25) (layer F.Cu) (net 11) (status 10))
  (segment (start 87.884 84.4804) (end 85.6996 84.4804) (width 0.25) (layer F.Cu) (net 11) (status 10))
  (segment (start 85.6996 84.4804) (end 83.82 86.36) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825EA3) (status 20))
  (segment (start 87.884 83.1596) (end 85.6996 83.1596) (width 0.25) (layer F.Cu) (net 11) (status 10))
  (segment (start 85.61 68.58) (end 83.82 68.58) (width 0.25) (layer F.Cu) (net 11) (status 20))
  (segment (start 87.884 71.7804) (end 85.6996 71.7804) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 85.6996 71.7804) (end 83.82 73.66) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825E74) (status 20))
  (segment (start 87.884 70.4596) (end 85.6996 70.4596) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 85.6996 70.4596) (end 83.82 68.58) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825E70) (status 20))
  (segment (start 85.6107 55.88) (end 83.82 55.88) (width 0.25) (layer F.Cu) (net 11) (status 20))
  (segment (start 87.884 59.0804) (end 85.6996 59.0804) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 85.6996 59.0804) (end 83.82 60.96) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825C75) (status 20))
  (segment (start 87.884 57.7596) (end 85.6996 57.7596) (width 0.25) (layer F.Cu) (net 11))
  (segment (start 85.6996 57.7596) (end 83.82 55.88) (width 0.25) (layer F.Cu) (net 11) (tstamp 57825C6F) (status 20))
  (segment (start 106.68 142.24) (end 99.06 152.4) (width 0.25) (layer B.Cu) (net 21))
  (segment (start 99.06 152.4) (end 99.06 152.4) (width 0.25) (layer B.Cu) (net 21) (tstamp 57826FC1) (status 20))
  (segment (start 91.38 125.15) (end 91.38 126.11) (width 0.25) (layer F.Cu) (net 21))
  (segment (start 91.38 126.11) (end 106.68 142.24) (width 0.25) (layer F.Cu) (net 21) (tstamp 578240A6))
  (segment (start 109.22 139.7) (end 111.76 142.24) (width 0.25) (layer B.Cu) (net 22) (status 10))
  (segment (start 98.298 154.432) (end 96.52 152.4) (width 0.25) (layer B.Cu) (net 22) (tstamp 57826FC9) (status 20))
  (segment (start 110.998 154.432) (end 98.298 154.432) (width 0.25) (layer B.Cu) (net 22) (tstamp 57826FC8))
  (segment (start 111.76 153.67) (end 110.998 154.432) (width 0.25) (layer B.Cu) (net 22) (tstamp 57826FC6))
  (segment (start 111.76 142.24) (end 111.76 153.67) (width 0.25) (layer B.Cu) (net 22) (tstamp 57826FC5))
  (segment (start 92.13 124.4) (end 92.89 124.4) (width 0.25) (layer F.Cu) (net 22))
  (segment (start 92.89 124.4) (end 109.22 139.7) (width 0.25) (layer F.Cu) (net 22) (tstamp 57823DF7) (status 20))
  (segment (start 109.22 134.62) (end 113.03 138.43) (width 0.25) (layer B.Cu) (net 23) (status 10))
  (segment (start 96.012 154.686) (end 93.98 152.4) (width 0.25) (layer B.Cu) (net 23) (tstamp 57826FD1) (status 20))
  (segment (start 112.014 154.686) (end 96.012 154.686) (width 0.25) (layer B.Cu) (net 23) (tstamp 57826FD0))
  (segment (start 113.03 153.67) (end 112.014 154.686) (width 0.25) (layer B.Cu) (net 23) (tstamp 57826FCE))
  (segment (start 113.03 138.43) (end 113.03 153.67) (width 0.25) (layer B.Cu) (net 23) (tstamp 57826FCD))
  (segment (start 92.13 123.4) (end 93.39 123.4) (width 0.25) (layer F.Cu) (net 23))
  (segment (start 93.39 123.4) (end 109.22 134.62) (width 0.25) (layer F.Cu) (net 23) (tstamp 57821592) (status 20))
  (segment (start 109.22 119.38) (end 114.3 124.46) (width 0.25) (layer B.Cu) (net 24) (status 10))
  (segment (start 93.472 154.94) (end 91.44 152.4) (width 0.25) (layer B.Cu) (net 24) (tstamp 57826FD9) (status 20))
  (segment (start 113.03 154.94) (end 93.472 154.94) (width 0.25) (layer B.Cu) (net 24) (tstamp 57826FD8))
  (segment (start 114.3 153.67) (end 113.03 154.94) (width 0.25) (layer B.Cu) (net 24) (tstamp 57826FD6))
  (segment (start 114.3 124.46) (end 114.3 153.67) (width 0.25) (layer B.Cu) (net 24) (tstamp 57826FD5))
  (segment (start 92.13 120.4) (end 94.64 120.4) (width 0.25) (layer F.Cu) (net 24))
  (segment (start 94.64 120.4) (end 109.22 119.38) (width 0.25) (layer F.Cu) (net 24) (tstamp 578215E3) (status 20))
  (segment (start 109.22 114.3) (end 115.57 120.65) (width 0.25) (layer B.Cu) (net 25) (status 10))
  (segment (start 90.932 155.194) (end 88.9 152.4) (width 0.25) (layer B.Cu) (net 25) (tstamp 57826FE1) (status 20))
  (segment (start 114.046 155.194) (end 90.932 155.194) (width 0.25) (layer B.Cu) (net 25) (tstamp 57826FE0))
  (segment (start 115.57 153.67) (end 114.046 155.194) (width 0.25) (layer B.Cu) (net 25) (tstamp 57826FDE))
  (segment (start 115.57 120.65) (end 115.57 153.67) (width 0.25) (layer B.Cu) (net 25) (tstamp 57826FDD))
  (segment (start 94.14 119.4) (end 109.22 114.3) (width 0.25) (layer F.Cu) (net 25) (tstamp 57823DD7) (status 20))
  (segment (start 92.13 119.4) (end 94.14 119.4) (width 0.25) (layer F.Cu) (net 25))
  (segment (start 66.04 139.7) (end 63.5 142.24) (width 0.25) (layer B.Cu) (net 26))
  (segment (start 83.566 149.606) (end 86.36 152.4) (width 0.25) (layer B.Cu) (net 26) (tstamp 5782C209))
  (segment (start 70.866 149.606) (end 83.566 149.606) (width 0.25) (layer B.Cu) (net 26) (tstamp 5782C1FC))
  (segment (start 63.5 142.24) (end 70.866 149.606) (width 0.25) (layer B.Cu) (net 26) (tstamp 5782C1F5))
  (segment (start 83.13 124.4) (end 82.14 124.4) (width 0.25) (layer F.Cu) (net 26))
  (segment (start 82.14 124.4) (end 66.04 139.7) (width 0.25) (layer F.Cu) (net 26) (tstamp 57824066))
  (segment (start 66.04 134.62) (end 62.23 138.43) (width 0.25) (layer B.Cu) (net 27))
  (segment (start 69.85 149.86) (end 77.216 149.86) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0B6))
  (segment (start 62.23 142.24) (end 69.85 149.86) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0B2))
  (segment (start 62.23 138.43) (end 62.23 142.24) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0B0))
  (segment (start 77.216 149.86) (end 81.28 149.86) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0BD))
  (segment (start 81.28 149.86) (end 83.82 152.4) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0D5))
  (segment (start 81.28 149.86) (end 81.28 149.86) (width 0.25) (layer B.Cu) (net 27) (tstamp 5782C0D3))
  (segment (start 83.13 123.4) (end 81.64 123.4) (width 0.25) (layer F.Cu) (net 27))
  (segment (start 81.64 123.4) (end 66.04 134.62) (width 0.25) (layer F.Cu) (net 27) (tstamp 5782405E))
  (segment (start 66.04 119.38) (end 60.96 124.46) (width 0.25) (layer B.Cu) (net 28))
  (segment (start 78.994 150.114) (end 81.28 152.4) (width 0.25) (layer B.Cu) (net 28) (tstamp 5782C09D))
  (segment (start 68.834 150.114) (end 78.994 150.114) (width 0.25) (layer B.Cu) (net 28) (tstamp 5782C095))
  (segment (start 60.96 142.24) (end 68.834 150.114) (width 0.25) (layer B.Cu) (net 28) (tstamp 5782C091))
  (segment (start 60.96 124.46) (end 60.96 142.24) (width 0.25) (layer B.Cu) (net 28) (tstamp 5782C08C))
  (segment (start 83.13 120.4) (end 80.39 120.4) (width 0.25) (layer F.Cu) (net 28))
  (segment (start 80.39 120.4) (end 66.04 119.38) (width 0.25) (layer F.Cu) (net 28) (tstamp 57824046))
  (segment (start 66.04 114.3) (end 59.69 120.65) (width 0.25) (layer B.Cu) (net 29))
  (segment (start 76.708 150.368) (end 78.74 152.4) (width 0.25) (layer B.Cu) (net 29) (tstamp 5782C07E))
  (segment (start 67.818 150.368) (end 76.708 150.368) (width 0.25) (layer B.Cu) (net 29) (tstamp 5782C06B))
  (segment (start 59.69 142.24) (end 67.818 150.368) (width 0.25) (layer B.Cu) (net 29) (tstamp 5782C05C))
  (segment (start 59.69 138.43) (end 59.69 142.24) (width 0.25) (layer B.Cu) (net 29) (tstamp 5782C049))
  (segment (start 59.69 120.65) (end 59.69 138.43) (width 0.25) (layer B.Cu) (net 29) (tstamp 5782C042))
  (segment (start 80.89 119.4) (end 66.04 114.3) (width 0.25) (layer F.Cu) (net 29) (tstamp 5782403E))
  (segment (start 83.13 119.4) (end 80.89 119.4) (width 0.25) (layer F.Cu) (net 29))
  (segment (start 104.14 142.24) (end 99.06 147.32) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 99.06 147.32) (end 99.06 147.32) (width 0.25) (layer F.Cu) (net 30) (tstamp 57826FB9) (status 20))
  (segment (start 90.88 125.15) (end 90.88 126.36) (width 0.25) (layer F.Cu) (net 30))
  (segment (start 90.88 126.36) (end 104.14 142.24) (width 0.25) (layer F.Cu) (net 30) (tstamp 578240A2))
  (segment (start 109.22 137.16) (end 111.76 139.7) (width 0.25) (layer F.Cu) (net 31) (status 10))
  (segment (start 98.298 149.352) (end 96.52 147.32) (width 0.25) (layer F.Cu) (net 31) (tstamp 57826FAD) (status 20))
  (segment (start 105.918 149.352) (end 98.298 149.352) (width 0.25) (layer F.Cu) (net 31) (tstamp 57826FAC))
  (segment (start 111.76 143.51) (end 105.918 149.352) (width 0.25) (layer F.Cu) (net 31) (tstamp 57826FAA))
  (segment (start 111.76 139.7) (end 111.76 143.51) (width 0.25) (layer F.Cu) (net 31) (tstamp 57826FA9))
  (segment (start 92.13 123.9) (end 93.139889 123.89737) (width 0.25) (layer F.Cu) (net 31))
  (segment (start 93.139889 123.90263) (end 109.22 137.16) (width 0.25) (layer F.Cu) (net 31) (tstamp 57821567) (status 20))
  (segment (start 109.22 132.08) (end 113.03 135.89) (width 0.25) (layer F.Cu) (net 32) (status 10))
  (segment (start 96.012 149.606) (end 93.98 147.32) (width 0.25) (layer F.Cu) (net 32) (tstamp 57826FB5) (status 20))
  (segment (start 106.934 149.606) (end 96.012 149.606) (width 0.25) (layer F.Cu) (net 32) (tstamp 57826FB3))
  (segment (start 113.03 143.51) (end 106.934 149.606) (width 0.25) (layer F.Cu) (net 32) (tstamp 57826FB2))
  (segment (start 113.03 135.89) (end 113.03 143.51) (width 0.25) (layer F.Cu) (net 32) (tstamp 57826FB1))
  (segment (start 93.64 122.9) (end 109.22 132.08) (width 0.25) (layer F.Cu) (net 32) (tstamp 578215A9) (status 20))
  (segment (start 92.13 122.9) (end 93.64 122.9) (width 0.25) (layer F.Cu) (net 32))
  (segment (start 109.22 116.84) (end 114.3 121.92) (width 0.25) (layer F.Cu) (net 33) (status 10))
  (segment (start 93.726 149.86) (end 91.44 147.32) (width 0.25) (layer F.Cu) (net 33) (tstamp 57826FE9) (status 20))
  (segment (start 107.95 149.86) (end 93.726 149.86) (width 0.25) (layer F.Cu) (net 33) (tstamp 57826FE8))
  (segment (start 114.3 143.51) (end 107.95 149.86) (width 0.25) (layer F.Cu) (net 33) (tstamp 57826FE6))
  (segment (start 114.3 121.92) (end 114.3 143.51) (width 0.25) (layer F.Cu) (net 33) (tstamp 57826FE5))
  (segment (start 92.13 119.9) (end 94.39 119.9) (width 0.25) (layer F.Cu) (net 33))
  (segment (start 94.39 119.9) (end 109.22 116.84) (width 0.25) (layer F.Cu) (net 33) (tstamp 57823DD3) (status 20))
  (segment (start 109.22 111.76) (end 115.57 118.11) (width 0.25) (layer F.Cu) (net 34) (status 10))
  (segment (start 91.186 150.114) (end 88.9 147.32) (width 0.25) (layer F.Cu) (net 34) (tstamp 57826FF1) (status 20))
  (segment (start 108.966 150.114) (end 91.186 150.114) (width 0.25) (layer F.Cu) (net 34) (tstamp 57826FF0))
  (segment (start 115.57 143.51) (end 108.966 150.114) (width 0.25) (layer F.Cu) (net 34) (tstamp 57826FEE))
  (segment (start 115.57 118.11) (end 115.57 143.51) (width 0.25) (layer F.Cu) (net 34) (tstamp 57826FED))
  (segment (start 92.13 118.9) (end 93.89 118.9) (width 0.25) (layer F.Cu) (net 34))
  (segment (start 93.89 118.9) (end 109.22 111.76) (width 0.25) (layer F.Cu) (net 34) (tstamp 57823DDB) (status 20))
  (segment (start 66.04 137.16) (end 63.5 139.7) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 83.82 144.526) (end 86.36 147.32) (width 0.25) (layer F.Cu) (net 35) (tstamp 57826F8A) (status 20))
  (segment (start 65.786 144.526) (end 83.82 144.526) (width 0.25) (layer F.Cu) (net 35) (tstamp 57826F88))
  (segment (start 63.5 142.24) (end 65.786 144.526) (width 0.25) (layer F.Cu) (net 35) (tstamp 57826F86))
  (segment (start 63.5 139.7) (end 63.5 142.24) (width 0.25) (layer F.Cu) (net 35) (tstamp 57826F85))
  (segment (start 83.13 123.9) (end 81.89 123.9) (width 0.25) (layer F.Cu) (net 35))
  (segment (start 81.89 123.9) (end 66.04 137.16) (width 0.25) (layer F.Cu) (net 35) (tstamp 57824062))
  (segment (start 66.04 132.08) (end 62.23 135.89) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 81.534 144.78) (end 83.82 147.32) (width 0.25) (layer F.Cu) (net 36) (tstamp 57826F93) (status 20))
  (segment (start 64.77 144.78) (end 81.534 144.78) (width 0.25) (layer F.Cu) (net 36) (tstamp 57826F91))
  (segment (start 62.23 142.24) (end 64.77 144.78) (width 0.25) (layer F.Cu) (net 36) (tstamp 57826F8F))
  (segment (start 62.23 135.89) (end 62.23 142.24) (width 0.25) (layer F.Cu) (net 36) (tstamp 57826F8E))
  (segment (start 81.39 122.9) (end 66.04 132.08) (width 0.25) (layer F.Cu) (net 36) (tstamp 5782405A))
  (segment (start 83.13 122.9) (end 81.39 122.9) (width 0.25) (layer F.Cu) (net 36))
  (segment (start 78.994 145.034) (end 81.28 147.32) (width 0.25) (layer F.Cu) (net 37) (tstamp 57826F9C) (status 20))
  (segment (start 63.754 145.034) (end 78.994 145.034) (width 0.25) (layer F.Cu) (net 37) (tstamp 57826F9A))
  (segment (start 60.96 142.24) (end 63.754 145.034) (width 0.25) (layer F.Cu) (net 37) (tstamp 57826F98))
  (segment (start 60.96 121.92) (end 60.96 142.24) (width 0.25) (layer F.Cu) (net 37) (tstamp 57826F97))
  (segment (start 66.04 116.84) (end 60.96 121.92) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 80.64 119.9) (end 66.04 116.84) (width 0.25) (layer F.Cu) (net 37) (tstamp 57824042))
  (segment (start 83.13 119.9) (end 80.64 119.9) (width 0.25) (layer F.Cu) (net 37))
  (segment (start 66.04 111.76) (end 59.69 118.11) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 76.708 145.288) (end 78.74 147.32) (width 0.25) (layer F.Cu) (net 38) (tstamp 57826FA5) (status 20))
  (segment (start 62.738 145.288) (end 76.708 145.288) (width 0.25) (layer F.Cu) (net 38) (tstamp 57826FA3))
  (segment (start 59.69 142.24) (end 62.738 145.288) (width 0.25) (layer F.Cu) (net 38) (tstamp 57826FA1))
  (segment (start 59.69 118.11) (end 59.69 142.24) (width 0.25) (layer F.Cu) (net 38) (tstamp 57826FA0))
  (segment (start 81.14 118.9) (end 66.04 111.76) (width 0.25) (layer F.Cu) (net 38) (tstamp 5782403A))
  (segment (start 83.13 118.9) (end 81.14 118.9) (width 0.25) (layer F.Cu) (net 38))
  (segment (start 88.38 116.15) (end 88.38 113.61) (width 0.25) (layer F.Cu) (net 39))
  (segment (start 66.04 127) (end 62.23 130.81) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 62.23 130.81) (end 61.71 130.81) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838D58))
  (segment (start 116.32 128.27) (end 116.84 128.27) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 99.06 55.88) (end 93.98 55.88) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 116.84 128.27) (end 118.11 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838B82))
  (segment (start 118.11 127) (end 118.11 74.93) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838B84))
  (segment (start 118.11 74.93) (end 118.11 49.53) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838B96))
  (segment (start 118.11 49.53) (end 113.03 44.45) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838B9B))
  (segment (start 113.03 44.45) (end 110.49 44.45) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838BA1))
  (segment (start 110.49 44.45) (end 99.06 55.88) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838BA3))
  (segment (start 109.22 127) (end 113.03 130.81) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 113.03 130.81) (end 113.55 130.81) (width 0.25) (layer F.Cu) (net 40) (tstamp 57838AF8))
  (segment (start 90.38 126.61) (end 101.6 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 5782409E))
  (segment (start 94.14 121.9) (end 109.22 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 578215BB) (status 20))
  (segment (start 80.89 121.9) (end 66.04 127) (width 0.25) (layer F.Cu) (net 40) (tstamp 57824056))
  (segment (start 92.1893 55.88) (end 93.98 55.88) (width 0.25) (layer F.Cu) (net 40) (status 20))
  (segment (start 89.916 57.7596) (end 92.1004 57.7596) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 92.1004 57.7596) (end 93.98 55.88) (width 0.25) (layer F.Cu) (net 40) (tstamp 57825C7B) (status 20))
  (segment (start 90.38 125.15) (end 90.38 126.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 88.38 125.15) (end 88.38 127.61) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 88.38 127.61) (end 91.44 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 5782408E))
  (segment (start 85.38 125.15) (end 85.38 126.86) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 83.13 121.9) (end 80.89 121.9) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 92.13 121.9) (end 94.14 121.9) (width 0.25) (layer F.Cu) (net 40))
  (segment (start 85.38 126.86) (end 76.2 142.24) (width 0.25) (layer F.Cu) (net 40) (tstamp 57824076))
  (segment (start 89.916 84.4804) (end 92.1004 84.4804) (width 0.25) (layer F.Cu) (net 41) (status 10))
  (segment (start 89.916 59.0804) (end 92.1004 59.0804) (width 0.25) (layer F.Cu) (net 42))
  (segment (start 89.916 71.7804) (end 92.1004 71.7804) (width 0.25) (layer F.Cu) (net 43))
  (segment (start 83.13 116.9) (end 82.14 116.9) (width 0.25) (layer F.Cu) (net 44))
  (segment (start 82.14 116.9) (end 66.04 101.6) (width 0.25) (layer F.Cu) (net 44) (tstamp 5782402A))
  (segment (start 81.39 118.4) (end 66.04 109.22) (width 0.25) (layer F.Cu) (net 45) (tstamp 57824036))
  (segment (start 83.13 118.4) (end 81.39 118.4) (width 0.25) (layer F.Cu) (net 45))
  (segment (start 104.14 99.06) (end 109.22 93.98) (width 0.25) (layer F.Cu) (net 46))
  (segment (start 109.22 69.596) (end 111.76 67.056) (width 0.25) (layer F.Cu) (net 46) (tstamp 5782BF05))
  (segment (start 109.22 93.98) (end 109.22 69.596) (width 0.25) (layer F.Cu) (net 46) (tstamp 5782BF01))
  (segment (start 90.88 116.15) (end 90.88 114.86) (width 0.25) (layer F.Cu) (net 46))
  (segment (start 90.88 114.86) (end 104.14 99.06) (width 0.25) (layer F.Cu) (net 46) (tstamp 57823FEA))
  (segment (start 101.6 99.06) (end 107.95 92.71) (width 0.25) (layer F.Cu) (net 47))
  (segment (start 107.95 68.326) (end 111.76 64.516) (width 0.25) (layer F.Cu) (net 47) (tstamp 5782BF10))
  (segment (start 107.95 92.71) (end 107.95 68.326) (width 0.25) (layer F.Cu) (net 47) (tstamp 5782BF0F))
  (segment (start 90.38 116.15) (end 90.38 114.61) (width 0.25) (layer F.Cu) (net 47))
  (segment (start 90.38 114.61) (end 101.6 99.06) (width 0.25) (layer F.Cu) (net 47) (tstamp 57823FEE))
  (segment (start 99.06 99.06) (end 106.68 91.44) (width 0.25) (layer F.Cu) (net 48))
  (segment (start 106.68 67.056) (end 111.76 61.976) (width 0.25) (layer F.Cu) (net 48) (tstamp 5782BF18))
  (segment (start 106.68 91.44) (end 106.68 67.056) (width 0.25) (layer F.Cu) (net 48) (tstamp 5782BF16))
  (segment (start 89.88 116.15) (end 89.88 114.36) (width 0.25) (layer F.Cu) (net 48))
  (segment (start 89.88 114.36) (end 99.06 99.06) (width 0.25) (layer F.Cu) (net 48) (tstamp 57823FF2))
  (segment (start 96.52 99.06) (end 105.41 90.17) (width 0.25) (layer F.Cu) (net 49))
  (segment (start 105.41 65.786) (end 111.76 59.436) (width 0.25) (layer F.Cu) (net 49) (tstamp 5782BF1E))
  (segment (start 105.41 90.17) (end 105.41 65.786) (width 0.25) (layer F.Cu) (net 49) (tstamp 5782BF1D))
  (segment (start 89.38 116.15) (end 89.38 114.11) (width 0.25) (layer F.Cu) (net 49))
  (segment (start 89.38 114.11) (end 96.52 99.06) (width 0.25) (layer F.Cu) (net 49) (tstamp 57823FF9))
  (segment (start 84.88 114.61) (end 73.66 99.06) (width 0.25) (layer F.Cu) (net 51) (tstamp 5782401E))
  (segment (start 84.88 116.15) (end 84.88 114.61) (width 0.25) (layer F.Cu) (net 51))
  (segment (start 85.38 114.36) (end 76.2 99.06) (width 0.25) (layer F.Cu) (net 52) (tstamp 5782401A))
  (segment (start 85.38 116.15) (end 85.38 114.36) (width 0.25) (layer F.Cu) (net 52))
  (segment (start 85.88 116.15) (end 85.88 114.11) (width 0.25) (layer F.Cu) (net 53))
  (segment (start 85.88 114.11) (end 78.74 99.06) (width 0.25) (layer F.Cu) (net 53) (tstamp 57824016))
  (segment (start 86.38 116.15) (end 86.38 113.86) (width 0.25) (layer F.Cu) (net 54))
  (segment (start 86.38 113.86) (end 81.28 99.06) (width 0.25) (layer F.Cu) (net 54) (tstamp 57824012))
  (segment (start 86.88 116.15) (end 86.88 113.61) (width 0.25) (layer F.Cu) (net 55))
  (segment (start 86.88 113.61) (end 83.82 99.06) (width 0.25) (layer F.Cu) (net 55) (tstamp 5782400E))
  (segment (start 87.38 116.15) (end 87.38 113.36) (width 0.25) (layer F.Cu) (net 56))
  (segment (start 87.38 113.36) (end 86.36 99.06) (width 0.25) (layer F.Cu) (net 56) (tstamp 5782400A))
  (segment (start 88.9 99.06) (end 91.44 96.52) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 96.52 83.82) (end 93.98 81.28) (width 0.25) (layer F.Cu) (net 57) (tstamp 5782BEC6))
  (segment (start 96.52 93.98) (end 96.52 83.82) (width 0.25) (layer F.Cu) (net 57) (tstamp 5782BEBC))
  (segment (start 93.98 96.52) (end 96.52 93.98) (width 0.25) (layer F.Cu) (net 57) (tstamp 5782BEB8))
  (segment (start 91.44 96.52) (end 93.98 96.52) (width 0.25) (layer F.Cu) (net 57) (tstamp 5782BEB3))
  (segment (start 92.19 81.28) (end 93.98 81.28) (width 0.25) (layer F.Cu) (net 57) (status 20))
  (segment (start 89.916 83.1596) (end 92.1004 83.1596) (width 0.25) (layer F.Cu) (net 57) (status 10))
  (segment (start 92.1004 83.1596) (end 93.98 81.28) (width 0.25) (layer F.Cu) (net 57) (tstamp 57825E8D) (status 20))
  (segment (start 91.38 115.11) (end 106.68 99.06) (width 0.25) (layer F.Cu) (net 57) (tstamp 57823FE6))
  (segment (start 87.88 113.36) (end 88.9 99.06) (width 0.25) (layer F.Cu) (net 57) (tstamp 57824006))
  (segment (start 86.38 127.36) (end 81.28 142.24) (width 0.25) (layer F.Cu) (net 57) (tstamp 5782407E))
  (segment (start 87.38 125.15) (end 87.38 127.86) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 86.88 125.15) (end 86.88 127.61) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 86.88 127.61) (end 83.82 142.24) (width 0.25) (layer F.Cu) (net 57) (tstamp 57824082))
  (segment (start 86.38 125.15) (end 86.38 127.36) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 87.88 116.15) (end 87.88 113.36) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 91.38 116.15) (end 91.38 115.11) (width 0.25) (layer F.Cu) (net 57))
  (segment (start 87.38 127.86) (end 86.36 142.24) (width 0.25) (layer F.Cu) (net 57) (tstamp 57824086))
  (segment (start 88.38 113.61) (end 91.44 99.06) (width 0.25) (layer F.Cu) (net 58) (tstamp 57824002))
  (segment (start 84.88 126.61) (end 73.66 142.24) (width 0.25) (layer F.Cu) (net 59) (tstamp 57824072))
  (segment (start 88.88 127.36) (end 93.98 142.24) (width 0.25) (layer F.Cu) (net 60) (tstamp 57824092))
  (segment (start 93.64 118.4) (end 109.22 109.22) (width 0.25) (layer F.Cu) (net 61) (tstamp 57823DDF) (status 20))
  (segment (start 92.13 118.4) (end 93.64 118.4) (width 0.25) (layer F.Cu) (net 61))
  (segment (start 93.39 117.9) (end 109.22 106.68) (width 0.25) (layer F.Cu) (net 62) (tstamp 57823DE3) (status 20))
  (segment (start 92.13 117.9) (end 93.39 117.9) (width 0.25) (layer F.Cu) (net 62))
  (segment (start 92.13 117.4) (end 93.14 117.4) (width 0.25) (layer F.Cu) (net 63))
  (segment (start 93.14 117.4) (end 109.22 104.14) (width 0.25) (layer F.Cu) (net 63) (tstamp 57823DE7) (status 20))
  (segment (start 92.89 116.9) (end 109.22 101.6) (width 0.25) (layer F.Cu) (net 64) (tstamp 57823DEB) (status 20))
  (segment (start 92.13 116.9) (end 92.89 116.9) (width 0.25) (layer F.Cu) (net 64))
  (segment (start 84.38 116.15) (end 84.38 114.86) (width 0.25) (layer F.Cu) (net 65))
  (segment (start 84.38 114.86) (end 71.12 99.06) (width 0.25) (layer F.Cu) (net 65) (tstamp 57824022))
  (segment (start 83.88 115.11) (end 68.58 99.06) (width 0.25) (layer F.Cu) (net 66) (tstamp 57824026))
  (segment (start 83.88 116.15) (end 83.88 115.11) (width 0.25) (layer F.Cu) (net 66))
  (segment (start 83.13 117.4) (end 81.89 117.4) (width 0.25) (layer F.Cu) (net 67))
  (segment (start 81.89 117.4) (end 66.04 104.14) (width 0.25) (layer F.Cu) (net 67) (tstamp 5782402E))
  (segment (start 81.64 117.9) (end 66.04 106.68) (width 0.25) (layer F.Cu) (net 68) (tstamp 57824032))
  (segment (start 83.13 117.9) (end 81.64 117.9) (width 0.25) (layer F.Cu) (net 68))
  (segment (start 83.88 126.11) (end 68.58 142.24) (width 0.25) (layer F.Cu) (net 69) (tstamp 5782406A))
  (segment (start 83.88 125.15) (end 83.88 126.11) (width 0.25) (layer F.Cu) (net 69))
  (segment (start 87.88 127.86) (end 88.9 142.24) (width 0.25) (layer F.Cu) (net 70) (tstamp 5782408A))
  (segment (start 87.88 125.15) (end 87.88 127.86) (width 0.25) (layer F.Cu) (net 70))
  (segment (start 110.49 45.72) (end 96.52 59.69) (width 0.25) (layer F.Cu) (net 71))
  (segment (start 116.84 123.19) (end 116.84 109.22) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838B25))
  (segment (start 116.84 109.22) (end 116.84 77.47) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838B42))
  (segment (start 116.84 77.47) (end 116.84 49.53) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838B4F))
  (segment (start 116.84 49.53) (end 113.03 45.72) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838B53))
  (segment (start 113.03 45.72) (end 110.49 45.72) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838B58))
  (segment (start 116.32 123.19) (end 116.84 123.19) (width 0.25) (layer F.Cu) (net 71))
  (segment (start 96.52 66.04) (end 93.98 68.58) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838CAD))
  (segment (start 96.52 59.69) (end 96.52 66.04) (width 0.25) (layer F.Cu) (net 71) (tstamp 57838CA5))
  (segment (start 113.55 125.73) (end 113.03 125.73) (width 0.25) (layer F.Cu) (net 71) (status 10))
  (segment (start 113.03 125.73) (end 109.22 121.92) (width 0.25) (layer F.Cu) (net 71) (tstamp 57826548) (status 20))
  (segment (start 61.71 125.73) (end 62.23 125.73) (width 0.25) (layer F.Cu) (net 71) (status 10))
  (segment (start 62.23 125.73) (end 66.04 121.92) (width 0.25) (layer F.Cu) (net 71) (tstamp 57826496))
  (segment (start 109.22 121.92) (end 109.74 121.92) (width 0.25) (layer F.Cu) (net 71) (status 30))
  (segment (start 92.19 68.58) (end 93.98 68.58) (width 0.25) (layer F.Cu) (net 71) (status 20))
  (segment (start 89.916 70.4596) (end 92.1004 70.4596) (width 0.25) (layer F.Cu) (net 71))
  (segment (start 92.1004 70.4596) (end 93.98 68.58) (width 0.25) (layer F.Cu) (net 71) (tstamp 57825E78) (status 20))
  (segment (start 80.39 120.9) (end 66.04 121.92) (width 0.25) (layer F.Cu) (net 71) (tstamp 5782404A))
  (segment (start 94.64 120.9) (end 109.22 121.92) (width 0.25) (layer F.Cu) (net 71) (tstamp 578215D7) (status 20))
  (segment (start 83.13 120.9) (end 80.39 120.9) (width 0.25) (layer F.Cu) (net 71))
  (segment (start 92.13 120.9) (end 94.64 120.9) (width 0.25) (layer F.Cu) (net 71))
  (segment (start 92.1004 84.4804) (end 93.98 86.36) (width 0.25) (layer F.Cu) (net 72) (tstamp 57825E91) (status 20))
  (segment (start 92.1004 59.0804) (end 93.98 60.96) (width 0.25) (layer F.Cu) (net 74) (tstamp 57825C7F) (status 20))
  (segment (start 92.1004 71.7804) (end 93.98 73.66) (width 0.25) (layer F.Cu) (net 76) (tstamp 57825E7C) (status 20))
  (segment (start 84.88 125.15) (end 84.88 126.61) (width 0.25) (layer F.Cu) (net 78))
  (segment (start 88.88 125.15) (end 88.88 127.36) (width 0.25) (layer F.Cu) (net 79))

)
