- Main Page
- Modules
- Data Structures
- Files

- Search for |

- Alphabetical List
- Data Structures
- Class Hierarchy
- Data Fields

# xed_state_s Struct Reference
[XED initialization]

Encapsulates machine modes for decoder/encoder requests. More...

`#include <xed-state.h>`

## Data Fields

xed_machine_mode_enum_t | mmode
| real architected machine modes
xed_address_width_enum_t | stack_addr_width
| for 16b/32b modes

## Detailed Description

Encapsulates machine modes for decoder/encoder requests.

It specifies the machine operating mode as a xed_machine_mode_enum_t for decoding and encoding. The machine mode corresponds to the default data operand width for that mode. For all modes other than the 64b long mode (XED_MACHINE_MODE_LONG_64), a default addressing width, and a stack addressing width must be supplied of type xed_address_width_enum_t .

Definition at line 52 of file xed-state.h.

## Field Documentation

xed_machine_mode_enum_t mmode

| real architected machine modes Definition at line 54 of file xed-state.h.

xed_address_width_enum_t stack_addr_width

| for 16b/32b modes Definition at line 56 of file xed-state.h.

The documentation for this struct was generated from the following file:

- xed-state.h