McPAT (version 1.0 of Aug, 2013) is computing the target processor...
 

McPAT (version 1.0 of Aug, 2013) results  (current print level is 5)
*****************************************************************************************
  Technology 32 nm
  Using Long Channel Devices When Appropriate
  Interconnect metal projection= aggressive interconnect technology projection
  Core clock Rate(MHz) 2000

*****************************************************************************************
Processor: 
  Area = 4.35718 mm^2
  Peak Power = 0.642285 W
  Total Leakage = 0.336603 W
  Peak Dynamic = 0.305682 W
  Subthreshold Leakage = 0.19356 W
  Subthreshold Leakage with power gating = 0.0823132 W
  Gate Leakage = 0.143043 W
  Runtime Dynamic = 0.00960892 W

  Total Cores: 1 cores 
  Device Type= ITRS high performance device type
    Area = 4.28113 mm^2
    Peak Dynamic = 0.305682 W
    Subthreshold Leakage = 0.191062 W
    Subthreshold Leakage with power gating = 0.0813032 W
    Gate Leakage = 0.141077 W
    Runtime Dynamic = 0.00960892 W

  Total NoCs (Network/Bus): 
  Device Type= ITRS high performance device type
    Area = 0.076047 mm^2
    Peak Dynamic = 0 W
    Subthreshold Leakage = 0.00249838 W
    Subthreshold Leakage with power gating = 0.00101185 W
    Gate Leakage = 0.00196629 W
    Runtime Dynamic = 0 W

*****************************************************************************************
Core:
      Area = 4.28113 mm^2
      Peak Dynamic = 0.305682 W
      Subthreshold Leakage = 0.191062 W
      Subthreshold Leakage with power gating = 0.0813032 W
      Gate Leakage = 0.141077 W
      Runtime Dynamic = 0.00960892 W

      Instruction Fetch Unit:
        Area = 0.847537 mm^2
        Peak Dynamic = 0.19487 W
        Subthreshold Leakage = 0.057375 W
        Subthreshold Leakage with power gating = 0.0252469 W
        Gate Leakage = 0.035415 W
        Runtime Dynamic = 0.00210085 W

          Instruction Cache:
            Area = 0.108965 mm^2
            Peak Dynamic = 0.00362902 W
            Subthreshold Leakage = 0.00321582 W
            Subthreshold Leakage with power gating = 0.00182079 W
            Gate Leakage = 0.00241204 W
            Runtime Dynamic = 5.4769e-05 W

          Branch Target Buffer:
            Area = 0.40049 mm^2
            Peak Dynamic = 0.0639598 W
            Subthreshold Leakage = 0.00884916 W
            Subthreshold Leakage with power gating = 0.00481186 W
            Gate Leakage = 0.00459494 W
            Runtime Dynamic = 0.000199441 W

          Branch Predictor:
            Area = 0.0802363 mm^2
            Peak Dynamic = 0.0247518 W
            Subthreshold Leakage = 0.00187037 W
            Subthreshold Leakage with power gating = 0.00101875 W
            Gate Leakage = 0.000851618 W
            Runtime Dynamic = 8.0956e-05 W

              Global Predictor:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.000706728 W
                Subthreshold Leakage with power gating = 0.000385143 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 2.74283e-05 W

              Local Predictor:
              L1_Local Predictor:
                Area = 0.0132151 mm^2
                Peak Dynamic = 0.00485939 W
                Subthreshold Leakage = 0.000367899 W
                Subthreshold Leakage with power gating = 0.000199139 W
                Gate Leakage = 0.000173252 W
                Runtime Dynamic = 1.73539e-05 W

              L2_Local Predictor:
                Area = 0.00654633 mm^2
                Peak Dynamic = 0.00242012 W
                Subthreshold Leakage = 0.000161788 W
                Subthreshold Leakage with power gating = 9.13414e-05 W
                Gate Leakage = 8.86473e-05 W
                Runtime Dynamic = 8.64228e-06 W

              Chooser:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.000706728 W
                Subthreshold Leakage with power gating = 0.000385143 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 2.74283e-05 W

              RAS:
                Area = 0.00544471 mm^2
                Peak Dynamic = 0.00392128 W
                Subthreshold Leakage = 8.90113e-05 W
                Subthreshold Leakage with power gating = 4.93257e-05 W
                Gate Leakage = 5.19378e-05 W
                Runtime Dynamic = 8.74553e-06 W

          Instruction Buffer:
            Area = 0.00081721 mm^2
            Peak Dynamic = 0.00270259 W
            Subthreshold Leakage = 2.1965e-05 W
            Subthreshold Leakage with power gating = 1.13037e-05 W
            Gate Leakage = 1.81693e-05 W
            Runtime Dynamic = 4.7255e-05 W

          Instruction Decoder:
            Area = 0.234886 mm^2
            Peak Dynamic = 0.0982797 W
            Subthreshold Leakage = 0.0415955 W
            Subthreshold Leakage with power gating = 0.0168462 W
            Gate Leakage = 0.0240558 W
            Runtime Dynamic = 0.00171843 W

      Load Store Unit:
        Area = 0.247541 mm^2
        Peak Dynamic = 0.0582755 W
        Subthreshold Leakage = 0.0074199 W
        Subthreshold Leakage with power gating = 0.00388533 W
        Gate Leakage = 0.00746811 W
        Runtime Dynamic = 0.00281005 W

          Data Cache:
            Area = 0.153165 mm^2
            Peak Dynamic = 0.0561965 W
            Subthreshold Leakage = 0.00424059 W
            Subthreshold Leakage with power gating = 0.00237379 W
            Gate Leakage = 0.00304732 W
            Runtime Dynamic = 0.000508816 W

          Load/Store Queue:
            Area = 0.0517429 mm^2
            Peak Dynamic = 0.00115063 W
            Subthreshold Leakage = 0.00135708 W
            Subthreshold Leakage with power gating = 0.000773538 W
            Gate Leakage = 0.000938396 W
            Runtime Dynamic = 0.00230124 W

      Memory Management Unit:
        Area = 0.10002 mm^2
        Peak Dynamic = 0.0461389 W
        Subthreshold Leakage = 0.00428974 W
        Subthreshold Leakage with power gating = 0.00214449 W
        Gate Leakage = 0.00513284 W
        Runtime Dynamic = 0.00107652 W

          Itlb:
            Area = 0.0320988 mm^2
            Peak Dynamic = 0.000704059 W
            Subthreshold Leakage = 0.000947026 W
            Subthreshold Leakage with power gating = 0.000539805 W
            Gate Leakage = 0.000646352 W
            Runtime Dynamic = 0.000294014 W

          Dtlb:
            Area = 0.0457784 mm^2
            Peak Dynamic = 0.000731685 W
            Subthreshold Leakage = 0.00152049 W
            Subthreshold Leakage with power gating = 0.000866678 W
            Gate Leakage = 0.0010041 W
            Runtime Dynamic = 0.000782509 W

      Execution Unit:
        Area = 2.63663 mm^2
        Peak Dynamic = 0.00548804 W
        Subthreshold Leakage = 0.0998683 W
        Subthreshold Leakage with power gating = 0.0404605 W
        Gate Leakage = 0.0779155 W
        Runtime Dynamic = 0.00342326 W

          Register Files:
            Area = 0.0267181 mm^2
            Peak Dynamic = 0.000278458 W
            Subthreshold Leakage = 0.000176443 W
            Subthreshold Leakage with power gating = 8.53072e-05 W
            Gate Leakage = 0.000112132 W
            Runtime Dynamic = 0.000227639 W

              Integer RF:
                Area = 0.0119557 mm^2
                Peak Dynamic = 0.000278458 W
                Subthreshold Leakage = 7.14531e-05 W
                Subthreshold Leakage with power gating = 3.31566e-05 W
                Gate Leakage = 4.79651e-05 W
                Runtime Dynamic = 0.000189859 W

              Floating Point RF:
                Area = 0.0147624 mm^2
                Peak Dynamic = 0 W
                Subthreshold Leakage = 0.00010499 W
                Subthreshold Leakage with power gating = 5.21506e-05 W
                Gate Leakage = 6.41672e-05 W
                Runtime Dynamic = 3.77803e-05 W

          Instruction Scheduler:
            Area = 0 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0 W
            Subthreshold Leakage with power gating = -nan W
            Gate Leakage = 0 W
            Runtime Dynamic = 0 W

          Integer ALUs (Count: 1 ):
            Area = 0.0549349 mm^2
            Peak Dynamic = 0.00235021 W
            Subthreshold Leakage = 0.00629522 W
            Subthreshold Leakage with power gating = 0.00254956 W
            Gate Leakage = 0.00478051 W
            Runtime Dynamic = 0.00249816 W

          Floating Point Units (FPUs) (Count: 2 ):
            Area = 2.35571 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0674876 W
            Subthreshold Leakage with power gating = 0.0273325 W
            Gate Leakage = 0.0512492 W
            Runtime Dynamic = 0 W

          Complex ALUs (Mul/Div) (Count: 1 ):
            Area = 0.164805 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0188857 W
            Subthreshold Leakage with power gating = 0.00764869 W
            Gate Leakage = 0.0143415 W
            Runtime Dynamic = 0 W

          Results Broadcast Bus:
            Area Overhead = 0.012321 mm^2
            Peak Dynamic = 0.00131232 W
            Subthreshold Leakage = 0.00520114 W
            Subthreshold Leakage with power gating = 0.00210646 W
            Gate Leakage = 0.00394968 W
            Runtime Dynamic = 0.000697466 W

    L2
    Area = 0.158712 mm^2
    Peak Dynamic = 0.000910008 W
    Subthreshold Leakage = 0.00545254 W
    Subthreshold Leakage with power gating = 0.00282027 W
    Gate Leakage = 0.00249689 W
    Runtime Dynamic = 0.000198235 W

*****************************************************************************************
BUSES
      Area = 0.076047 mm^2
      Peak Dynamic = 0 W
      Subthreshold Leakage = 0.00249838 W
      Subthreshold Leakage with power gating = 0.00101185 W
      Gate Leakage = 0.00196629 W
      Runtime Dynamic = 0 W

      Bus: 
        Area = 0.076047 mm^2
        Peak Dynamic = 0 W
        Subthreshold Leakage = 0.00249838 W
        Subthreshold Leakage with power gating = 0.00101185 W
        Gate Leakage = 0.00196629 W
        Runtime Dynamic = 0 W

*****************************************************************************************
