- Main Page
- Modules
- Classes

- Search for |

# CONTROLLER_START_ADDRESS_GENERIC
[CONTROLLER]

## Classes

class | INSTLIB::CONTROL_START_ADDRESS_GENERIC

## Functions

INT32 | INSTLIB::CONTROL_START_ADDRESS_GENERIC::Activate (CONTROL_HANDLER ch, VOID *val, BOOL passContext)

## Detailed Description

Generic controller for detecting the start of an interval using an address or symbol and a count, etc. This takes a generic event, knob and knob usage string.

## Function Documentation

INT32 INSTLIB::CONTROL_START_ADDRESS_GENERIC::Activate | ( | CONTROL_HANDLER | ch,
|  | VOID * | val,
|  | BOOL | passContext
| ) | `[inline, inherited]`

| Activate the controller if the -start_address knob is provided

Returns:
  1 if controller can start an interval, otherwise 0