McPAT (version 1.0 of Aug, 2013) is computing the target processor...
 

McPAT (version 1.0 of Aug, 2013) results  (current print level is 5)
*****************************************************************************************
  Technology 32 nm
  Using Long Channel Devices When Appropriate
  Interconnect metal projection= aggressive interconnect technology projection
  Core clock Rate(MHz) 2000

*****************************************************************************************
Processor: 
  Area = 10.5565 mm^2
  Peak Power = 5.32476 W
  Total Leakage = 0.928496 W
  Peak Dynamic = 4.39626 W
  Subthreshold Leakage = 0.619199 W
  Subthreshold Leakage with power gating = 0.272102 W
  Gate Leakage = 0.309297 W
  Runtime Dynamic = 1.05859 W

  Total Cores: 1 cores 
  Device Type= ITRS high performance device type
    Area = 10.4378 mm^2
    Peak Dynamic = 4.39626 W
    Subthreshold Leakage = 0.615298 W
    Subthreshold Leakage with power gating = 0.270586 W
    Gate Leakage = 0.306227 W
    Runtime Dynamic = 1.05859 W

  Total NoCs (Network/Bus): 
  Device Type= ITRS high performance device type
    Area = 0.118743 mm^2
    Peak Dynamic = 0 W
    Subthreshold Leakage = 0.00390107 W
    Subthreshold Leakage with power gating = 0.00157993 W
    Gate Leakage = 0.00307023 W
    Runtime Dynamic = 0 W

*****************************************************************************************
Core:
      Area = 10.4378 mm^2
      Peak Dynamic = 4.39626 W
      Subthreshold Leakage = 0.615298 W
      Subthreshold Leakage with power gating = 0.270586 W
      Gate Leakage = 0.306227 W
      Runtime Dynamic = 1.05859 W

      Instruction Fetch Unit:
        Area = 1.5013 mm^2
        Peak Dynamic = 1.37739 W
        Subthreshold Leakage = 0.104952 W
        Subthreshold Leakage with power gating = 0.0493871 W
        Gate Leakage = 0.0460309 W
        Runtime Dynamic = 0.10493 W

          Instruction Cache:
            Area = 0.778924 mm^2
            Peak Dynamic = 1.17008 W
            Subthreshold Leakage = 0.0298653 W
            Subthreshold Leakage with power gating = 0.016857 W
            Gate Leakage = 0.0155753 W
            Runtime Dynamic = 0.0196804 W

          Branch Target Buffer:
            Area = 0.40049 mm^2
            Peak Dynamic = 0.0639598 W
            Subthreshold Leakage = 0.0125781 W
            Subthreshold Leakage with power gating = 0.00683951 W
            Gate Leakage = 0.00459494 W
            Runtime Dynamic = 0.00739521 W

          Branch Predictor:
            Area = 0.0802363 mm^2
            Peak Dynamic = 0.0247518 W
            Subthreshold Leakage = 0.00265851 W
            Subthreshold Leakage with power gating = 0.00144804 W
            Gate Leakage = 0.000851618 W
            Runtime Dynamic = 0.00295417 W

              Global Predictor:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.00100453 W
                Subthreshold Leakage with power gating = 0.000547437 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 0.000984164 W

              Local Predictor:
              L1_Local Predictor:
                Area = 0.0132151 mm^2
                Peak Dynamic = 0.00485939 W
                Subthreshold Leakage = 0.000522926 W
                Subthreshold Leakage with power gating = 0.000283053 W
                Gate Leakage = 0.000173252 W
                Runtime Dynamic = 0.000614852 W

              L2_Local Predictor:
                Area = 0.00654633 mm^2
                Peak Dynamic = 0.00242012 W
                Subthreshold Leakage = 0.000229963 W
                Subthreshold Leakage with power gating = 0.000129831 W
                Gate Leakage = 8.86473e-05 W
                Runtime Dynamic = 0.000306203 W

              Chooser:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.00100453 W
                Subthreshold Leakage with power gating = 0.000547437 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 0.000984164 W

              RAS:
                Area = 0.00544471 mm^2
                Peak Dynamic = 0.00392128 W
                Subthreshold Leakage = 0.000126519 W
                Subthreshold Leakage with power gating = 7.01108e-05 W
                Gate Leakage = 5.19378e-05 W
                Runtime Dynamic = 0.000370993 W

          Instruction Buffer:
            Area = 0.00081721 mm^2
            Peak Dynamic = 0.00270259 W
            Subthreshold Leakage = 3.12207e-05 W
            Subthreshold Leakage with power gating = 1.6067e-05 W
            Gate Leakage = 1.81693e-05 W
            Runtime Dynamic = 0.00200454 W

          Instruction Decoder:
            Area = 0.234886 mm^2
            Peak Dynamic = 0.0982797 W
            Subthreshold Leakage = 0.0591232 W
            Subthreshold Leakage with power gating = 0.0239449 W
            Gate Leakage = 0.0240558 W
            Runtime Dynamic = 0.0728952 W

      Renaming Unit:
        Area = 0.102664 mm^2
        Peak Dynamic = 1.1159 W
        Subthreshold Leakage = 0.00764216 W
        Subthreshold Leakage with power gating = 0.00424022 W
        Gate Leakage = 0.00716061 W
        Runtime Dynamic = 0.0157495 W

          Int Front End RAT:
            Area = 0.00927052 mm^2
            Peak Dynamic = 0.0199286 W
            Subthreshold Leakage = 0.000295591 W
            Subthreshold Leakage with power gating = 0.000168487 W
            Gate Leakage = 0.000173494 W
            Runtime Dynamic = 0.0133047 W

          FP Front End RAT:
            Area = 0.0852001 mm^2
            Peak Dynamic = 1.07057 W
            Subthreshold Leakage = 0.00660739 W
            Subthreshold Leakage with power gating = 0.00376621 W
            Gate Leakage = 0.00602705 W
            Runtime Dynamic = 0 W

          Free List:
            Area = 0.00224812 mm^2
            Peak Dynamic = 0.00164806 W
            Subthreshold Leakage = 4.37176e-05 W
            Subthreshold Leakage with power gating = 2.38595e-05 W
            Gate Leakage = 2.5014e-05 W
            Runtime Dynamic = 0.00244478 W

      Load Store Unit:
        Area = 1.6172 mm^2
        Peak Dynamic = 1.05108 W
        Subthreshold Leakage = 0.0448153 W
        Subthreshold Leakage with power gating = 0.0248749 W
        Gate Leakage = 0.022966 W
        Runtime Dynamic = 0.186317 W

          Data Cache:
            Area = 1.24059 mm^2
            Peak Dynamic = 0.978874 W
            Subthreshold Leakage = 0.0408129 W
            Subthreshold Leakage with power gating = 0.0227083 W
            Gate Leakage = 0.02038 W
            Runtime Dynamic = 0.0856742 W

          LoadQ:
            Area = 0.043215 mm^2
            Peak Dynamic = 0.0280294 W
            Subthreshold Leakage = 0.00137797 W
            Subthreshold Leakage with power gating = 0.000785444 W
            Gate Leakage = 0.000712518 W
            Runtime Dynamic = 0.0280294 W

          StoreQ:
            Area = 0.0517429 mm^2
            Peak Dynamic = 0.0363065 W
            Subthreshold Leakage = 0.00192894 W
            Subthreshold Leakage with power gating = 0.0010995 W
            Gate Leakage = 0.000938396 W
            Runtime Dynamic = 0.072613 W

      Memory Management Unit:
        Area = 0.0838228 mm^2
        Peak Dynamic = 0.0687643 W
        Subthreshold Leakage = 0.00420275 W
        Subthreshold Leakage with power gating = 0.00228082 W
        Gate Leakage = 0.0025855 W
        Runtime Dynamic = 0.0276471 W

          Itlb:
            Area = 0.0320988 mm^2
            Peak Dynamic = 0.0298661 W
            Subthreshold Leakage = 0.00134609 W
            Subthreshold Leakage with power gating = 0.000767271 W
            Gate Leakage = 0.000646352 W
            Runtime Dynamic = 0.00434089 W

          Dtlb:
            Area = 0.0457784 mm^2
            Peak Dynamic = 0.0230872 W
            Subthreshold Leakage = 0.0021612 W
            Subthreshold Leakage with power gating = 0.00123188 W
            Gate Leakage = 0.0010041 W
            Runtime Dynamic = 0.0233062 W

      Execution Unit:
        Area = 2.83224 mm^2
        Peak Dynamic = 0.766884 W
        Subthreshold Leakage = 0.143732 W
        Subthreshold Leakage with power gating = 0.0588186 W
        Gate Leakage = 0.0772386 W
        Runtime Dynamic = 0.721339 W

          Register Files:
            Area = 0.0267181 mm^2
            Peak Dynamic = 0.0118122 W
            Subthreshold Leakage = 0.000250794 W
            Subthreshold Leakage with power gating = 0.000121254 W
            Gate Leakage = 0.000112132 W
            Runtime Dynamic = 0.00965638 W

              Integer RF:
                Area = 0.0119557 mm^2
                Peak Dynamic = 0.0118122 W
                Subthreshold Leakage = 0.000101562 W
                Subthreshold Leakage with power gating = 4.71283e-05 W
                Gate Leakage = 4.79651e-05 W
                Runtime Dynamic = 0.00805375 W

              Floating Point RF:
                Area = 0.0147624 mm^2
                Peak Dynamic = 0 W
                Subthreshold Leakage = 0.000149232 W
                Subthreshold Leakage with power gating = 7.41261e-05 W
                Gate Leakage = 6.41672e-05 W
                Runtime Dynamic = 0.00160263 W

          Instruction Scheduler:
            Area = 0.211479 mm^2
            Peak Dynamic = 0.481006 W
            Subthreshold Leakage = 0.00371368 W
            Subthreshold Leakage with power gating = 0.00209154 W
            Gate Leakage = 0.001891 W
            Runtime Dynamic = 0.168184 W

              Instruction Window:
                Area = 0.0198314 mm^2
                Peak Dynamic = 0.040679 W
                Subthreshold Leakage = 0.000550864 W
                Subthreshold Leakage with power gating = 0.000312644 W
                Gate Leakage = 0.000300325 W
                Runtime Dynamic = 0.0405463 W

              FP Instruction Window:
                Area = 0.16824 mm^2
                Peak Dynamic = 0.400407 W
                Subthreshold Leakage = 0.0025486 W
                Subthreshold Leakage with power gating = 0.00145135 W
                Gate Leakage = 0.00137824 W
                Runtime Dynamic = 0.0975142 W

              ROB:
                Area = 0.023407 mm^2
                Peak Dynamic = 0.0399203 W
                Subthreshold Leakage = 0.000614224 W
                Subthreshold Leakage with power gating = 0.000327543 W
                Gate Leakage = 0.000212432 W
                Runtime Dynamic = 0.0301238 W

          Integer ALUs (Count: 1 ):
            Area = 0.0549349 mm^2
            Peak Dynamic = 0.150631 W
            Subthreshold Leakage = 0.00894794 W
            Subthreshold Leakage with power gating = 0.00362391 W
            Gate Leakage = 0.00478051 W
            Runtime Dynamic = 0.154559 W

          Floating Point Units (FPUs) (Count: 2 ):
            Area = 2.35571 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0959259 W
            Subthreshold Leakage with power gating = 0.03885 W
            Gate Leakage = 0.0512492 W
            Runtime Dynamic = 0.206016 W

          Complex ALUs (Mul/Div) (Count: 1 ):
            Area = 0.164805 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0268438 W
            Subthreshold Leakage with power gating = 0.0108717 W
            Gate Leakage = 0.0143415 W
            Runtime Dynamic = 0.137344 W

          Results Broadcast Bus:
            Area Overhead = 0.0126498 mm^2
            Peak Dynamic = 0.105814 W
            Subthreshold Leakage = 0.00735445 W
            Subthreshold Leakage with power gating = 0.00297855 W
            Gate Leakage = 0.00392918 W
            Runtime Dynamic = 0.0455788 W

    L2
    Area = 1.22286 mm^2
    Peak Dynamic = 0.0162441 W
    Subthreshold Leakage = 0.0593036 W
    Subthreshold Leakage with power gating = 0.0294701 W
    Gate Leakage = 0.0163326 W
    Runtime Dynamic = 0.0026054 W

*****************************************************************************************
BUSES
      Area = 0.118743 mm^2
      Peak Dynamic = 0 W
      Subthreshold Leakage = 0.00390107 W
      Subthreshold Leakage with power gating = 0.00157993 W
      Gate Leakage = 0.00307023 W
      Runtime Dynamic = 0 W

      Bus: 
        Area = 0.118743 mm^2
        Peak Dynamic = 0 W
        Subthreshold Leakage = 0.00390107 W
        Subthreshold Leakage with power gating = 0.00157993 W
        Gate Leakage = 0.00307023 W
        Runtime Dynamic = 0 W

*****************************************************************************************
