McPAT (version 1.0 of Aug, 2013) is computing the target processor...
 

McPAT (version 1.0 of Aug, 2013) results  (current print level is 5)
*****************************************************************************************
  Technology 32 nm
  Using Long Channel Devices When Appropriate
  Interconnect metal projection= aggressive interconnect technology projection
  Core clock Rate(MHz) 2000

*****************************************************************************************
Processor: 
  Area = 16.81 mm^2
  Peak Power = 13.3142 W
  Total Leakage = 1.21734 W
  Peak Dynamic = 12.0968 W
  Subthreshold Leakage = 0.795863 W
  Subthreshold Leakage with power gating = 0.34939 W
  Gate Leakage = 0.421474 W
  Runtime Dynamic = 2.0296 W

  Total Cores: 1 cores 
  Device Type= ITRS high performance device type
    Area = 16.66 mm^2
    Peak Dynamic = 12.0968 W
    Subthreshold Leakage = 0.790935 W
    Subthreshold Leakage with power gating = 0.347473 W
    Gate Leakage = 0.417596 W
    Runtime Dynamic = 2.0296 W

  Total NoCs (Network/Bus): 
  Device Type= ITRS high performance device type
    Area = 0.150017 mm^2
    Peak Dynamic = 0 W
    Subthreshold Leakage = 0.00492853 W
    Subthreshold Leakage with power gating = 0.00199605 W
    Gate Leakage = 0.00387887 W
    Runtime Dynamic = 0 W

*****************************************************************************************
Core:
      Area = 16.66 mm^2
      Peak Dynamic = 12.0968 W
      Subthreshold Leakage = 0.790935 W
      Subthreshold Leakage with power gating = 0.347473 W
      Gate Leakage = 0.417596 W
      Runtime Dynamic = 2.0296 W

      Instruction Fetch Unit:
        Area = 3.21989 mm^2
        Peak Dynamic = 3.70806 W
        Subthreshold Leakage = 0.109946 W
        Subthreshold Leakage with power gating = 0.0514399 W
        Gate Leakage = 0.0522881 W
        Runtime Dynamic = 0.211093 W

          Instruction Cache:
            Area = 0.778924 mm^2
            Peak Dynamic = 1.31828 W
            Subthreshold Leakage = 0.0298653 W
            Subthreshold Leakage with power gating = 0.016857 W
            Gate Leakage = 0.0155753 W
            Runtime Dynamic = 0.0221731 W

          Branch Target Buffer:
            Area = 0.40049 mm^2
            Peak Dynamic = 0.0639598 W
            Subthreshold Leakage = 0.0125781 W
            Subthreshold Leakage with power gating = 0.00683951 W
            Gate Leakage = 0.00459494 W
            Runtime Dynamic = 0.00833189 W

          Branch Predictor:
            Area = 0.0802363 mm^2
            Peak Dynamic = 0.0247518 W
            Subthreshold Leakage = 0.00265851 W
            Subthreshold Leakage with power gating = 0.00144804 W
            Gate Leakage = 0.000851618 W
            Runtime Dynamic = 0.00332845 W

              Global Predictor:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.00100453 W
                Subthreshold Leakage with power gating = 0.000547437 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 0.00110885 W

              Local Predictor:
              L1_Local Predictor:
                Area = 0.0132151 mm^2
                Peak Dynamic = 0.00485939 W
                Subthreshold Leakage = 0.000522926 W
                Subthreshold Leakage with power gating = 0.000283053 W
                Gate Leakage = 0.000173252 W
                Runtime Dynamic = 0.000692761 W

              L2_Local Predictor:
                Area = 0.00654633 mm^2
                Peak Dynamic = 0.00242012 W
                Subthreshold Leakage = 0.000229963 W
                Subthreshold Leakage with power gating = 0.000129831 W
                Gate Leakage = 8.86473e-05 W
                Runtime Dynamic = 0.000345003 W

              Chooser:
                Area = 0.0275151 mm^2
                Peak Dynamic = 0.00798554 W
                Subthreshold Leakage = 0.00100453 W
                Subthreshold Leakage with power gating = 0.000547437 W
                Gate Leakage = 0.000313214 W
                Runtime Dynamic = 0.00110885 W

              RAS:
                Area = 0.00544471 mm^2
                Peak Dynamic = 0.00392128 W
                Subthreshold Leakage = 0.000126519 W
                Subthreshold Leakage with power gating = 7.01108e-05 W
                Gate Leakage = 5.19378e-05 W
                Runtime Dynamic = 0.000417983 W

          Instruction Buffer:
            Area = 0.0366066 mm^2
            Peak Dynamic = 1.36609 W
            Subthreshold Leakage = 0.000510583 W
            Subthreshold Leakage with power gating = 0.000240193 W
            Gate Leakage = 0.000204744 W
            Runtime Dynamic = 0.0951317 W

          Instruction Decoder:
            Area = 1.87909 mm^2
            Peak Dynamic = 0.786237 W
            Subthreshold Leakage = 0.0591232 W
            Subthreshold Leakage with power gating = 0.0239449 W
            Gate Leakage = 0.0240558 W
            Runtime Dynamic = 0.082128 W

      Renaming Unit:
        Area = 0.303585 mm^2
        Peak Dynamic = 2.73369 W
        Subthreshold Leakage = 0.0113647 W
        Subthreshold Leakage with power gating = 0.00561434 W
        Gate Leakage = 0.0120767 W
        Runtime Dynamic = 0.155333 W

          Int Front End RAT:
            Area = 0.15267 mm^2
            Peak Dynamic = 1.44001 W
            Subthreshold Leakage = 0.00138017 W
            Subthreshold Leakage with power gating = 0.000786699 W
            Gate Leakage = 0.000701627 W
            Runtime Dynamic = 0.147883 W

          FP Front End RAT:
            Area = 0.0662667 mm^2
            Peak Dynamic = 1.08002 W
            Subthreshold Leakage = 0.00466202 W
            Subthreshold Leakage with power gating = 0.00265735 W
            Gate Leakage = 0.00432143 W
            Runtime Dynamic = 0 W

          Free List:
            Area = 0.040102 mm^2
            Peak Dynamic = 0.0356646 W
            Subthreshold Leakage = 0.000111881 W
            Subthreshold Leakage with power gating = 5.9989e-05 W
            Gate Leakage = 4.79023e-05 W
            Runtime Dynamic = 0.00745083 W

      Load Store Unit:
        Area = 1.6558 mm^2
        Peak Dynamic = 1.18706 W
        Subthreshold Leakage = 0.0493304 W
        Subthreshold Leakage with power gating = 0.0267036 W
        Gate Leakage = 0.0290366 W
        Runtime Dynamic = 0.210097 W

          Data Cache:
            Area = 1.24059 mm^2
            Peak Dynamic = 1.04818 W
            Subthreshold Leakage = 0.0408129 W
            Subthreshold Leakage with power gating = 0.0227083 W
            Gate Leakage = 0.02038 W
            Runtime Dynamic = 0.096707 W

          LoadQ:
            Area = 0.043215 mm^2
            Peak Dynamic = 0.0315795 W
            Subthreshold Leakage = 0.00137797 W
            Subthreshold Leakage with power gating = 0.000785444 W
            Gate Leakage = 0.000712518 W
            Runtime Dynamic = 0.0315795 W

          StoreQ:
            Area = 0.0517429 mm^2
            Peak Dynamic = 0.040905 W
            Subthreshold Leakage = 0.00192894 W
            Subthreshold Leakage with power gating = 0.0010995 W
            Gate Leakage = 0.000938396 W
            Runtime Dynamic = 0.08181 W

      Memory Management Unit:
        Area = 0.122423 mm^2
        Peak Dynamic = 0.181854 W
        Subthreshold Leakage = 0.00871791 W
        Subthreshold Leakage with power gating = 0.00410945 W
        Gate Leakage = 0.00865614 W
        Runtime Dynamic = 0.0311656 W

          Itlb:
            Area = 0.0320988 mm^2
            Peak Dynamic = 0.0336489 W
            Subthreshold Leakage = 0.00134609 W
            Subthreshold Leakage with power gating = 0.000767271 W
            Gate Leakage = 0.000646352 W
            Runtime Dynamic = 0.00489064 W

          Dtlb:
            Area = 0.0457784 mm^2
            Peak Dynamic = 0.0260114 W
            Subthreshold Leakage = 0.0021612 W
            Subthreshold Leakage with power gating = 0.00123188 W
            Gate Leakage = 0.0010041 W
            Runtime Dynamic = 0.0262749 W

      Execution Unit:
        Area = 7.05778 mm^2
        Peak Dynamic = 4.26681 W
        Subthreshold Leakage = 0.301621 W
        Subthreshold Leakage with power gating = 0.128622 W
        Gate Leakage = 0.165293 W
        Runtime Dynamic = 1.4188 W

          Register Files:
            Area = 0.994458 mm^2
            Peak Dynamic = 0.0545393 W
            Subthreshold Leakage = 0.0046848 W
            Subthreshold Leakage with power gating = 0.00198037 W
            Gate Leakage = 0.00240354 W
            Runtime Dynamic = 0.0628618 W

              Integer RF:
                Area = 0.637216 mm^2
                Peak Dynamic = 0.0545393 W
                Subthreshold Leakage = 0.00302413 W
                Subthreshold Leakage with power gating = 0.00125939 W
                Gate Leakage = 0.00158577 W
                Runtime Dynamic = 0.0557789 W

              Floating Point RF:
                Area = 0.357242 mm^2
                Peak Dynamic = 0 W
                Subthreshold Leakage = 0.00166067 W
                Subthreshold Leakage with power gating = 0.000720975 W
                Gate Leakage = 0.000817768 W
                Runtime Dynamic = 0.00708287 W

          Instruction Scheduler:
            Area = 2.80335 mm^2
            Peak Dynamic = 4.02631 W
            Subthreshold Leakage = 0.0433121 W
            Subthreshold Leakage with power gating = 0.0239237 W
            Gate Leakage = 0.0231668 W
            Runtime Dynamic = 0.555288 W

              Instruction Window:
                Area = 1.60276 mm^2
                Peak Dynamic = 2.20519 W
                Subthreshold Leakage = 0.0363267 W
                Subthreshold Leakage with power gating = 0.02069 W
                Gate Leakage = 0.0194384 W
                Runtime Dynamic = 0.299709 W

              FP Instruction Window:
                Area = 0.141355 mm^2
                Peak Dynamic = 0.381128 W
                Subthreshold Leakage = 0.00223175 W
                Subthreshold Leakage with power gating = 0.00125592 W
                Gate Leakage = 0.00124765 W
                Runtime Dynamic = 0.102548 W

              ROB:
                Area = 1.05923 mm^2
                Peak Dynamic = 1.43999 W
                Subthreshold Leakage = 0.0047537 W
                Subthreshold Leakage with power gating = 0.00197779 W
                Gate Leakage = 0.00248082 W
                Runtime Dynamic = 0.153031 W

          Integer ALUs (Count: 12 ):
            Area = 0.659219 mm^2
            Peak Dynamic = 0.117105 W
            Subthreshold Leakage = 0.107375 W
            Subthreshold Leakage with power gating = 0.043487 W
            Gate Leakage = 0.0573661 W
            Runtime Dynamic = 0.165437 W

          Floating Point Units (FPUs) (Count: 2 ):
            Area = 2.35571 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0959259 W
            Subthreshold Leakage with power gating = 0.03885 W
            Gate Leakage = 0.0512492 W
            Runtime Dynamic = 0.206016 W

          Complex ALUs (Mul/Div) (Count: 1 ):
            Area = 0.164805 mm^2
            Peak Dynamic = 0 W
            Subthreshold Leakage = 0.0268438 W
            Subthreshold Leakage with power gating = 0.0108717 W
            Gate Leakage = 0.0143415 W
            Runtime Dynamic = 0.137344 W

          Results Broadcast Bus:
            Area Overhead = 0.0357035 mm^2
            Peak Dynamic = 0.0564635 W
            Subthreshold Leakage = 0.0182686 W
            Subthreshold Leakage with power gating = 0.00739878 W
            Gate Leakage = 0.00976015 W
            Runtime Dynamic = 0.291856 W

    L2
    Area = 1.22286 mm^2
    Peak Dynamic = 0.0193423 W
    Subthreshold Leakage = 0.0593036 W
    Subthreshold Leakage with power gating = 0.0294701 W
    Gate Leakage = 0.0163326 W
    Runtime Dynamic = 0.00310483 W

*****************************************************************************************
BUSES
      Area = 0.150017 mm^2
      Peak Dynamic = 0 W
      Subthreshold Leakage = 0.00492853 W
      Subthreshold Leakage with power gating = 0.00199605 W
      Gate Leakage = 0.00387887 W
      Runtime Dynamic = 0 W

      Bus: 
        Area = 0.150017 mm^2
        Peak Dynamic = 0 W
        Subthreshold Leakage = 0.00492853 W
        Subthreshold Leakage with power gating = 0.00199605 W
        Gate Leakage = 0.00387887 W
        Runtime Dynamic = 0 W

*****************************************************************************************
