- Main Page
- Modules
- Data Structures
- Files

- Search for |

# Decoding Instructions

## Data Structures

struct | xed_decoded_inst_s
| The main container for instructions. More...
struct | xed_inst_s
| constant information about a decoded instruction form, including the pointer to the constant operand properties xed_operand_t for this instruction form. More...
struct | xed_operand_s
| Constant information about an individual generic operand, like an operand template, describing the operand properties. More...

## xed_inst_t Attribute access

XED_DLL_EXPORT xed_attribute_enum_t | xed_attribute (unsigned int i)
| Return the i'th global attribute in a linear sequence, independent of any instruction.
XED_DLL_EXPORT unsigned int | xed_attribute_max (void)
| Return the maximum number of defined attributes, independent of any instruction.
XED_DLL_EXPORT xed_uint32_t | xed_inst_get_attribute (const xed_inst_t *p, xed_attribute_enum_t attr)
| Scan for the attribute attr and return 1 if it is found, 0 otherwise.
XED_DLL_EXPORT xed_attributes_t | xed_inst_get_attributes (const xed_inst_t *p)
| Return the attributes bit vector.

## xed_decoded_inst_t Operand Field Details

XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_conditionally_writes_registers (const xed_decoded_inst_t *p)
XED_DLL_EXPORT xed_reg_enum_t | xed_decoded_inst_get_base_reg (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_int32_t | xed_decoded_inst_get_branch_displacement (const xed_decoded_inst_t *p)
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_branch_displacement_width (const xed_decoded_inst_t *p)
| Result in BYTES.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_branch_displacement_width_bits (const xed_decoded_inst_t *p)
| Result in BITS.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_immediate_is_signed (const xed_decoded_inst_t *p)
| Return true if the first immediate (IMM0) is signed.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_immediate_width (const xed_decoded_inst_t *p)
| Return the immediate width in BYTES.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_immediate_width_bits (const xed_decoded_inst_t *p)
| Return the immediate width in BITS.
XED_DLL_EXPORT xed_reg_enum_t | xed_decoded_inst_get_index_reg (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT unsigned int | xed_decoded_inst_get_memop_address_width (const xed_decoded_inst_t *p, xed_uint_t memop_idx)
XED_DLL_EXPORT xed_int64_t | xed_decoded_inst_get_memory_displacement (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_memory_displacement_width (const xed_decoded_inst_t *p, unsigned int mem_idx)
| Result in BYTES.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_memory_displacement_width_bits (const xed_decoded_inst_t *p, unsigned int mem_idx)
| Result in BITS.
XED_DLL_EXPORT unsigned int | xed_decoded_inst_get_memory_operand_length (const xed_decoded_inst_t *p, unsigned int memop_idx)
XED_DLL_EXPORT xed_reg_enum_t | xed_decoded_inst_get_reg (const xed_decoded_inst_t *p, xed_operand_enum_t reg_operand)
| Return the specified register operand.
XED_DLL_EXPORT const xed_simple_flag_t * | xed_decoded_inst_get_rflags_info (const xed_decoded_inst_t *p)
| See the comment on xed_decoded_inst_uses_rflags().
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_scale (const xed_decoded_inst_t *p, unsigned int mem_idx)
static XED_INLINE xed_uint8_t | xed_decoded_inst_get_second_immediate (const xed_decoded_inst_t *p)
| Return the second immediate.
XED_DLL_EXPORT xed_reg_enum_t | xed_decoded_inst_get_seg_reg (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_int32_t | xed_decoded_inst_get_signed_immediate (const xed_decoded_inst_t *p)
XED_DLL_EXPORT xed_uint64_t | xed_decoded_inst_get_unsigned_immediate (const xed_decoded_inst_t *p)
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_is_prefetch (const xed_decoded_inst_t *p)
| Returns true if the instruction is a prefetch.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_mem_read (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_mem_written (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_mem_written_only (const xed_decoded_inst_t *p, unsigned int mem_idx)
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_number_of_memory_operands (const xed_decoded_inst_t *p)
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_uses_rflags (const xed_decoded_inst_t *p)
| This returns 1 if the flags are read or written.

## xed_decoded_inst_t Printers

XED_DLL_EXPORT void | xed_decoded_inst_dump (const xed_decoded_inst_t *p, char *buf, int buflen)
| Print out all the information about the decoded instruction to the buffer buf whose length is maximally buflen.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_dump_att_format (const xed_decoded_inst_t *p, char *buf, int buflen, xed_uint64_t runtime_address)
| Print the instructions with the destination operand on the right, with several exceptions (bound, invlpga, enter, and other instructions with two immediate operands).
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_dump_att_format_context (const xed_decoded_inst_t *p, char *buf, int buflen, xed_uint64_t runtime_address, void *context)
| Print the instructions with the destination operand on the right, with several exceptions (bound, invlpga, enter, and other instructions with two immediate operands).
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_dump_intel_format (const xed_decoded_inst_t *p, char *buf, int buflen, xed_uint64_t runtime_address)
| Print the instructions with the destination on the left.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_dump_intel_format_context (const xed_decoded_inst_t *p, char *buf, int buflen, xed_uint64_t runtime_address, void *context)
| Print the instructions with the destination on the left.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_dump_xed_format (const xed_decoded_inst_t *p, char *buf, int buflen, xed_uint64_t runtime_address)
| Print the instruction information in an verbose format.

## xed_decoded_inst_t Attirbutes and properties

XED_DLL_EXPORT xed_uint32_t | xed_decoded_inst_get_attribute (const xed_decoded_inst_t *p, xed_attribute_enum_t attr)
| Returns 1 if the attribute is defined for this instruction.
XED_DLL_EXPORT xed_attributes_t | xed_decoded_inst_get_attributes (const xed_decoded_inst_t *p)
| Returns the attribute bitvector.

## xed_decoded_inst_t get Byte

static XED_INLINE xed_uint8_t | xed_decoded_inst_get_byte (const xed_decoded_inst_t *p, xed_uint_t byte_index)
| Read itext byte.

## xed_decoded_inst_t High-level accessors

static XED_INLINE xed_category_enum_t | xed_decoded_inst_get_category (const xed_decoded_inst_t *p)
| Return the instruction xed_category_enum_t enumeration.
static XED_INLINE xed_extension_enum_t | xed_decoded_inst_get_extension (const xed_decoded_inst_t *p)
| Return the instruction xed_extension_enum_t enumeration.
static XED_INLINE xed_iclass_enum_t | xed_decoded_inst_get_iclass (const xed_decoded_inst_t *p)
| Return the instruction xed_iclass_enum_t enumeration.
static XED_INLINE xed_isa_set_enum_t | xed_decoded_inst_get_isa_set (xed_decoded_inst_t const *const p)
| Return the instruction xed_isa_set_enum_t enumeration.
static XED_INLINE const xed_inst_t * | xed_decoded_inst_inst (const xed_decoded_inst_t *p)
| Return the xed_inst_t structure for this instruction.
static XED_INLINE xed_bool_t | xed_decoded_inst_valid (const xed_decoded_inst_t *p)
| Return true if the instruction is valid.

## IFORM handling

static XED_INLINE xed_iform_enum_t | xed_decoded_inst_get_iform_enum (const xed_decoded_inst_t *p)
| Return the instruction iform enum of type xed_iform_enum_t .
static XED_INLINE unsigned int | xed_decoded_inst_get_iform_enum_dispatch (const xed_decoded_inst_t *p)
| Return the instruction zero-based iform number based on masking the corresponding xed_iform_enum_t.

## Modes

static XED_INLINE xed_chip_enum_t | xed_decoded_inst_get_input_chip (const xed_decoded_inst_t *p)
| Return the user-specified xed_chip_enum_t chip name, or XED_CHIP_INVALID if not set.
static XED_INLINE xed_uint_t | xed_decoded_inst_get_machine_mode_bits (const xed_decoded_inst_t *p)
| Returns 16/32/64 indicating the machine mode with in bits.
XED_DLL_EXPORT xed_uint32_t | xed_decoded_inst_get_operand_width (const xed_decoded_inst_t *p)
| Returns the operand width in bits: 8/16/32/64.
static XED_INLINE xed_uint_t | xed_decoded_inst_get_stack_address_mode_bits (const xed_decoded_inst_t *p)
| Returns 16/32/64 indicating the stack addressing mode with in bits.
static XED_INLINE void | xed_decoded_inst_set_input_chip (xed_decoded_inst_t *p, xed_chip_enum_t chip)
| Set a user-specified xed_chip_enum_t chip name for restricting decode.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_valid_for_chip (xed_decoded_inst_t const *const p, xed_chip_enum_t chip)
| Indicate if this decoded instruction is valid for the specified xed_chip_enum_t chip.

## xed_decoded_inst_t Length

static XED_INLINE xed_uint_t | xed_decoded_inst_get_length (const xed_decoded_inst_t *p)
| Return the length of the decoded instruction in bytes.

## xed_decoded_inst_t User Data Field

static XED_INLINE xed_uint64_t | xed_decoded_inst_get_user_data (xed_decoded_inst_t *p)
| Return a user data field for arbitrary use by the user after decoding.
static XED_INLINE void | xed_decoded_inst_set_user_data (xed_decoded_inst_t *p, xed_uint64_t new_value)
| Modify the user data field.

## xed_decoded_inst_t Inc Length

static XED_INLINE xed_uint_t | xed_decoded_inst_inc_length (xed_decoded_inst_t *p)
| Increment the length of the decoded instruction in bytes.

## xed_decoded_inst_t Operands

static XED_INLINE unsigned int | xed_decoded_inst_noperands (const xed_decoded_inst_t *p)
| Return the number of operands.
XED_DLL_EXPORT unsigned int | xed_decoded_inst_operand_element_size_bits (const xed_decoded_inst_t *p, unsigned int operand_index)
| Return the size of an element in bits (for SSE and AVX operands).
XED_DLL_EXPORT xed_operand_element_type_enum_t | xed_decoded_inst_operand_element_type (const xed_decoded_inst_t *p, unsigned int operand_index)
| Return the type of an element of type xed_operand_element_type_enum_t (for SSE and AVX operands).
XED_DLL_EXPORT unsigned int | xed_decoded_inst_operand_elements (const xed_decoded_inst_t *p, unsigned int operand_index)
| Return the number of element in the operand (for SSE and AVX operands).
XED_DLL_EXPORT unsigned int | xed_decoded_inst_operand_length (const xed_decoded_inst_t *p, unsigned int operand_index)
| Deprecated -- returns the length in bytes of the operand_index'th operand.
XED_DLL_EXPORT unsigned int | xed_decoded_inst_operand_length_bits (const xed_decoded_inst_t *p, unsigned int operand_index)
| Return the length in bits of the operand_index'th operand.
static XED_INLINE xed_operand_values_t * | xed_decoded_inst_operands (xed_decoded_inst_t *p)
| Obtain a non-constant pointer to the operands.
static XED_INLINE const xed_operand_values_t * | xed_decoded_inst_operands_const (const xed_decoded_inst_t *p)
| Obtain a constant pointer to the operands.

## xed_decoded_inst_t Modification

XED_DLL_EXPORT void | xed_decoded_inst_set_branch_displacement (xed_decoded_inst_t *p, xed_int32_t disp, xed_uint_t length_bytes)
| Set the branch displacement using a BYTE length.
XED_DLL_EXPORT void | xed_decoded_inst_set_branch_displacement_bits (xed_decoded_inst_t *p, xed_int32_t disp, xed_uint_t length_bits)
| Set the branch displacement a BITS length.
XED_DLL_EXPORT void | xed_decoded_inst_set_immediate_signed (xed_decoded_inst_t *p, xed_int32_t x, xed_uint_t length_bytes)
| Set the signed immediate a BYTE length.
XED_DLL_EXPORT void | xed_decoded_inst_set_immediate_signed_bits (xed_decoded_inst_t *p, xed_int32_t x, xed_uint_t length_bits)
| Set the signed immediate a BITS length.
XED_DLL_EXPORT void | xed_decoded_inst_set_immediate_unsigned (xed_decoded_inst_t *p, xed_uint64_t x, xed_uint_t length_bytes)
| Set the unsigned immediate a BYTE length.
XED_DLL_EXPORT void | xed_decoded_inst_set_immediate_unsigned_bits (xed_decoded_inst_t *p, xed_uint64_t x, xed_uint_t length_bits)
| Set the unsigned immediate a BITS length.
XED_DLL_EXPORT void | xed_decoded_inst_set_memory_displacement (xed_decoded_inst_t *p, xed_int64_t disp, xed_uint_t length_bytes)
| Set the memory displacement using a BYTE length.
XED_DLL_EXPORT void | xed_decoded_inst_set_memory_displacement_bits (xed_decoded_inst_t *p, xed_int64_t disp, xed_uint_t length_bits)
| Set the memory displacement a BITS length.
XED_DLL_EXPORT void | xed_decoded_inst_set_scale (xed_decoded_inst_t *p, xed_uint_t scale)

## xed_decoded_inst_t Set Length

static XED_INLINE xed_uint_t | xed_decoded_inst_set_length (xed_decoded_inst_t *p, unsigned char length)
| Set the length of the decoded instruction in bytes.

## xed_decoded_inst_t Initialization

static XED_INLINE void | xed_decoded_inst_set_mode (xed_decoded_inst_t *p, xed_machine_mode_enum_t mmode, xed_address_width_enum_t stack_addr_width)
| Set the machine mode and stack addressing width directly.
XED_DLL_EXPORT void | xed_decoded_inst_zero (xed_decoded_inst_t *p)
| Zero the decode structure completely.
XED_DLL_EXPORT void | xed_decoded_inst_zero_keep_mode (xed_decoded_inst_t *p)
| Zero the decode structure, but preserve the existing machine state/mode information.
XED_DLL_EXPORT void | xed_decoded_inst_zero_keep_mode_from_operands (xed_decoded_inst_t *p, const xed_operand_values_t *operands)
| Zero the decode structure, but copy the existing machine state/mode information from the supplied operands pointer.
XED_DLL_EXPORT void | xed_decoded_inst_zero_set_mode (xed_decoded_inst_t *p, const xed_state_t *dstate)
| Zero the decode structure, but set the machine state/mode information.

## xed_inst_t Template Instruction Information

XED_DLL_EXPORT unsigned int | xed_inst_cpl (const xed_inst_t *p)
| xed_inst_cpl() is DEPRECATED.
static XED_INLINE unsigned int | xed_inst_noperands (const xed_inst_t *p)
| Number of instruction operands.
XED_DLL_EXPORT const xed_operand_t * | xed_inst_operand (const xed_inst_t *p, unsigned int i)
| Obtain a pointer to an individual operand.

## Exceptions

static XED_INLINE xed_exception_enum_t | xed_inst_exception (const xed_inst_t *p)
| Return xed_exception_enum_t if present for the specified instruction.

## xed_inst_t Template Operand Read/Written

XED_DLL_EXPORT xed_uint_t | xed_operand_conditional_read (const xed_operand_t *p)
| If the operand has a conditional read (may also write).
XED_DLL_EXPORT xed_uint_t | xed_operand_conditional_write (const xed_operand_t *p)
| If the operand has a conditional write (may also read).
XED_DLL_EXPORT xed_uint_t | xed_operand_read (const xed_operand_t *p)
| If the operand is read, including conditional reads.
XED_DLL_EXPORT xed_uint_t | xed_operand_read_and_written (const xed_operand_t *p)
| If the operand is read-and-written, conditional reads and conditional writes.
XED_DLL_EXPORT xed_uint_t | xed_operand_read_only (const xed_operand_t *p)
| If the operand is read-only, including conditional reads.
static XED_INLINE xed_operand_action_enum_t | xed_operand_rw (const xed_operand_t *p)
| Returns the raw R/W action.
XED_DLL_EXPORT xed_uint_t | xed_operand_written (const xed_operand_t *p)
| If the operand is written, including conditional writes.
XED_DLL_EXPORT xed_uint_t | xed_operand_written_only (const xed_operand_t *p)
| If the operand is written-only, including conditional writes.

## xed_inst_t Template Operands Access

static XED_INLINE xed_uint32_t | xed_operand_imm (const xed_operand_t *p)
static XED_INLINE xed_operand_enum_t | xed_operand_name (const xed_operand_t *p)
static XED_INLINE xed_nonterminal_enum_t | xed_operand_nonterminal_name (const xed_operand_t *p)
static XED_INLINE xed_operand_visibility_enum_t | xed_operand_operand_visibility (const xed_operand_t *p)
XED_DLL_EXPORT void | xed_operand_print (const xed_operand_t *p, char *buf, int buflen)
| Print the operand p into the buffer buf, of length buflen.
static XED_INLINE xed_reg_enum_t | xed_operand_reg (const xed_operand_t *p)
| Careful with this one -- use xed_decoded_inst_get_reg()! This one is probably not what you think it is.
static XED_INLINE xed_uint_t | xed_operand_template_is_register (const xed_operand_t *p)
| Careful with this one; See xed_operand_is_register().
static XED_INLINE xed_operand_type_enum_t | xed_operand_type (const xed_operand_t *p)
static XED_INLINE xed_operand_width_enum_t | xed_operand_width (const xed_operand_t *p)
XED_DLL_EXPORT xed_uint32_t | xed_operand_width_bits (const xed_operand_t *p, const xed_uint32_t eosz)
static XED_INLINE xed_operand_element_xtype_enum_t | xed_operand_xtype (const xed_operand_t *p)

## xed_inst_t Template Operand Enum Name Classification

static XED_INLINE xed_uint_t | xed_operand_is_memory_addressing_register (xed_operand_enum_t name)
| Tests the enum for inclusion in XED_OPERAND_{BASE0,BASE1,INDEX,SEG0,SEG1}.
static XED_INLINE xed_uint_t | xed_operand_is_register (xed_operand_enum_t name)
| Tests the enum for inclusion in XED_OPERAND_REG0 through XED_OPERAND_REG15.

## Typedefs

typedef xed_decoded_inst_s | xed_decoded_inst_t
| The main container for instructions.
typedef xed_inst_s | xed_inst_t
| constant information about a decoded instruction form, including the pointer to the constant operand properties xed_operand_t for this instruction form.
typedef xed_operand_s | xed_operand_t
| Constant information about an individual generic operand, like an operand template, describing the operand properties.

## Functions

XED_DLL_EXPORT xed_error_enum_t | xed_decode (xed_decoded_inst_t *xedd, const xed_uint8_t *itext, const unsigned int bytes)
| This is the main interface to the decoder.
XED_DLL_EXPORT xed_uint8_t | xed_decoded_inst_get_modrm (const xed_decoded_inst_t *p)
| Returns the modrm byte.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_get_nprefixes (xed_decoded_inst_t *p)
| Returns the number of legacy prefixes.
XED_DLL_EXPORT xed_uint32_t | xed_decoded_inst_has_mpx_prefix (const xed_decoded_inst_t *p)
| Returns 1 if the instruction has mpx prefix.
XED_DLL_EXPORT xed_uint32_t | xed_decoded_inst_is_xacquire (const xed_decoded_inst_t *p)
| Returns 1 if the instruction is xacquire.
XED_DLL_EXPORT xed_uint32_t | xed_decoded_inst_is_xrelease (const xed_decoded_inst_t *p)
| Returns 1 if the instruction is xrelease.
XED_DLL_EXPORT xed_bool_t | xed_decoded_inst_masked_vector_operation (xed_decoded_inst_t *p)
| Returns 1 iff the instruction uses destination-masking.
XED_DLL_EXPORT xed_uint_t | xed_decoded_inst_vector_length_bits (xed_decoded_inst_t const *const p)
| Returns 128, 256 or 512 for operations in the VEX, EVEX (or XOP) encoding space and returns 0 for (most) nonvector operations.
XED_DLL_EXPORT xed_error_enum_t | xed_ild_decode (xed_decoded_inst_t *xedd, const xed_uint8_t *itext, const unsigned int bytes)
| This function just does instruction length decoding.
XED_DLL_EXPORT const xed_inst_t * | xed_inst_table_base (void)
| Return the base of instruction table.

## Detailed Description

To decode an instruction you are required to provide

- a machine state (operating mode and stack addressing width)
- a pointer to the instruction text array of bytes
- a length of the text array

The machine state is passed in to decoder via the class xed_state_t . That state is set via the constructor of each xed_decoded_inst_t .

The xed_decoded_inst_t contains the results of decoding after a successful decode.

The xed_decoded_inst_t includes an array of xed_operand_values_t and that is where most of the information about the operands, resources etc. are stored. See the Operand storage fields interface. The array is indexed by the xed_operand_enum_t enumeration. Do not access it directly though; use the interface functions in the Operand storage fields interface for portability.

After decoding the xed_decoded_inst_t contains a pointer to the xed_inst_t which acts like a kind of template giving static information about the decoded instruction: what are the types of the operands, the iclass, category extension, etc. The xed_inst_t is accessed via the xed_decoded_inst_inst(cont xed_decoded_inst_t* xedd) function.

Before every decode, you must call one of the initialization functions. The most common case would be to use xed_decoded_inst_zero_keep_mode() or maybe xed_decoded_inst_zero_set_mode().

## Typedef Documentation

typedef struct xed_decoded_inst_s xed_decoded_inst_t

| The main container for instructions. After decode, it holds an array of operands with derived information from decode and also valid xed_inst_t pointer which describes the operand templates and the operand order. See Decoding Instructions for API documentation.

typedef struct xed_inst_s xed_inst_t

| constant information about a decoded instruction form, including the pointer to the constant operand properties xed_operand_t for this instruction form.

typedef struct xed_operand_s xed_operand_t

| Constant information about an individual generic operand, like an operand template, describing the operand properties. See Decoding Instructions for API information.

## Function Documentation

XED_DLL_EXPORT xed_attribute_enum_t xed_attribute | ( | unsigned int | i | ) |

| Return the i'th global attribute in a linear sequence, independent of any instruction. This is used for scanning and printing all attributes.

XED_DLL_EXPORT unsigned int xed_attribute_max | ( | void |  | ) |

| Return the maximum number of defined attributes, independent of any instruction.

XED_DLL_EXPORT xed_error_enum_t xed_decode | ( | xed_decoded_inst_t * | xedd,
|  | const xed_uint8_t * | itext,
|  | const unsigned int | bytes
| ) |

| This is the main interface to the decoder.

Parameters:

  | xedd | the decoded instruction of type xed_decoded_inst_t . Mode/state sent in via xedd; See the xed_state_t
  | itext | the pointer to the array of instruction text bytes
  | bytes | the length of the itext input array. 1 to 15 bytes, anything more is ignored.

Returns:
  xed_error_enum_t indiciating success (XED_ERROR_NONE) or failure. Note failure can be due to not enough bytes in the input array.

The maximum instruction is 15B and XED will tell you how long the actual instruction is via an API function call xed_decoded_inst_get_length(). However, it is not always safe or advisable for XED to read 15 bytes if the decode location is at the boundary of some sort of protection limit. For example, if one is decoding near the end of a page and the XED user does not want to cause extra page faults, one might send in the number of bytes that would stop at the page boundary. In this case, XED might not be able to decode the instruction and would return an error. The XED user would then have to decide if it was safe to touch the next page and try again to decode with more bytes. Also sometimes the user process does not have read access to the next page and this allows the user to prevent XED from causing process termination by limiting the memory range that XED will access.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_conditionally_writes_registers | ( | const xed_decoded_inst_t * | p | ) |

XED_DLL_EXPORT void xed_decoded_inst_dump | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen
| ) |

| Print out all the information about the decoded instruction to the buffer buf whose length is maximally buflen.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_dump_att_format | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen,
|  | xed_uint64_t | runtime_address
| ) |

| Print the instructions with the destination operand on the right, with several exceptions (bound, invlpga, enter, and other instructions with two immediate operands). Also use instruction name suffixes to indicate operation width. Several instructions names are different as well. Recommendation: buflen must be more than 16 bytes, preferably at least 100 bytes.

Parameters:

  | p | a xed_decoded_inst_t for a decoded instruction
  | buf | a buffer to write the disassembly in to.
  | buflen | maximum length of the disassembly buffer
  | runtime_address | the address of the instruction being disassembled. If zero, the offset is printed for relative branches. If nonzero, XED attempts to print the target address for relative branches.

Returns:
  Returns 0 if the disassembly fails, 1 otherwise.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_dump_att_format_context | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen,
|  | xed_uint64_t | runtime_address,
|  | void * | context
| ) |

| Print the instructions with the destination operand on the right, with several exceptions (bound, invlpga, enter, and other instructions with two immediate operands). Also use instruction name suffixes to indicate operation width. Several instructions names are different as well. buflen must be at least 100 bytes.

Parameters:

  | p | a xed_decoded_inst_t for a decoded instruction
  | buf | a buffer to write the disassembly in to.
  | buflen | maximum length of the disassembly buffer
  | runtime_address | the address of the instruction being disassembled. If zero, the offset is printed for relative branches. If nonzero, XED attempts to print the target address for relative branches.
  | context | A void* used only for the call back routine for symbolic disassembly if one is registered.

Returns:
  Returns 0 if the disassembly fails, 1 otherwise.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_dump_intel_format | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen,
|  | xed_uint64_t | runtime_address
| ) |

| Print the instructions with the destination on the left. Use PTR qualifiers for memory access widths. Recommendation: buflen must be more than 16 bytes, preferably at least 100 bytes.

Parameters:

  | p | a xed_decoded_inst_t for a decoded instruction
  | buf | a buffer to write the disassembly in to.
  | buflen | maximum length of the disassembly buffer
  | runtime_address | the address of the instruction being disassembled. If zero, the offset is printed for relative branches. If nonzero, XED attempts to print the target address for relative branches.

Returns:
  Returns 0 if the disassembly fails, 1 otherwise.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_dump_intel_format_context | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen,
|  | xed_uint64_t | runtime_address,
|  | void * | context
| ) |

| Print the instructions with the destination on the left. Use PTR qualifiers for memory access widths. Recommendation: buflen must be more than 16 bytes, preferably at least 100 bytes.

Parameters:

  | p | a xed_decoded_inst_t for a decoded instruction
  | buf | a buffer to write the disassembly in to.
  | buflen | maximum length of the disassembly buffer
  | runtime_address | the address of the instruction being disassembled. If zero, the offset is printed for relative branches. If nonzero, XED attempts to print the target address for relative branches.
  | context | A void* used only for the call back routine for symbolic disassembly if one is registered.

Returns:
  Returns 0 if the disassembly fails, 1 otherwise.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_dump_xed_format | ( | const xed_decoded_inst_t * | p,
|  | char * | buf,
|  | int | buflen,
|  | xed_uint64_t | runtime_address
| ) |

| Print the instruction information in an verbose format.

Parameters:

  | p | a xed_decoded_inst_t for a decoded instruction
  | buf | a buffer to write the disassembly in to.
  | buflen | maximum length of the disassembly buffer
  | runtime_address | the address of the instruction being disassembled. If zero, the offset is printed for relative branches. If nonzero, XED attempts to print the target address for relative branches.

Returns:
  Returns 0 if the disassembly fails, 1 otherwise.

XED_DLL_EXPORT xed_uint32_t xed_decoded_inst_get_attribute | ( | const xed_decoded_inst_t * | p,
|  | xed_attribute_enum_t | attr
| ) |

| Returns 1 if the attribute is defined for this instruction.

XED_DLL_EXPORT xed_attributes_t xed_decoded_inst_get_attributes | ( | const xed_decoded_inst_t * | p | ) |

| Returns the attribute bitvector.

XED_DLL_EXPORT xed_reg_enum_t xed_decoded_inst_get_base_reg | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

XED_DLL_EXPORT xed_int32_t xed_decoded_inst_get_branch_displacement | ( | const xed_decoded_inst_t * | p | ) |

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_branch_displacement_width | ( | const xed_decoded_inst_t * | p | ) |

| Result in BYTES.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_branch_displacement_width_bits | ( | const xed_decoded_inst_t * | p | ) |

| Result in BITS.

static XED_INLINE xed_uint8_t xed_decoded_inst_get_byte | ( | const xed_decoded_inst_t * | p,
|  | xed_uint_t | byte_index
| ) | `[static]`

| Read itext byte. Read a whole byte from the normal input bytes. Definition at line 272 of file xed-decoded-inst-api.h.

static XED_INLINE xed_category_enum_t xed_decoded_inst_get_category | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the instruction xed_category_enum_t enumeration. Definition at line 62 of file xed-decoded-inst-api.h.

static XED_INLINE xed_extension_enum_t xed_decoded_inst_get_extension | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the instruction xed_extension_enum_t enumeration. Definition at line 68 of file xed-decoded-inst-api.h.

static XED_INLINE xed_iclass_enum_t xed_decoded_inst_get_iclass | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the instruction xed_iclass_enum_t enumeration. Definition at line 80 of file xed-decoded-inst-api.h.

static XED_INLINE xed_iform_enum_t xed_decoded_inst_get_iform_enum | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the instruction iform enum of type xed_iform_enum_t . Definition at line 337 of file xed-decoded-inst-api.h.

static XED_INLINE unsigned int xed_decoded_inst_get_iform_enum_dispatch | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the instruction zero-based iform number based on masking the corresponding xed_iform_enum_t. This value is suitable for dispatching. The maximum value for a particular iclass is provided by xed_iform_max_per_iclass() . Definition at line 347 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_immediate_is_signed | ( | const xed_decoded_inst_t * | p | ) |

| Return true if the first immediate (IMM0) is signed.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_immediate_width | ( | const xed_decoded_inst_t * | p | ) |

| Return the immediate width in BYTES.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_immediate_width_bits | ( | const xed_decoded_inst_t * | p | ) |

| Return the immediate width in BITS.

XED_DLL_EXPORT xed_reg_enum_t xed_decoded_inst_get_index_reg | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

static XED_INLINE xed_chip_enum_t xed_decoded_inst_get_input_chip | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the user-specified xed_chip_enum_t chip name, or XED_CHIP_INVALID if not set. Definition at line 311 of file xed-decoded-inst-api.h.

static XED_INLINE xed_isa_set_enum_t xed_decoded_inst_get_isa_set | ( | xed_decoded_inst_t const *const | p | ) | `[static]`

| Return the instruction xed_isa_set_enum_t enumeration. Definition at line 74 of file xed-decoded-inst-api.h.

static XED_INLINE xed_uint_t xed_decoded_inst_get_length | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the length of the decoded instruction in bytes. Definition at line 233 of file xed-decoded-inst-api.h.

static XED_INLINE xed_uint_t xed_decoded_inst_get_machine_mode_bits | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Returns 16/32/64 indicating the machine mode with in bits. This is derived from the input mode information. Definition at line 286 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT unsigned int xed_decoded_inst_get_memop_address_width | ( | const xed_decoded_inst_t * | p,
|  | xed_uint_t | memop_idx
| ) |

| This factors in things like whether or not the reference is an implicit stack push/pop reference, the machine mode and

XED_DLL_EXPORT xed_int64_t xed_decoded_inst_get_memory_displacement | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_memory_displacement_width | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

| Result in BYTES.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_memory_displacement_width_bits | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

| Result in BITS.

XED_DLL_EXPORT unsigned int xed_decoded_inst_get_memory_operand_length | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | memop_idx
| ) |

XED_DLL_EXPORT xed_uint8_t xed_decoded_inst_get_modrm | ( | const xed_decoded_inst_t * | p | ) |

| Returns the modrm byte.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_nprefixes | ( | xed_decoded_inst_t * | p | ) |

| Returns the number of legacy prefixes.

XED_DLL_EXPORT xed_uint32_t xed_decoded_inst_get_operand_width | ( | const xed_decoded_inst_t * | p | ) |

| Returns the operand width in bits: 8/16/32/64. This is different than the xed_operand_values_get_effective_operand_width() which only returns 16/32/64. This factors in the BYTEOP attribute when computing its return value. This is a convenience function.

XED_DLL_EXPORT xed_reg_enum_t xed_decoded_inst_get_reg | ( | const xed_decoded_inst_t * | p,
|  | xed_operand_enum_t | reg_operand
| ) |

| Return the specified register operand. The specifier is of type xed_operand_enum_t .

XED_DLL_EXPORT const xed_simple_flag_t* xed_decoded_inst_get_rflags_info | ( | const xed_decoded_inst_t * | p | ) |

| See the comment on xed_decoded_inst_uses_rflags(). This can return 0 if the flags are really not used by this instruction.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_get_scale | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

static XED_INLINE xed_uint8_t xed_decoded_inst_get_second_immediate | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the second immediate. Definition at line 478 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_reg_enum_t xed_decoded_inst_get_seg_reg | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

XED_DLL_EXPORT xed_int32_t xed_decoded_inst_get_signed_immediate | ( | const xed_decoded_inst_t * | p | ) |

static XED_INLINE xed_uint_t xed_decoded_inst_get_stack_address_mode_bits | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Returns 16/32/64 indicating the stack addressing mode with in bits. This is derived from the input mode information. Definition at line 295 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_uint64_t xed_decoded_inst_get_unsigned_immediate | ( | const xed_decoded_inst_t * | p | ) |

static XED_INLINE xed_uint64_t xed_decoded_inst_get_user_data | ( | xed_decoded_inst_t * | p | ) | `[static]`

| Return a user data field for arbitrary use by the user after decoding. Definition at line 570 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_uint32_t xed_decoded_inst_has_mpx_prefix | ( | const xed_decoded_inst_t * | p | ) |

| Returns 1 if the instruction has mpx prefix.

static XED_INLINE xed_uint_t xed_decoded_inst_inc_length | ( | xed_decoded_inst_t * | p | ) | `[static]`

| Increment the length of the decoded instruction in bytes. Definition at line 258 of file xed-decoded-inst-api.h.

static XED_INLINE const xed_inst_t* xed_decoded_inst_inst | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the xed_inst_t structure for this instruction. This is the route to the basic operands form information. Definition at line 55 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_is_prefetch | ( | const xed_decoded_inst_t * | p | ) |

| Returns true if the instruction is a prefetch.

XED_DLL_EXPORT xed_uint32_t xed_decoded_inst_is_xacquire | ( | const xed_decoded_inst_t * | p | ) |

| Returns 1 if the instruction is xacquire.

XED_DLL_EXPORT xed_uint32_t xed_decoded_inst_is_xrelease | ( | const xed_decoded_inst_t * | p | ) |

| Returns 1 if the instruction is xrelease.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_masked_vector_operation | ( | xed_decoded_inst_t * | p | ) |

| Returns 1 iff the instruction uses destination-masking. This is 0 for blend operations that use their mask field as a control.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_mem_read | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_mem_written | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_mem_written_only | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | mem_idx
| ) |

static XED_INLINE unsigned int xed_decoded_inst_noperands | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return the number of operands. Definition at line 172 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_number_of_memory_operands | ( | const xed_decoded_inst_t * | p | ) |

XED_DLL_EXPORT unsigned int xed_decoded_inst_operand_element_size_bits | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | operand_index
| ) |

| Return the size of an element in bits (for SSE and AVX operands).

XED_DLL_EXPORT xed_operand_element_type_enum_t xed_decoded_inst_operand_element_type | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | operand_index
| ) |

| Return the type of an element of type xed_operand_element_type_enum_t (for SSE and AVX operands).

XED_DLL_EXPORT unsigned int xed_decoded_inst_operand_elements | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | operand_index
| ) |

| Return the number of element in the operand (for SSE and AVX operands).

XED_DLL_EXPORT unsigned int xed_decoded_inst_operand_length | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | operand_index
| ) |

| Deprecated -- returns the length in bytes of the operand_index'th operand. Use xed_decoded_inst_operand_length_bits() instead.

XED_DLL_EXPORT unsigned int xed_decoded_inst_operand_length_bits | ( | const xed_decoded_inst_t * | p,
|  | unsigned int | operand_index
| ) |

| Return the length in bits of the operand_index'th operand.

static XED_INLINE xed_operand_values_t* xed_decoded_inst_operands | ( | xed_decoded_inst_t * | p | ) | `[static]`

| Obtain a non-constant pointer to the operands. Definition at line 153 of file xed-decoded-inst-api.h.

static XED_INLINE const xed_operand_values_t* xed_decoded_inst_operands_const | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Obtain a constant pointer to the operands. Definition at line 147 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT void xed_decoded_inst_set_branch_displacement | ( | xed_decoded_inst_t * | p,
|  | xed_int32_t | disp,
|  | xed_uint_t | length_bytes
| ) |

| Set the branch displacement using a BYTE length.

XED_DLL_EXPORT void xed_decoded_inst_set_branch_displacement_bits | ( | xed_decoded_inst_t * | p,
|  | xed_int32_t | disp,
|  | xed_uint_t | length_bits
| ) |

| Set the branch displacement a BITS length.

XED_DLL_EXPORT void xed_decoded_inst_set_immediate_signed | ( | xed_decoded_inst_t * | p,
|  | xed_int32_t | x,
|  | xed_uint_t | length_bytes
| ) |

| Set the signed immediate a BYTE length.

XED_DLL_EXPORT void xed_decoded_inst_set_immediate_signed_bits | ( | xed_decoded_inst_t * | p,
|  | xed_int32_t | x,
|  | xed_uint_t | length_bits
| ) |

| Set the signed immediate a BITS length.

XED_DLL_EXPORT void xed_decoded_inst_set_immediate_unsigned | ( | xed_decoded_inst_t * | p,
|  | xed_uint64_t | x,
|  | xed_uint_t | length_bytes
| ) |

| Set the unsigned immediate a BYTE length.

XED_DLL_EXPORT void xed_decoded_inst_set_immediate_unsigned_bits | ( | xed_decoded_inst_t * | p,
|  | xed_uint64_t | x,
|  | xed_uint_t | length_bits
| ) |

| Set the unsigned immediate a BITS length.

static XED_INLINE void xed_decoded_inst_set_input_chip | ( | xed_decoded_inst_t * | p,
|  | xed_chip_enum_t | chip
| ) | `[static]`

| Set a user-specified xed_chip_enum_t chip name for restricting decode. Definition at line 317 of file xed-decoded-inst-api.h.

static XED_INLINE xed_uint_t xed_decoded_inst_set_length | ( | xed_decoded_inst_t * | p,
|  | unsigned char | length
| ) | `[static]`

| Set the length of the decoded instruction in bytes. Definition at line 245 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT void xed_decoded_inst_set_memory_displacement | ( | xed_decoded_inst_t * | p,
|  | xed_int64_t | disp,
|  | xed_uint_t | length_bytes
| ) |

| Set the memory displacement using a BYTE length.

XED_DLL_EXPORT void xed_decoded_inst_set_memory_displacement_bits | ( | xed_decoded_inst_t * | p,
|  | xed_int64_t | disp,
|  | xed_uint_t | length_bits
| ) |

| Set the memory displacement a BITS length.

static XED_INLINE void xed_decoded_inst_set_mode | ( | xed_decoded_inst_t * | p,
|  | xed_machine_mode_enum_t | mmode,
|  | xed_address_width_enum_t | stack_addr_width
| ) | `[static]`

| Set the machine mode and stack addressing width directly. This is NOT a full initialization; Call xed_decoded_inst_zero() before using this if you want a clean slate. Definition at line 212 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT void xed_decoded_inst_set_scale | ( | xed_decoded_inst_t * | p,
|  | xed_uint_t | scale
| ) |

static XED_INLINE void xed_decoded_inst_set_user_data | ( | xed_decoded_inst_t * | p,
|  | xed_uint64_t | new_value
| ) | `[static]`

| Modify the user data field. Definition at line 575 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_uses_rflags | ( | const xed_decoded_inst_t * | p | ) |

| This returns 1 if the flags are read or written. This will return 0 otherwise. This will return 0 if the flags are really not used by this instruction. For some shifts/rotates, XED puts a flags operand in the operand array before it knows if the flags are used because of mode-dependent masking effects on the immediate.

static XED_INLINE xed_bool_t xed_decoded_inst_valid | ( | const xed_decoded_inst_t * | p | ) | `[static]`

| Return true if the instruction is valid. Definition at line 50 of file xed-decoded-inst-api.h.

XED_DLL_EXPORT xed_bool_t xed_decoded_inst_valid_for_chip | ( | xed_decoded_inst_t const *const | p,
|  | xed_chip_enum_t | chip
| ) |

| Indicate if this decoded instruction is valid for the specified xed_chip_enum_t chip.

XED_DLL_EXPORT xed_uint_t xed_decoded_inst_vector_length_bits | ( | xed_decoded_inst_t const *const | p | ) |

| Returns 128, 256 or 512 for operations in the VEX, EVEX (or XOP) encoding space and returns 0 for (most) nonvector operations. This usually the content of the VEX.L or EVEX.LL field, reinterpreted. Some GPR instructions (like the BMI1/BMI2) are encoded in the VEX space and return non-zero values from this API.

XED_DLL_EXPORT void xed_decoded_inst_zero | ( | xed_decoded_inst_t * | p | ) |

| Zero the decode structure completely. Re-initializes all operands.

XED_DLL_EXPORT void xed_decoded_inst_zero_keep_mode | ( | xed_decoded_inst_t * | p | ) |

| Zero the decode structure, but preserve the existing machine state/mode information. Re-initializes all operands.

XED_DLL_EXPORT void xed_decoded_inst_zero_keep_mode_from_operands | ( | xed_decoded_inst_t * | p,
|  | const xed_operand_values_t * | operands
| ) |

| Zero the decode structure, but copy the existing machine state/mode information from the supplied operands pointer. Same as xed_decoded_inst_zero_keep_mode.

XED_DLL_EXPORT void xed_decoded_inst_zero_set_mode | ( | xed_decoded_inst_t * | p,
|  | const xed_state_t * | dstate
| ) |

| Zero the decode structure, but set the machine state/mode information. Re-initializes all operands.

XED_DLL_EXPORT xed_error_enum_t xed_ild_decode | ( | xed_decoded_inst_t * | xedd,
|  | const xed_uint8_t * | itext,
|  | const unsigned int | bytes
| ) |

| This function just does instruction length decoding. It does not return a fully decoded instruction.

Parameters:

  | xedd | the decoded instruction of type xed_decoded_inst_t . Mode/state sent in via xedd; See the xed_state_t .
  | itext | the pointer to the array of instruction text bytes
  | bytes | the length of the itext input array. 1 to 15 bytes, anything more is ignored.

Returns:
  xed_error_enum_t indiciating success (XED_ERROR_NONE) or failure. Only two failure codes are valid for this function: XED_ERROR_BUFFER_TOO_SHORT and XED_ERROR_GENERAL_ERROR. In general this function cannot tell if the instruction is valid or not. For valid instructions, XED can figure out if enough bytes were provided to decode the instruction. If not enough were provided, XED returns XED_ERROR_BUFFER_TOO_SHORT. From this function, the XED_ERROR_GENERAL_ERROR is an indication that XED could not decode the instruction's length because the instruction was so invalid that even its length may across implmentations.

XED_DLL_EXPORT unsigned int xed_inst_cpl | ( | const xed_inst_t * | p | ) |

| xed_inst_cpl() is DEPRECATED. Please use "xed_decoded_inst_get_attribute(xedd, XED_ATTRIBUTE_RING0)" instead. Return the current privilege level (CPL) required for execution, 0 or 3. If the value is zero, then the instruction can only execute in ring 0.

static XED_INLINE xed_exception_enum_t xed_inst_exception | ( | const xed_inst_t * | p | ) | `[static]`

| Return xed_exception_enum_t if present for the specified instruction. This is currently only used for SSE and AVX instructions. Definition at line 344 of file xed-inst.h.

XED_DLL_EXPORT xed_uint32_t xed_inst_get_attribute | ( | const xed_inst_t * | p,
|  | xed_attribute_enum_t | attr
| ) |

| Scan for the attribute attr and return 1 if it is found, 0 otherwise.

XED_DLL_EXPORT xed_attributes_t xed_inst_get_attributes | ( | const xed_inst_t * | p | ) |

| Return the attributes bit vector.

static XED_INLINE unsigned int xed_inst_noperands | ( | const xed_inst_t * | p | ) | `[static]`

| Number of instruction operands. Definition at line 299 of file xed-inst.h.

XED_DLL_EXPORT const xed_operand_t* xed_inst_operand | ( | const xed_inst_t * | p,
|  | unsigned int | i
| ) |

| Obtain a pointer to an individual operand.

XED_DLL_EXPORT const xed_inst_t* xed_inst_table_base | ( | void |  | ) |

| Return the base of instruction table.

XED_DLL_EXPORT xed_uint_t xed_operand_conditional_read | ( | const xed_operand_t * | p | ) |

| If the operand has a conditional read (may also write).

XED_DLL_EXPORT xed_uint_t xed_operand_conditional_write | ( | const xed_operand_t * | p | ) |

| If the operand has a conditional write (may also read).

static XED_INLINE xed_uint32_t xed_operand_imm | ( | const xed_operand_t * | p | ) | `[static]`

Parameters:

  | p | an operand template, xed_operand_t. These operands represent branch displacements, memory displacements and various immediates

Definition at line 164 of file xed-inst.h.

static XED_INLINE xed_uint_t xed_operand_is_memory_addressing_register | ( | xed_operand_enum_t | name | ) | `[static]`

| Tests the enum for inclusion in XED_OPERAND_{BASE0,BASE1,INDEX,SEG0,SEG1}.

Parameters:

  | name | the operand name, type xed_operand_enum_t

Returns:
  1 if the operand name is for a memory addressing register operand, 0 otherwise. See also xed_operand_is_register .

Definition at line 192 of file xed-inst.h.

static XED_INLINE xed_uint_t xed_operand_is_register | ( | xed_operand_enum_t | name | ) | `[static]`

| Tests the enum for inclusion in XED_OPERAND_REG0 through XED_OPERAND_REG15.

Parameters:

  | name | the operand name, type xed_operand_enum_t

Returns:
  1 if the operand name is REG0...REG15, 0 otherwise.

Note there are other registers for memory addressing; See xed_operand_is_memory_addressing_register .

Definition at line 184 of file xed-inst.h.

static XED_INLINE xed_operand_enum_t xed_operand_name | ( | const xed_operand_t * | p | ) | `[static]`

| Definition at line 86 of file xed-inst.h.

static XED_INLINE xed_nonterminal_enum_t xed_operand_nonterminal_name | ( | const xed_operand_t * | p | ) | `[static]`

| Definition at line 128 of file xed-inst.h.

static XED_INLINE xed_operand_visibility_enum_t xed_operand_operand_visibility | ( | const xed_operand_t * | p | ) | `[static]`

| Definition at line 93 of file xed-inst.h.

XED_DLL_EXPORT void xed_operand_print | ( | const xed_operand_t * | p,
|  | char * | buf,
|  | int | buflen
| ) |

| Print the operand p into the buffer buf, of length buflen.

Parameters:

  | p | an operand template, xed_operand_t.
  | buf | buffer that gets filled in
  | buflen | maximum buffer length

XED_DLL_EXPORT xed_uint_t xed_operand_read | ( | const xed_operand_t * | p | ) |

| If the operand is read, including conditional reads.

XED_DLL_EXPORT xed_uint_t xed_operand_read_and_written | ( | const xed_operand_t * | p | ) |

| If the operand is read-and-written, conditional reads and conditional writes.

XED_DLL_EXPORT xed_uint_t xed_operand_read_only | ( | const xed_operand_t * | p | ) |

| If the operand is read-only, including conditional reads.

static XED_INLINE xed_reg_enum_t xed_operand_reg | ( | const xed_operand_t * | p | ) | `[static]`

| Careful with this one -- use xed_decoded_inst_get_reg()! This one is probably not what you think it is. It is only used for hard-coded registers implicit in the instruction encoding. Most likely you want to get the xed_operand_enum_t and then look up the instruction using xed_decoded_inst_get_reg(). The hard-coded registers are also available that way.

Parameters:

  | p | an operand template, xed_operand_t.

Returns:
  the hard-wired (implicit or suppressed) registers, type xed_reg_enum_t

Definition at line 141 of file xed-inst.h.

static XED_INLINE xed_operand_action_enum_t xed_operand_rw | ( | const xed_operand_t * | p | ) | `[static]`

| Returns the raw R/W action. There are many cases for conditional reads and writes. Definition at line 207 of file xed-inst.h.

static XED_INLINE xed_uint_t xed_operand_template_is_register | ( | const xed_operand_t * | p | ) | `[static]`

| Careful with this one; See xed_operand_is_register().

Parameters:

  | p | an operand template, xed_operand_t.

Returns:
  1 if the operand template represents are register-type operand.

Related functions: Use xed_decoded_inst_get_reg() to get the decoded name of /// the register, xed_reg_enum_t. Use xed_operand_is_register() to test xed_operand_enum_t names.

Definition at line 157 of file xed-inst.h.

static XED_INLINE xed_operand_type_enum_t xed_operand_type | ( | const xed_operand_t * | p | ) | `[static]`

Returns:
  The xed_operand_type_enum_t of the operand template. This is probably not what you want.

Definition at line 101 of file xed-inst.h.

static XED_INLINE xed_operand_width_enum_t xed_operand_width | ( | const xed_operand_t * | p | ) | `[static]`

| Definition at line 114 of file xed-inst.h.

XED_DLL_EXPORT xed_uint32_t xed_operand_width_bits | ( | const xed_operand_t * | p,
|  | const xed_uint32_t | eosz
| ) |

Parameters:

  | p | an operand template, xed_operand_t.
  | eosz | effective operand size of the instruction, 0 | 1 | 2 | 3 for 8 | 16 | 32 | 64 bits respectively.

Returns:
  the actual width of operand in bits.

XED_DLL_EXPORT xed_uint_t xed_operand_written | ( | const xed_operand_t * | p | ) |

| If the operand is written, including conditional writes.

XED_DLL_EXPORT xed_uint_t xed_operand_written_only | ( | const xed_operand_t * | p | ) |

| If the operand is written-only, including conditional writes.

static XED_INLINE xed_operand_element_xtype_enum_t xed_operand_xtype | ( | const xed_operand_t * | p | ) | `[static]`

Returns:
  The xed_operand_element_xtype_enum_t of the operand template. This is probably not what you want.

Definition at line 108 of file xed-inst.h.